BusinessPhone – ACD Agent
Description

## Dialog 4222 Office

1 Display

2x20 characters. See section Display info.

2 Dual-Function programmable keys

Storing numbers, program functions.

3 2nd

Key for access to secondary key functions (These functions are stated on the second line of the corresponding key).

4 Transfer / Diversion

a. |  | Transfer an ongoing call. See section During Calls.

b. |  | Activate/Deactivate diversion. See section Call Forwarding.

5 Inquiry / Conference

a. |  | To make an inquiry to an internal or external party.

b. |  | To establish a telephone conference.

See section During Calls.

6 Line 2 / Read &

a. |  | Line key 2 for in and outgoing calls.

b. |  | Read information. See section Absence Information.

7 Line 1 / Save/Redial

a. |  | Line key 1 for in and outgoing calls.

b. |  | Save or redial an external number. See section Outgoing Calls.

8 Message / Info

a. |  | To send and receive messages. See section Messages.

b. |  | To enter information. See section Absence Information.

9 Mute

To switch the microphone on or off. See sections During Calls and Silent ringing.

10 Loudspeaker on/off

To switch the loudspeaker on or off. See section During Calls.

11 Headset key

See section Headset - Dialog 4222 Office.

12 Volume control

13 Clear

To disconnect calls or to clear the display in programming.

14 Microphone

15 Optional key panel

17 Dual-Function programmable keys.

Note:

Use only an optional key panel of type DBY 419 01.

16 Loudspeaker

17 Handset with hearing aid function

Please note:

The handset may attract and retain small metal objects in the earcap region.

© Ericsson Enterprise 2004