BusinessPhone – Dialog 4224 Operator / Dialog 3214
Description

## Display info

The display assists your actions on the phone with step-by-step instructions.

The tiltable display consist of 5 rows, with space for 40 characters on each row. The fields in the display consists of the following information.

When your phone is idle, the first (upper) line shows date, time, temperature, name and extension number. The second line presents queue information. The lower line presents the available menu key functions.

During an external outgoing call the third line will show the directory number of the external line and dialled/connected telephone number. The fourth line displays the call type.

During an internal call the third line will show the extension number and traffic state. The fourth line displays the caller’s name.

If you make an internal call to someone who has activated a diversion, the first and second line shows the name and extension number of the person you called and the third and fourth line shows where the call is diverted.

During an external incoming call the third line will show the directory number of the external line and traffic state. The fourth line displays the caller’s telephone number and call type.

#### Status information

The status information of incoming and outgoing calls is sometimes given as an abbreviation and sometimes as a complete word:

|  |  |  | Radio Paging receiver not in use. |
|  |  |  | Number or function blocked. |
|  |  |  | Extension is busy (queue situation is displayed). |
|  |  |  | Ordered Paging is completed. |
|  |  |  | Congestion in the system, call cannot be put through. |
|  |  |  | Number of calls waiting in the common queue. |
|  |  |  | Call redirected. |
|  |  |  | Line 1 on called extension is free. |
|  |  |  | Line 1 on called extension is busy, but Line 2 is free. |
|  |  |  | Number of calls waiting in the individual queue. |
|  |  |  | Intercom call. |
|  |  |  | The number was incomplete. |
|  |  |  | Voice information activated. |
|  |  |  | Text information activated. |
|  |  |  | The called extension has text or Voice info stored. |
|  |  |  | Inquiry call. |
|  |  |  | Intrusion into ongoing call. |
|  |  |  | Malicious Call Identification accepted. |
|  |  |  | Malicious Call Identification rejected. |
|  |  |  | Call charging. |
|  |  |  | Call not previously answered. |
|  |  |  | Recall of previously answered call. |
|  |  |  | An external incoming call was rerouted to the operator. |
|  |  |  | Restricted extension, calls cannot be handled. |
|  |  |  | Ring to announce call. |
|  |  |  | Serial calls. |
|  |  |  | Speech connection. |
|  |  |  | Transferred call. |
|  |  |  | Non assigned number. |
|  |  |  | Radio Paging waiting. |
|  |  |  | Indicates outside temperature and tendency (up or down) if your telephone system is equipped with optional temperature sensor. |

© Ericsson Enterprise 2003