BusinessPhone – Dialog 4224 Operator / Dialog 3214
Outgoing Calls

## Busy extension

An incoming call would like to be transferred to a specific extension, but the called extension is busy. You have several options:

Note:

You can intrude on a busy extension, see section Intrusion and forced release.

#### Option 1

To transfer the call to the busy extension:

Press and hold (see display).

The conversation partner of the busy extension, is shown in the display.

Press to place the call.

The call will be placed automatically when the extension becomes free. The extension will hear a call waiting signal.

#### Option 2

To camp-on the call:

Notify

Press.

Loop 1

Press any free Loop key.

The key lamp shows steady light. The call is now in camped on state, with notification of free extension. You can answer new incoming calls.

Note:

Calls cannot be camped on to internal group numbers.

A ringing signal and the Loop key lamp flashing indicates that the extension is free. Answer within eight seconds by pressing the Loop key, otherwise the call will be placed automatically.

Loop 1

Press.

The Loop key light extinguishes.

Speech

Press to call the extension.

Press to place the call.

Or:

If the caller wants another extension:

Loop 1

Press.

Clear

Press.

Call the new extension and place the call in the normal way.

#### Option 3

The caller prefers to call again later:

Clear

Press to disconnect.

Clear

Press to disconnect.

© Ericsson Enterprise 2003