 	 
getenginestatus
Enables you to retrieve the status information of the SUM session.

Syntax

smartupdate getenginestatus

Windows usage

C:/>smartupdate getenginestatus

Linux usage

$ ./smartupdate getenginestatus

Example output

No SUM engine found running.

Example output

Process name:

Copyright:

Version:

Active Sessions:

Engine status:

Total number of sessions:

Return codes
SUCCESS_NO_REBOOT
Windows: 0

Linux: 0

Text: The command was successful.

SUCCESS_REBOOT
Windows: 1

Linux: 1

Text: The command was successful but a reboot is required.

SUCCESS_NOT_REQUIRED
Windows: 3

Linux: 3

Text: The command completed successfully, but was not required or everything is already current.

FAILURE_GENERAL
Windows: -1

Linux: 255

Text: A general failure occurred. For details, see the logs.

FAILURE_BAD_PARM
Windows: -2

Linux: 254

Text: A bad input parameter was encountered. For details, see the logs.

FAILURE_COMPONENT_FAILED
Windows: -3

Linux: 253

Text: The installation of the component failed.

FAILURE_COMMAND_FAILED
Windows: -4

Linux: 252

Text: The command failed. For details, see the logs.

 	 	 