 	 
getcomponentlogs
Enables you to view the component logs for a node.

Syntax

smartupdate getcomponentlogs [--nodes [<nodelist>]] [--component <componentname>]

Parameters

--nodes [<nodelist>]
Nodes for this request. If you do not provide a nodelist, all nodes in the session are used.

--component <componentname>
The name of the component that SUM will display the log. If you use this parameter, you must enter a component name. If you do not specify a component, SUM generates logs for all components.

Windows usage

C:\> smartupdate getcomponentlogs /nodes localhost

Linux usage

$ ./smartupdate getcomponentlogs --nodes 10.0.1.1 --component cp020024.exe

Return codes
SUCCESS_NO_REBOOT
Windows: 0

Linux: 0

Text: The command was successful.

SUCCESS_REBOOT
Windows: 1

Linux: 1

Text: The command was successful but a reboot is required.

SUCCESS_NOT_REQUIRED
Windows: 3

Linux: 3

Text: The command completed successfully, but was not required or everything is already current.

FAILURE_GENERAL
Windows: -1

Linux: 255

Text: A general failure occurred. For details, see the logs.

FAILURE_BAD_PARM
Windows: -2

Linux: 254

Text: A bad input parameter was encountered. For details, see the logs.

FAILURE_COMPONENT_FAILED
Windows: -3

Linux: 253

Text: The installation of the component failed.

FAILURE_COMMAND_FAILED
Windows: -4

Linux: 252

Text: The command failed. For details, see the logs.

 	 	 