//
//  %Z% %I% %W% %G% %U%
//
//  ZZ_Copyright_BEGIN
//
//
//  Licensed Materials - Property of Hewlett Packard Enterprise Development LP
//
//  HPE StoreOpen Software Version 3.4
//
//  (C) Copyright 2015 - 2018 Hewlett Packard Enterprise Development LP
//
//  This file is part of the HPE StoreOpen Software
//
//  HPE StoreOpen Software is free software;
//  you can redistribute it and/or modify it under the terms of the GNU Lesser
//  General Public License as published by the Free Software Foundation,
//  version 2.1 of the License.
//
//  HPE StoreOpen Software is distributed in the
//  hope that it will be useful, but WITHOUT ANY WARRANTY; without even the
//  implied warranty of MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
//  See the GNU Lesser General Public License for more details.
//
//  You should have received a copy of the GNU Lesser General Public
//  License along with this library; if not, write to the Free Software
//  Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA 02111-1307 USA
//  or download the license from <http://www.gnu.org/licenses/>.
//
//
//  ZZ_Copyright_END
//

// Messages for the ltotape backend.
// This backend uses IDs in the range 20000-20999.

root:table {
	messages:table {
		start_id:int { 20000 }
		end_id:int { 20999 }

		// First ten slots reserved..

		// Messages for the ltotape backend:
		20010D:string { "SCSI request: [ %s] Requested length=%d" }
		20011D:string { "SCSI outcome: Driver status=0x%02X SCSI status=0x%02X Actual length=%d" }
		20012D:string { "SCSI sense  : %s" }
		20013I:string { "Drive type is %s, serial number is %s" }
		20014E:string { "Drive requires firmware update to enable LTFS (current=%s)" }
		20015I:string { "Unable to read device serial number" }
		20016W:string { "Cannot find valid snapshot log" }
		20017D:string { "Cannot take snapshot log, drive type (%s) does not support feature" }
		20018D:string { "Snapshot in process of creation, pausing before retry" }
		20019E:string { "Internal program error: size %d too large in (%s)" }
		20020D:string { "SG_RESERVED_SIZE (max block size) now set to %d bytes" }
		20021D:string { "Cannot locate, tape appears to be uninitialized" }
		20022I:string { "Tape has passed the Early Warning EOM point, so forcing to Read Only mode" }
		20023E:string { "Backend SCSI subsystem error from %s (0x%0X)" }
		20024W:string { "Cannot store attribute 0x%0X (%d)" }
		20025D:string { "Stored EWSTATE attribute as %d" }
		20026I:string { "Tape was previously formatted by application '%s'" }
		20027E:string { "Failed to find specific device instance %d" }
		20028D:string { "Found device class 0x%X at index %d" }
		20029E:string { "Failed to create device interface - device may be busy?" }
		20030E:string { "Failed to get exclusive access - device may be busy? (%d)" }
		20031D:string { "Looking for sg device corresponding to %s" }
		20032E:string { "Error remapping st device %s to sg : %s" }
		20033E:string { "Unable to find matching sg device for %s" }
		20034D:string { "Mapped %s to %s (%d.%d.%d.%d)" }
		20035E:string { "Unable to lock device (%s)" }
		20036E:string { "Parsing log page: buffer too small, copying %zu bytes from %lx" }
		20037E:string { "Option parsing for the ltotape backend failed (%d)" }
		20038D:string { "Read block: file mark detected" }
		20039D:string { "Backend %s: %zu bytes" }
		20040E:string { "EBUSY in %s" }
		20041E:string { "EFAULT in %s" }
		20042E:string { "EIO in %s" }
		20043E:string { "ENOMEM in %s" }
		20044E:string { "ENXIO in %s" }
		20045E:string { "EPERM in %s" }
		20046E:string { "ETIMEDOUT in %s" }
		20047E:string { "EINVAL in %s" }
		20048W:string { "Received low space warning in %s" }
		20049E:string { "EACCES in %s" }
		20050E:string { "EOVERFLOW in %s" }
		20051E:string { "ENOSYS in %s" }
		20052E:string { "EROFS in %s" }
		20053E:string { "ENOMEDIUM in %s" }
		20054E:string { "Unknown error in %s (%d)" }
		20055E:string { "EAGAIN in %s" }
		20056D:string { "Backend %s: %zu" }
		20057D:string { "Backend %s: (%llu, %llu)" }
		20058D:string { "Backend %s" }
		20059D:string { "Backend %s: %llu" }
		20060D:string { "Backend ReadPosition: Partition=%llu, LogObject=%llu, FMcount=%llu" }
		20061D:string { "Backend %s: 0x%02X" }
		20062E:string { "Unsupported cartridge type (%s)" }
		20063D:string { "Locate encountered EOD : ignoring sense data" }
		20064E:string { "Locate failed (%d)" }
		20065E:string { "Space: unrecognized type (%d)" }
		20066E:string { "Cannot read position (%d)" }
		20067E:string { "Invalid format mode (%d)" }
		20068E:string { "Format operation failed (%d)" }
		20069E:string { "Cannot get remaining capacity: get log page 0x%02x failed (%d)" }
		20070E:string { "Cannot get remaining capacity: failed to parse the log page" }
		20071E:string { "Cannot get remaining capacity: loop index error (%d)" }
		20072E:string { "Failed to read mode data (%d)" }
		20073E:string { "Failed to set mode data (%d)" }
		20074E:string { "Failed to read attribute 0x%X (%d)" }
		20075E:string { "Failed to write attribute (%d)" }
		20076I:string { "Triggering drive diagnostic dump" }
		20077W:string { "Unable to generate drive dump" }
		20078W:string { "Unable to read drive dump" }
		20079W:string { "Unable to save drive dump to file" }
		20080D:string { "Saved drive dump to %s" }
		20081W:string { "Error saving drive dump: wrote %d bytes out, expected %d" }
		20082W:string { "Error saving drive dump: unable to close %s" }
		20083E:string { "Cannot open device: inquiry failed (%d)" }
		20084D:string { "Drive identification is \'%s\'" }
		20085E:string { "Unsupported drive \'%s\'" }
		20086E:string { "%s: medium is already mounted or in use" }
		20087E:string { "Cannot open device \'%s\' (%d)" }
		20088W:string { "Had to open device \'%s\' in read-only mode" }
		20089D:string { "Driver detail: %16s = 0x%X" }
		20090W:string { "Unable to create dumpfile \'%s\' - %s" }
		20091I:string { "Unable to get %s properties for \'%s\' - %s" }
		20092D:string { "Found %d log snapshot files, oldest is \'%s\'" }
		20093E:string { "Unable to delete file \'%s\' - %s" }
		20094D:string { "Removed old snapshot file \'%s\'" }
		20095D:string { "Snapshot directory set to \'%s\'" }
		20096I:string { "Diagnostic dump complete" }
		20097D:string { "Drive firmware update needed to enable EOD status check" }
		20098D:string { "Attribute 0x%X not found" }
		20099I:string { "Log snapshot cannot be used, \'%s\' is not available" }
		20100E:string { "Memory allocation failed" }
		20101D:string { "Device name %s modified to a non-rewind-on-close type %s" }
		20102W:string { "Cannot create work directory (%d)" }
		20103W:string { "Path \'%s\' exists, but is not a directory" }
		20104W:string { "Invalid log-directory path \'%s\', setting back to default log-directory" }
		20105E:string { "Attempting to write FM at BOP" }
		20106I:string { "Retaining existing MAM barcode %s" }
		20107I:string { "Replacing existing MAM barcode %s with user-specified %s" }
	}
}
