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	Affected System(s)
	n/a
	     Estimated Installation

     Time in Man/Hours
	15 min.

	Equipment

Title(s)
	Hi-Track Remote Access Control Center
	    Time Cycle for
Installation
	

	Equipment

Model Number(s)
	n/a
	       IMMEDIATELY
	

	Manufacturing

Number(s) (Mfg. No.)
	IP0860-1
	
	

	Prerequisite/
Corequisite
	Software only – see below
	
	


Purpose and Description of Change
This ECN announces the release of version 1.3 of the Hi-Track Remote Access Control Center (RACC). This is the second public release of this software.
	Version:
	1.3

	Build:
	1.3.0.0

	Build date:  
	March 12, 2012


Supported Platforms
· Microsoft Windows XP SP2 (32-bit) 

· Microsoft Windows Vista (32-bit) 

· Microsoft Windows Vista (64-bit) 

· Microsoft Windows Vista SP1 (32-bit) 

· Microsoft Windows 7 (64-bit) 

· Microsoft Windows Server 2003 SP2 (32-bit) 

· Microsoft Windows Server 2003 SP2 (32-bit) on VMware 

· Microsoft Windows Server 2008 (32-bit) on VMware 

· Microsoft Windows Server 2008 R2 (64-bit)
Bug Fixes
· Fixed the problem with launching RACC from the installation menu 

· If RACC is installed on SVP, create firewall ALLOW rules for the micro-processors of the storage array to allow Storage Navigator’s maintenance app to continue to function after enabling firewall from the RACC UI 

· Create an inbound rule to allow remote access to the RACC user interface when firewall is enabled 

· Correctly save the value of the ‘auto connection’ checkbox so it is not affected by system reboots 

New Features
· Native 64-bit OS support 

· Revamped LDAP authentication support that among others has the below improvements 

· SSL support 

· Store admin password encrypted in web.config 

· Enforce users to verify connectivity to the LDAP server before saving configuration 

· System configuration check that determines if the host system meets the minimum requirements to launch VPN sessions
· Log authentication attempts to the RACC user interface as well as user logouts 

· Log the remote desktop session information such as username
· Send notification email for pending connection requests 

· Configurable session timeout 

· Configurable banner message to be displayed on the login page
· Configurable SMTP port for email notification 

· Keep RACC logs for a configurable number of days ( default is 30 days)
· Support domain authentication for proxy servers 

Hitachi Data Systems   PROPRIETARY INFORMATION







ECN�
ECN 92HT113-0�
�
DATE�
March 12, 2012�
�
�
Hamid Toolloei�
�



























