==========================================================================
        S5BH serials AST2500(A2) BMC FW Release v4.65.06 (Only for S5Bx/S5Sx)
==========================================================================
Version: 4.65.06
Release Date: 2020.01.21

AMI Subversion Revision: AMI SPX RR11.5
Code Based: 4.80.00
DMTF Redfish Specification version:1.5.0

[Utility]:
1. Yafuflash2 (version 4.16.21_01)
2. MIB version 1.12

[Firmware Images]:
1. s5bxv4.65.06_rom.ima with checksum          :	EA461B5D
2. s5bxv4.65.06_rom.ima with MD5 checksum      :	728029ebde48906880e358b5d45c097f              
3. s5bxv4.65.06_rom.ima_enc with MD5 checksum  :	a4d027183f41b39d85be4a9a0b408315                 

[Fan Table]
Version:
S5Bx:
SKU0~2,80~82: v12
SKU3~4,83~84: v07
SKU5~7,85~87: v07
SKU8~9: v03

[Change/Add]: 
S5Bx:	
	1. BMC function - Add TLS protocol settings via IPMI/Redfish/Web GUI (New Function Request).
	2. BMC function - Add audit log sync to the system log when a user subscribes to the system log (New Function Request).
	3. BMC function - Remove login/logout from SEL, and record login/logout event in Audit log (New Function Request).
	4. BMC function - Add audit log can be exportable (New Function Request).
	5. Redfish - Add Redfish command support equivalent to IPMI command (New Function Request).
	   i.  Status LED in Redfish support.
	   ii. HBA port, WWN & WWPN in Redfish support.
	   iii.CPU present.
	   iv. Manufacture ID, Product ID. 
	   v.  Server FRUs.
	   vi. Get & Set Boot Options.
	   
[Bug Fixed]:
	1. BMC WebUI - #306773 The memory size calculation unit is show MB on Web GUI does not match with Redfish(MiB).
	2. BMC WebUI - #283952 #264205 #264176 #276012 #304801 Invalid IPv6 setting issues on Web GUI.
	3. BMC WebUI - #306557 There is no 'I forgot my password' link in web GUI login page.
	4. BMC function - #299118 SNMP settings can not restore to default value after restoring factory default.
	5. BMC function - #304951 After delete user account, the events about deleted account will add 'Account : xxxx ( UID)' at the end of the string.
	6. BMC function - #307012 Can not login web GUI with user created via IPMI inband by user name length is 16.
	7. BMC Redfish - #290456 Can not GET /redfish/v1/AccountService/Accounts/4.

[Known issue]: 
	n/a
	
[Notice]:
	1. Update BMC FW via command line:
		Refer to readme.txt
	2. Update BMC FW via Web UI:
		a) Please select s5bxvXX.YY.ZZ_rom.ima_enc as image file and doesn't upload Signimage key.
	3. login account: 
		a) IPMI access account for WEBGUI and IPMITOOL.
		username: admin
		password: cmb9.admin
	4. Please canceling preserve all configuration or only preserve 4 options (IPMI/Network/Authentication/SNMP) before upgrading this version BMC (if FW version is less v4.55.06).
	   Because of this version's BMC upgrade Redfish to 1.5 (i.e. update lots of ipmi lib part for Redfish ), 
	   we suggest canceling preserve all configuration or only preserve 4 options (IPMI/Network/Authentication/SNMP) before upgrading this version BMC to avoid unexpected defect occurred.
	5. Not support GPT image file when using the remote image function. 
	6. Please clear browser cache and cookies after finishing upgrades.
	7. Not support BMC FW downgrade with preservation.
	8. Please first update BMC then update BIOS with preserve function if need updates BMC and BIOS with preserve bios settings. 
	9. BMC 4.27.06 SSH login function error, please skip this version if need use SSH login.