# IP Location Traffic

#### Function

This report provides visibility into the incoming or attack traffic of a specific IP location.

Do not add user-defined IP locations to or delete them from an anti-DDoS device. Otherwise, the IP Location Top N report on the ATIC is inaccurate.

#### Parameter

Table 1 Query parameters of IP location traffic
Parameter | Description
--- | ---
Device | Select a device from the drop-down list.
Zone | Click , select a Zone on the Zone page that is displayed, and then click OK.
Location | Click . In Location that is displayed, select an IP location and click OK.
Time | Click to select the start time and end time of statistics. Or you can change the time values in corresponding text boxes. The end time should be later than the start time and the interval cannot be longer than one year. If the query interval is longer than or equal to seven days and shorter than one year, statistics are collected daily. If the query interval is longer than or equal to one day and shorter than seven days, statistics are collected hourly. If the query interval is shorter than one day, statistics are collected every five minutes.
Unit | Select a traffic measurement unit. The unit can be pps or kbps. The default unit is pps.

#### Example

If the device is set to DDoS-Cleaning and the Zone is set to All, the incoming traffic of a specific IP location in a specific period is displayed, as shown in Figure 1.

Figure 1 Incoming traffic of a specific IP traffic

#### Procedure

1. Choose Report > Report > Traffic Analysis.
2. Click the IP Location Traffic tab.
3. Set query parameters.
4. Click Search.

   Information about IP location traffic that matches the query conditions is displayed.

   If a Zone has been deleted, the Zone name is displayed as Unknown Zone.

5. Optional: Open or save the query results as files, or send queried reports to the specified email address.

   - Click to open or save the query results as PDF files. A maximum of 10,000 entries can be displayed.
   - Click to open or save the query results as EXCEL files. A maximum of 10,000 entries can be displayed.
   - Click to open or save the query results as CSV files. All data except figures can be displayed.
   - Click to enter a recipient mail address and select an attachment format. Then click OK.

Parent topic: Traffic Analysis

Copyright © Huawei Technologies Co., Ltd.