--
-- HUAWEI-FWD-RES-TRAP-MIB.mib
-- Copyright (C) 2023 by HUAWEI TECHNOLOGIES. All rights reserved
-- Thursday,Oct 28, 2014 at 18:46:56
-- Version: V5.31

    HUAWEI-FWD-RES-TRAP-MIB DEFINITIONS ::= BEGIN
 
        IMPORTS
            entPhysicalName            
                FROM ENTITY-MIB            
            hwDatacomm            
                FROM HUAWEI-MIB            
            OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP            
                FROM SNMPv2-CONF            
            Counter64, Unsigned32, Integer32, OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE ,IpAddress              
                FROM SNMPv2-SMI
            Ipv6Address
                FROM IPV6-TC;

           hwFwdResTrapMIB MODULE-IDENTITY 
            LAST-UPDATED "202309142013Z"            --  Sep 14, 2023 at 20:13 GMT
  
            ORGANIZATION 
                "Huawei Technologies Co.,Ltd."
            CONTACT-INFO 
                "Huawei Industrial Base
                  Bantian, Longgang
                   Shenzhen 518129
                   People's Republic of China
                   Website: http://www.huawei.com
                   Email: support@huawei.com
                 "

             DESCRIPTION
              "add hwEnterModeReasonId, hwEnterModeId, hwFesEnterSpecialMode ,hwFesEnterSpecialModeResume.
              add one reasonid for hwEnterModeReasonId:fesEnterSpecialMode(1)"
              REVISION "202309142013Z"            --  Sep 14, 2023 at 20:13 GMT

	     DESCRIPTION
              "add three reasonid for hwLCfwdResourceOverload:
              qppbOutCarStatResExceed90Threshold(1231),
              qppbOutCarStatResExceedThreshold(1232)"
              REVISION "202309141000Z"            --  Sep 14, 2023 at 11:52 GMT

	     DESCRIPTION
              "add hwBoardNetworkSliceConflict, hwBoardNetworkSliceConflictResume,
              add one reasonid for hwFwmSliceResourceReasonId
              chanIfBandwidthInsufficient(4)"
              REVISION "202309081000Z"            --  Sep 8, 2023 at 10:00 GMT

	     DESCRIPTION
              "add one reasonid for hwLCfwdResourceOverload:
              l2ExtAclGroupResOverload(1230)"
              REVISION "202309061700Z"            --  Sep 6, 2023 at 17:00 GMT		 
            
              DESCRIPTION
              "delete hwEntPhysicalName"
              REVISION "202308282100Z"            --  Aug 28, 2023 at 21:00 GMT

		DESCRIPTION
              "add 2 reasonid for hwLCfwdResourceOverload:
                slicePrefixMapNumOverload(1228),
                slicePrefixMapNumExceedingThreshold(1229)"
              REVISION "202308262129Z"

             DESCRIPTION
               "add 3 reasonid for camResWaring(1223),camcountidResWaring(1224),netrouteResWaring(1225)"
              REVISION "202308241603Z"	 


			DESCRIPTION
              "add 2 reasonid for hwLCfwdResourceOverload:
                inlifMplsNumOverload(1226),
                inlifSRv6NumOverload(1227)"
              REVISION "202308241517Z"


            DESCRIPTION
              "add hwEntPhysicalName"
              REVISION "202308141100Z"            --  Aug 14, 2023 at 11:00 GMT

            DESCRIPTION
              "add 1 reasonid for hwBoardResThresholdExceed:
              mcfibv4NumExceedForwardEngine(1222)"
              REVISION "202308121600Z"            --  Aug 12, 2023 at 16:00 GMT
	
              DESCRIPTION
              "add hwCapwapNoFragmentAlarm, hwCapwapDiscardBroadcastAlarm"
              REVISION "202308081700Z"            --  Aug 8, 2023 at 17:00 GMT

	   DESCRIPTION
            "add three reasonid for hwLCfwdResourceOverload:
              ipv4EnhanceCpAclGroupExceedThreshold(1122),
              ipv6EnhanceCpAclGroupExceedThreshold(1123),
              twampInJectAclGroupExceedThreshold(1124)"
              REVISION "202308041730Z"            --  Aug 4, 2023 at 17:30 GMT
		 
           DESCRIPTION
              "add hwFwdTblmScanHndOverloadClear, hwFwdTblmScanHndThresholdExceedClear"
              REVISION "202308041600Z"            --  Aug 4, 2023 at 16:00 GMT

           DESCRIPTION
              "add hwFwdTblmScanHndOverload, hwFwdTblmScanHndThresholdExceed"
              REVISION "202308031530Z"            --  Aug 3, 2023 at 15:30 GMT
			  
           DESCRIPTION
           "add one reasonid for hwLCfwdResourceOverload and hwBoardFwdResThresholdExceed:
              bgpLspNumExceedThreshold(1121)"
              REVISION "202307181730Z"            --  July 18, 2023 at 17:30 GMT

           DESCRIPTION
           "add two reasonid for hwLCfwdResourceOverload and hwBoardFwdResThresholdExceed:
              y1731SslmNumOverLoad(1116),
              y1731SslmNumExceedThreshold(1117),
              nqaL2RcvEAclGroupExceedThreshold(1118),
              nqaL3RcvEAclGroupExceedThreshold(1119),
              nqaL2RcvIAclGroupExceedThreshold(1120)"
              REVISION "202307151609Z"            --  July 15, 2023 at 16:09 GMT

          DESCRIPTION
           "add two reasonid for hwLCfwdResourceOverload and hwBoardFwdResThresholdExceed:
               mcPimBdrStatusResExceedThreshold(1114),
               mcPimBdrStatusResOverLoad(1115)"
              REVISION "202307102114Z"            --  July 10, 2023 at 21:14 GMT

           DESCRIPTION
            "add 12 reasonid for hwLCfwdResourceOverload:
               intfCarAclExceedThreshold(1102),
               intfCarAclExceed95Threshold(1103),
               upstreamL2AclGroupExceedThreshold(1104),
               downstreamL2AclGroupExceedThreshold(1105),
               upstreamIpv4AclGroupExceedThreshold(1106),
               downstreamIpv4AclGroupExceedThreshold(1107),
               upstreamIpv6AclGroupExceedThreshold(1108),
               downstreamIpv6AclGroupExceedThreshold(1109),
               upstreamMplsAclGroupExceedThreshold(1110),
               downstreamMplsAclGroupExceedThreshold(1111),
               twampIpv4AclGroupExceedThreshold(1112),
               twampIpv6AclGroupExceedThreshold(1113)"
              REVISION "202306022238Z"            --  Jun 2, 2023 at 22:38 GMT

            DESCRIPTION
            "add 4 reasonid for hwLCfwdResourceOverload:
               rev4NumOverload(1098),
               rev6NumOverload(1099),
               rev4NumExceedThreshold(1100),
               rev6NumExceedThreshold(1101)"
              REVISION "202305121855Z"            --  May 12, 2023 at 18:55 GMT

           DESCRIPTION
           "add 1 reasonid for mplsIlmResWarning(1097)"
             REVISION  "202305061745Z"        --  May 6, 2023 at 17:45 GMT
         
            DESCRIPTION
            "add 4 reasonid for hwLCfwdResourceOverload:
               tlmtActCar300s(1093),
               tlmtActCar300Pre(1094),
               tlmtPolicy300s(1095),
               tlmtPolicy300Pre(1096)"
              REVISION "202304182055Z"            --  April 18, 2023 at 20:55 GMT

        DESCRIPTION
	      "add 10 reasonid for vlanDomainResWarning(1083), veResWarning(1084), lacpResWarning(1085), aibsub1ResWarning(1086), aibsub2ResWarning(1087), aibsub3ResWarning(1088), ecmp2ResWarning(1089), mtuResWarning(1090), gltpResWarning(1091), lstResWarning(1092)"
	      REVISION "202304171911Z"        --   April 17, 2023 at 19:11 GMT

		DESCRIPTION 
           "The private mib file includes the alarm information of forwarding engine resouce overload."

                REVISION "202304101809Z"       --   April 10, 2023 at 18:09 GMT
		DESCRIPTION
        "add reason for BGP FlowSpec community resources are insufficient."
                REVISION "202304031948Z"       --   April 3, 2023 at 19:48 GMT
		DESCRIPTION
        "add reason for IPv6 flow-car flow table  resources are insufficient."

		REVISION "202303291630Z"       --   Mar 29, 2023 at 16:30 GMT
		DESCRIPTION
        "add hwMcastElbExceed, hwMcastElbExceedClear"

		REVISION "202303221010Z"       --   Mar 22, 2023 at 10:10 GMT
		DESCRIPTION
        "add hwL2mcGrpAddress, hwL2mcVlanIndex, hwVlanSrcExeedAlarm, hwVlanSrcExeedResume"
		
		REVISION "202303171720Z"        --  Mar 17, 2023 at 17:20 GMT
        DESCRIPTION
            "add 4 reasonid for bgplspResOverload:
            bgplspInStatisticsOverLoad(1077),
			bgplspOutStatisticsOverLoad(1078),
			bgplspInStatisticsExceedThreshold(1079),
			bgplspOutStatisticsExceedThreshold(1080)" 
			
		REVISION "202303131618Z"        --  March 13, 2023 at 16:18 GMT
        DESCRIPTION
            "add 4 reasonid for bgpepeResOverload:
            bgpepeInStatisticsOverLoad(1073),
			bgpepeOutStatisticsOverLoad(1074),
			bgpepeInStatisticsExceedThreshold(1075),
			bgpepeOutStatisticsExceedThreshold(1076)" 
			
        REVISION "202303031036Z"       --   Mar 3, 2023 at 10:36 GMT
		DESCRIPTION
        "add hwInSqExceedPreCfgNum, hwOutSqExceedPreCfgNum"

        REVISION "202302201000Z"       --   Feb 20, 2023 at 10:00 GMT
        DESCRIPTION
        "add hwNdLinkEncapResExceed, hwArpLinkEncapResExceed"

        REVISION "202301302024Z"        --   Jan 30, 2023 at 20:24 GMT
        DESCRIPTION
        "add hwSessLeakEntryNumberThresholdExceed,
         hwSessLeakEntryNumberThresholdExceedClear,
         hwSessUnrecEntryNumberThresholdExceed"

        REVISION "202301101039Z"        --   Jan 10, 2023 at 10:39 GMT
        DESCRIPTION
        "add TopNSourceIpAddress, update hwSessThresholdExceed, hwSessExceed"

        REVISION "202212291039Z"        --  Dec 29, 2022 at 10:39 GMT
        DESCRIPTION
			"add 14 reasonid for hwFwdResLackReasonId:
				bgpflowIfBaseV6EmNstExceedThreshold(1052),
				bgpflowIfBaseV6EmNstExceed90Threshold(1053),
				inIfCarAclExceedThreshold(1054),
				inIfCarAclExceed95Threshold(1055),
				l2upstreamAclGroupExceedThreshold(1056),
				l2downstreamAclGroupExceedThreshold(1057),
				ipv4upstreamAclGroupExceedThreshold(1058),
				ipv4downstreamAclGroupExceedThreshold(1059),
				ipv6upstreamAclGroupExceedThreshold(1060),
				ipv6downstreamAclGroupExceedThreshold(1061),
				mplsUpstreamAclGroupExceedThreshold(1062),
				mplsDownstreamAclGroupExceedThreshold(1063),
				ipv4TwampAclGroupExceedThreshold(1064),
				ipv6TwampAclGroupExceedThreshold(1065)"


        REVISION "202212021141Z"        --  Dec 2, 2022 at 11:41 GMT
        DESCRIPTION
        "add 5 reasonid for glemRes(1044), localFec1Res(1045), localFec2Res(1046), localFec3Res(1047), localFecEcmp(1048)"

        REVISION "202211251453Z"        --  Nov 25, 2022 at 14:53 GMT
        DESCRIPTION
        "add 1 reasonid for sliceRes(1043)"

        REVISION  "202211181730Z"        --  Nov 18, 2022 at 17:30 GMT
        DESCRIPTION  
            "modify name hwBoardNetworkSliceResourceAlarm to hwBoardNetworkSliceResourceInsufficient,
              hwBoardNetworkSliceForwardAlarm to hwBoardNetworkSliceTrafficAbnormal."


        REVISION  "202211141030Z"        --  Nov 14, 2022 at 10:30 GMT
        DESCRIPTION  
            "add 1 reason id about eedb for hwFwdResLackReasonId:
               hwBoardResThresholdExceed(1030)"


        REVISION  "202211091100Z"        --  Nov 21, 2022 at 11:00 GMT
        DESCRIPTION   
            "add 1 reasonid for hwFwdResLackReasonId:
              cgnAclTcamNumOfNpExceedThreshold(1040), 
              cgnAclTcamNumOfNpExhausted(1041)"


        REVISION  "202210211021Z"        --  Oct 21, 2022 at 10:21 GMT
        DESCRIPTION   
            "add 4 reasonid for hwFwdResLackReasonId:
            fe2UserNumExceed90Threshold(1036),
            fe2UserNumExceed100Threshold(1037),
            fe3UserNumExceed90Threshold(1038),
            fe3UserNumExceed100Threshold(1039)"



            REVISION "202210082145Z"   -- Oct 08, 2022 at 21:45 GMT
            DESCRIPTION 
                "add OBJECT hwFwmSliceInterfaceName, hwFwmSliceId, hwFwmSliceTrunkInterfaceName,
                 hwFwmSliceSrcInterfaceName, hwFwmSliceResourceReasonId, hwFwmSliceFwdReasonId.
                 add NOTIFICATION-TYPE hwBoardNetworkSliceResourceAlarm, hwBoardNetworkSliceResourceAlarmResume,
                 hwBoardNetworkSliceForwardAlarm, hwBoardNetworkSliceForwardAlarmResume."


            REVISION "202209282208Z"        --  Sep 28, 2022 at 22:08GMT 
            DESCRIPTION
            " add 6 reasonid for hwLCfwdResourceOverload:
              bgpflowMReResExceedThresHold(1030),
              bgpflowMReResExceed90ThresHold(1031),
              bgpflowNstResExceedThresHold(1032),
              bgpflowNstResExceed90ThresHold(1033),
              bgpflowNhpResExceedThresHold(1034),
              bgpflowNhpResExceed90ThresHold(1035)," 


            REVISION "202209281145Z"        --  Sep 28, 2022 at 11:00GMT 
            DESCRIPTION
            " add 1 reasonid for hwLCfwdResourceOverload:
              hqosPortWredIdResLac(1029)" 


            REVISION "202209190900Z"        --  Nov 19, 2022 at 09:00 GMT   
            DESCRIPTION 
            "update hwEcmpMemberLimitOverThresholdAlarm" 



            REVISION "202208311600Z"        --  Aug 31, 2022 at 16:00 GMT
            DESCRIPTION
            "add a trap info for deterministic-ip shaping exceed."

            REVISION "202208231200Z"        --  Jun 2, 2022 at 14:35 GMT
	        DESCRIPTION
            "add 1 reasonid for nativeIfitFlowIdRes(1024)"
                
            REVISION "202208181100Z"        --  Aug 18, 2022 at 11:00GMT 
            DESCRIPTION
            " add 1 reasonid for hwLCfwdResourceOverload:
              hqosPortWredIdResLac(1024)" 

            REVISION "202207202130Z"        -- Jun 20, 2022 at 21:30GMT
            DESCRIPTION 
                "add OBJECT hwFwmFaultSlotStr, hwFwmFaultCpuStr, hwFwmFaultReasonId, hwFwmFaultReasonDescription.
                 add NOTIFICATION-TYPE hwFwmFaultAlarm, hwFwmFaultAlarmResume." 

           REVISION "202207161539Z"   -- Jun 16, 2022 at 15:39 GMT
           DESCRIPTION
            "add hwNetStreamIPv4OriginalFlowResourceExceeded,
             hwNetStreamIPv4OriginalFlowResourceExceededClear,
             hwNetStreamIPv4FlexibleFlowResourceExceeded,
             hwNetStreamIPv4FlexibleFlowResourceExceededClear"

            REVISION  "202206101652Z"        --  Jun 10, 2022 at 16:53 GMT
            DESCRIPTION   
            "add 6 reasonid for hwLCfwdResourceOverload: 
             hqosBrasSlotSessionCarOverload(1018),
             hqosBrasNpSessionCarOverload(1019),
             hqosBrasSlotFamilyCarOverload(1020),
             hqosBrasNpFamilyCarOverload(1021),
             hqosBrasSessionCarStatOverload(1022),
             hqosBrasFamilyCarStatOverload(1023)."
           
           REVISION "202206072026Z"   -- Jun 7, 2022 at 20:26 GMT
           DESCRIPTION
            "add hwSaidPingPktModifiedAlarm,hwSaidPingDetectInterface"
            

            REVISION "202206021435Z"        --  Jun 2, 2022 at 14:35 GMT
            DESCRIPTION
            "add 1 reasonid for peerGroupRes(1017)"

            REVISION "202205171620Z"        --  May 17, 2022 at 16:20 GMT
            DESCRIPTION
            "add 2 reasonid for ifitAclRes(1015),
              ifitInstanceRes(1016)"

            REVISION "202205131431Z"        --  May 13, 2022 at 14:31 GMT
            DESCRIPTION
            "add 10 reasonid for hwLCfwdResourceOverload:
            l2tpLacSessionExceed90Threshold(1005)
            l2tpLacSessionExceed100Threshold(1006)
            l2tpLnsSessionExceed90Threshold(1007)
            l2tpLnsSessionExceed100Threshold(1008)
            l2tpLnsTunnelBoardSessionExceed90Threshold(1009)
            l2tpLnsTunnelBoardSessionExceed100Threshold(1010)
            l2tpLacTunnelExceed90Threshold(1011)
            l2tpLacTunnelExceed100Threshold(1012)
            l2tpLnsTunnelExceed90Threshold(1013)
            l2tpLnsTunnelExceed100Threshold(1014)" 
    
            REVISION "202204221747Z"        -- April 22, 2022 at 17:47GMT 
            DESCRIPTION 
            "add  dlbResOverLoad ."

            REVISION "202204020945Z"        -- April 2, 2022 at 09:45GMT 
            DESCRIPTION 
                "change OBJECT hwPacketChangeInPort's SYNTAX from InterfaceIndex to Unsigned32,
                change OBJECT hwPacketChangeOutPort's SYNTAX from InterfaceIndex to Unsigned32." 	

            REVISION "202203141818Z"        --  March 14, 2022 at 18:18 GMT
            DESCRIPTION
            "add 10 reasonid for apn6MappingResOverload:
            apn6TrafficSteeringMapOverLoad(994),
			apn6InterfaceMapOverLoad(995),
			apn6VPNPeerMapOverLoad(996),
			apn6TrafficIsolationMapOverLoad(997),
			apn6IsolationStatisticsOverLoad(998),
			apn6TrafficSteeringMapExceedThreshold(999),
			apn6InterfaceMapExceedThreshold(1000),
			apn6VPNPeerMapExceedThreshold(1001),
			apn6TrafficIsolationMapExceedThreshold(1002),
			apn6IsolationStatisticsExceedThreshold(1003)" 
			  
            REVISION "202202281606Z"        --  Feb 28, 2022 at 16:06GMT 
            DESCRIPTION
            " add 1 reasonid for hwFwdResLackReasonId:
              tunnelV6DecapsulationRes(993)" 

            REVISION "202202081606Z"        -- Feb 8, 2022 at 16:06GMT 
            DESCRIPTION 
                "add OBJECT hwPacketChange ." 	

            REVISION "202112310900Z"        -- Dec 31, 2021 at 09:00 GMT 
            DESCRIPTION 
            " add reasonid oam1agvlanbcResourceOverLoad(992)" 

	    REVISION "202111231400Z"   -- Nov 23, 2021 at 14:00 GMT
            DESCRIPTION
	     "modifiy description of REVISION 202111051400Z, change ifitNativeIpFlowRes(71) to ifitNativeIpFlowRes(971) "

	    REVISION "202111191500Z"   -- Nov 19, 2021 at 15:00 GMT
            DESCRIPTION
	     "add hwEMDIResLack,hwEMDIResLackResume,hwEMDISlotStr,hwEMDIResUsed,hwEMDIResTotal"

	    REVISION "202111101500Z"        --  Nov 10, 2021 at 15:00 GMT
            DESCRIPTION
	     "add 3 reasonid for hwFwdResLackReasonId:
              vxlanVpiOverThreshold(989),
              vxlanVpOverThreshold(990),
              vxlanTunnelOverThreshold(991)"

            REVISION "202111091400Z"        --  Nov 9, 2021 at 14:00 GMT  
            DESCRIPTION
            "add hwNvo3VxlanSrcIpDiffAlarm,hwNvo3VxlanSrcIpDiffAlarmResume,hwVxlanTnlPeerIpAddr"

            REVISION "202111051400Z"        -- Nov 05, 2021 at 14:00 GMT 
            DESCRIPTION 
            "Delete reasonid ifitDynFlowNumExceedThreshold(989), ifitFlowStatisticsNumExceedThreshold(972). Rename ifitFlowStatisticsNumOverLoad(971) to ifitNativeIpFlowRes(971),  ifitDynFlowNumOverLoad(988) to ifitDynFlowRes(988)" 

            REVISION "202111021500Z"        -- Nov 02, 2021 at 15:00 GMT 
            DESCRIPTION 
            "add reasonid ifitDynFlowNumOverLoad(988), ifitDynFlowNumExceedThreshold(989)" 

            REVISION "202111010900Z"            -- Dec 21, 2020 at 15:00 GMT
            DESCRIPTION
            "add 4 reasonid for hwLCfwdResourceOverload:
            srv6Dip90PerNumOverload(984),
            srv6Dip100PerNumOverload(985),
            elineSidTblExt90PerNumOverload(986),
            elineSidTblExt100PerNumOverload(987)"

            REVISION "202108161400Z"        --  Aug 16, 2021 at 14:00 GMT
            DESCRIPTION 
            " add reasonid inboundInterfaceCar95PercentOverLoad(982), outboundInterfaceCar95PercentOverLoad(983)" 

           REVISION  "202108051200Z"        --  Aug 05, 2021 at 12:00 GMT
           DESCRIPTION   
	      "add 2 reasonid for Srv6TeFlowGroupClassMapResOverload :
	       srv6TeFlowGroupClassMapOverLoad(980),
	       srv6TeFlowGroupClassMapExceedThreshold(981)"

           REVISION "202107202300Z"        -- July 20, 2021 at 23:00 GMT
           DESCRIPTION
           "add reasonid serviceCarResOverload(979)"

           REVISION "202107161600Z"        -- July 16, 2021 at 16:00 GMT
           DESCRIPTION
           " add reasonid fibHardwareNumOverLoad(973), fib6HardwareNumOverLoad(974), fibSoftwareNumOverLoad(975), fib6SoftwareNumOverLoad(976), fibSoftwareExceedThreshold(977), fib6SoftwareNumExceedThreshold(978)" 

           REVISION "202107061600Z"        -- July 06, 2021 at 16:00 GMT 
           DESCRIPTION 
            " add reasonid ifitFlowStatisticsNumOverLoad(971), ifitFlowStatisticsNumExceedThreshold(972)" 

            REVISION "202106220900Z"        -- June 22, 2021 at 09:00 GMT 
            DESCRIPTION 
            " add reasonid bgoflowRefluenceOverLoad(968), bgoflowIpv6Int90PercentOverLoad(969), bgoflowIpv6IntOverLoad(970)" 

            REVISION "202106150900Z"        -- June 15, 2021 at 09:00 GMT 
            DESCRIPTION 
            " add reasonid     fwdLagResourceOverLoad(967)" 

            REVISION "202106051600Z" -- June 5, 2021 at 16:00 GMT
            DESCRIPTION
            "add hwBoardResCriticalThresholdExceed, hwBoardResCriticalThresholdExceedResume"

           REVISION  "202104181500Z"        --  April 18, 2021 at 15:00GMT
           DESCRIPTION  
           "add hwAclRuleThreshold, hwAclGroupThreshold, hwAclRuleResUsage, hwAclGroupResUsage, hwAclRuleExceed, hwAclRuleExceedClear, hwAclGroupExceed, hwAclGroupExceedClear"

           REVISION  "202104181500Z"        --  April 18, 2021 at 15:00GMT
           DESCRIPTION
            "add new alarm hwPingfFail" 

            REVISION "202103251000Z"        --  March 25, 2021 at 10:00 GMT
            DESCRIPTION
            "add 23 reasonid for hwSysResChangedAlarm:
                enpResModeChanged(2)
                arpResAllocationModeChanged(3)
                riotResChanged(4)
                fibv4ResChanged(5)
                l3ResAllocationModeChanged(6)
                l3IfResAllocationModeChanged(7)
                aclExResChanged(8)
                ipv6LongMaskResChanged(9)
                l3ForwardHashResChanged(10)
                uatResAllocationModeChanged(11)
                ipv6VxlanResChanged(12)
                srHashResChanged(13)
                mplsResChanged(14)
                dot1q8021pResChanged(15)
                externalTcamResChanged(16)
                uatHashResModeChanged(17)
                ethtrunkModeChanged(18)
                ingressVlanXlateModeChanged(19)
                egressVlanXlateModeChanged(20)
                qosaifabricdppModeChanged(21)
                qosBuffAutoConfigChanged(22)
                qosLosslessModeChanged(23)
                incConfigChanged(24)"

            REVISION "202103181500Z"        --  March 18, 2021 at 15:00 GMT
            DESCRIPTION
            "add 14 reasonid for hwLCfwdResourceOverload:
                userdefinedcpaclNumOverLoad(953)
                userdefinedcpaclNum90PercentOverLoad(954)
                dlpcpaclNumOverLoad(955)
                dlpcpaclNum90PercentOverLoad(956)
                microisoAclNumOverLoad(957)
                microisoAclNum90PercentOverLoad(958)
                microisoLpmNumOverLoad(959)
                microisoLpmNum90PercentOverLoad(960)
                microisoCarNumOverLoad(961)
                microisoCarNum90PercentOverLoad(962)
                microisoCarStatNumOverLoad(963)
                microisoCarStatNum90PercentOverLoad(964)
                cpaclNumOverLoad(965)
                cpaclNum90PercentOverLoad(966)"

          REVISION  "202103111700Z"        -- March 11, 2021 at 17:00 GMT
          DESCRIPTION   
	      "add 2 reasonid for Srv6ColorSliceMapResOverload:
	       srv6ColorSliceMapOverLoad(951),
	       srv6ColorSliceMapExceedThreshold(952)"

        REVISION  "202103051100Z" -- March 5, 2021 at 11:00 GMT
        DESCRIPTION  
           "add hwSessThreshold, hwSessExceed, hwSessExceedClear, hwSessThresholdExceed, hwSessThresholdExceedClear"

        REVISION "202102191600Z" -- February 19, 2021 at 16:00 GMT
        DESCRIPTION 
            "Add hwSysResChangedAlarm,hwSysResChgReasonDescription,hwSysResChgSlotStr,hwSysResChgReasonId,hwSysResChgReasonDescription"

        REVISION "202102181600Z" -- February 18, 2021 at 16:00 GMT
        DESCRIPTION
           "add 1 reasonid for hwFwdResLackReasonId:
            bierv6StatCntResOverload(949)"

        REVISION "202102181600Z" -- February 18, 2021 at 16:00 GMT
        DESCRIPTION
           "add 1 reasonid for hwFwdResLackReasonId:
            bierv6StatNseResOverload(950)"

        REVISION "202101131600Z" -- January 13, 2021 at 16:00 GMT
        DESCRIPTION
           "add 1 reasonid for hwFwdResLackReasonId:
            vxlanv6TrunkResOverLoad(658)"

        REVISION "202012231500Z"            -- Dec 23, 2020 at 15:00 GMT
        DESCRIPTION
           "add 1 reasonid for hwBoardResThresholdExceed,hwBoardResWarningThresholdExceed:
           arpFastReplyInterface(630)"
 
        REVISION "202012231500Z"            -- Dec 23, 2020 at 15:00 GMT
        DESCRIPTION
           "add 1 reasonid for hwBoardResThresholdExceed:
               ipv6IgnoreOverLoad(657)"

        REVISION "202012231500Z"            -- Dec 23, 2020 at 15:00 GMT
        DESCRIPTION
           "add 6 reasonid for hwBoardResWarningThresholdExceed :
               pkteventCacheExceedThreshold(942),
               latencyeventCacheExceedThreshold(943),
               anyflowOriCacheExceedThreshold(944),
               anyflowAggreCacheExceedThreshold(945),
               anyflowFLCCacheExceedThreshold(946),
               taCacheExceedThreshold(947)"

        REVISION "202012211800Z"            -- Dec 21, 2020 at 18:00 GMT
        DESCRIPTION
           "add 5 reasonid for hwBoardResThresholdExceed:
               icibppTable(581),
               icibTable(582),
               isemTable(583),
               ecibTable(587),
               ecibextTable(588)"

        REVISION "202012211600Z"            -- Dec 21, 2020 at 15:00 GMT
        DESCRIPTION
           "add 4 reasonid for hwBoardResThresholdExceed,hwBoardResWarningThresholdExceed:
           fibv6NumWarning(624),
           level-1FEC(633),
           level-2FEC(634),
           level-3FEC(636)"

         REVISION "202012161800Z"          --  Dec 16, 2020 at 18:00 GMT
         DESCRIPTION   
            "add 1 reasonid for hwLCfwdResourceOverload:
            ifCarAclOverLoad(941)"

       REVISION  "202010261000Z"        --  Oct 26, 2020 at 10:00 GMT
       DESCRIPTION   
            "add 2 reasonid for hwBoardFwdResThresholdExceed, hwLCfwdResourceOverload:
            segmentlistSliceMapOverLoad(934),
            segmentlistSliceMapExceedThresHold(935)"

        REVISION "202008261600Z" -- August 26, 2020 at 16:00 GMT
        DESCRIPTION
           "add 1reasonid for hwBoardFwdResThresholdExceed:
           sharedGqResExceed90Threshold(933)"

        REVISION "202008251500Z" -- August 25, 2020 at 15:00 GMT
        DESCRIPTION
           "add 6 reasonid for SysfwdResourceOverload, hwWholeFwdResThresholdExceed, hwLCfwdResourceOverload, hwBoardFwdResThresholdExceed:
           bierv6TmgidOverLoad(927),
           bierv6TmgidExceedThresHold(928),
           bierv6VpnOverLoad(929),
           bierv6Ilmv6OverLoad(930),
           bierv6VpnExceedThresHold(931),
           bierv6Ilmv6ExceedThresHold(932)"

         REVISION "202008241900Z" -- August 24, 2020 at 19:00 GMT
         DESCRIPTION
           "add 6 reasonid for SysfwdResourceOverload, hwWholeFwdResThresholdExceed, hwLCfwdResourceOverload, hwBoardFwdResThresholdExceed:
           mcBierv6TmgidOverLoad(831),
           mcBierv6TmgidExceedThresHold(773),
           mcBierv6VpnOverLoad(924),
           mcBierv6Ilmv6OverLoad(925),
           mcBierv6VpnExceedThresHold(925),
           mcBierv6Ilmv6ExceedThresHold(926)"


         REVISION  "202008201900Z"        --  August 20, 2020 at 19:00 GMT
         DESCRIPTION   
            "add 2 reasonid for hwFwdResLackReasonId:
            inLabelMaplResOverLoad(925),
            labelTermResOverLoad(926)"

          REVISION  "202008181700Z"        --  August 18, 2020 at 17:00 GMT
          DESCRIPTION   
            "add 2 reasonid for Srv6SliceResOverload:
            srv6SliceOportinfoOverLoad(923),
            srv6SliceOportinfoExceedThreshold(924)"

         REVISION "202008050900Z"        --  August 05, 2020 at 09:00 GMT
         DESCRIPTION
            "add 1 reasonid for hwFwdResLackReasonId:
             vxlanMcTable(922)"

          REVISION "202007281700Z"        --  July 28, 2020 at 17:00 GMT
          DESCRIPTION
           "modify fowarding as forwarding"

          REVISION "202007281000Z"        --  July 28, 2020 at 10:00 GMT 
          DESCRIPTION
           "modify fowarding as forwarding"

          REVISION "202007241000Z"        --  July 24, 2020 at 10:00 GMT 
          DESCRIPTION
           "delete microIsolationPortCarLPMResOverLoad
                       microIsolationPortCarResOverLoad
                       microIsolationPortCarStatResOverLoad
                       microIsolationPortCarLPMResExceed90ThresHold
                       microIsolationPortCarResExceed90ThresHold
                       microIsolationPortCarStatResExceed90ThresHold"

          REVISION "202007201000Z"        --  July 20, 2020 at 10:00 GMT  
          DESCRIPTION
            "add node:
               hwNsOrigFlexFlowExceedAlarm
               hwNsOrigFlexFlowExceedResume
               hwNsAggFlowExceedAlarm
               hwNsAggFlowExceedResume"         

            REVISION "202007171000Z"        --  May 8, 2020 at 10:00 GMT 
            DESCRIPTION
           "delete microIsolationProtocalCarLPMResOverLoad
                    microIsolationProtocalCarIPv4ACLResOverLoad
                    microIsolationProtocalCarIPv6ACLResOverLoad
                    microIsolationProtocalCarL2ACLResResOverLoad
                    microIsolationProtocalIPv4CarResOverLoad
                    microIsolationProtocalIPv4CarStatResOverLoad
                    microIsolationProtocalCarLPMResExceed90ThresHold
                    microIsolationProtocalCarIPv4ACLResExceed90ThresHold
                    microIsolationProtocalCarIPv6ACLResExceed90ThresHold
                    microIsolationProtocalCarL2ACLResResExceed90ThresHold
                    microIsolationProtocalIPv4CarResExceed90ThresHold
                    microIsolationProtocalIPv4CarStatResExceed90ThresHold
                    microIsolationProtocalIPv6CarResOverLoad
                    microIsolationProtocalL2CarResOverLoad
                    microIsolationProtocalIPv6CarStatResOverLoad
                    microIsolationProtocalL2CarStatResOverLoad
                    microIsolationProtocalIPv6CarResExceed90ThresHold
                    microIsolationProtocalL2CarResExceed90ThresHold
                    microIsolationProtocalIPv6CarStatResExceed90ThresHold
                    microIsolationProtocalL2CarStatResExceed90ThresHold"

            REVISION "202006291500Z"        --  June 29, 2020 at 15:00 GMT  
            DESCRIPTION
            "modify 2 reasonid for hwLCfwdResourceOverload:
                cpIPv4AndIPv6AclNum90Overload(920)
               cpIPv4AndIPv6AclNumOverload(921)"
 
            REVISION "202005261500Z"        --  May 26, 2020 at 15:00 GMT    
            DESCRIPTION
            "add 15 reasonid for hwBoardFwdResThresholdExceed, hwLCfwdResourceOverload:
                microIsolationPortCarLPMResOverLoad(889)
                microIsolationProtocalCarLPMResOverLoad(890)
                microIsolationProtocalCarIPv4ACLResOverLoad(891)
                microIsolationProtocalCarIPv6ACLResOverLoad(892)
				microIsolationProtocalCarL2ACLResResOverLoad(893)
				microIsolationPortCarResOverLoad(894)
				microIsolationProtocalIPv4CarResOverLoad(895)
				microIsolationPortCarStatResOverLoad(896)
				microIsolationProtocalIPv4CarStatResOverLoad(897)
				microIsolationPortCarLPMResExceed90ThresHold(898)
				microIsolationProtocalCarLPMResExceed90ThresHold(899)
				microIsolationProtocalCarIPv4ACLResExceed90ThresHold(900)
				microIsolationProtocalCarIPv6ACLResExceed90ThresHold(901)
				microIsolationProtocalCarL2ACLResResExceed90ThresHold(902)
				microIsolationPortCarResExceed90ThresHold(903)
				microIsolationProtocalIPv4CarResExceed90ThresHold(904)
				microIsolationPortCarStatResExceed90ThresHold(905)
				microIsolationProtocalIPv4CarStatResExceed90ThresHold(906)
				microIsolationProtocalIPv6CarResOverLoad(912)
				microIsolationProtocalL2CarResOverLoad(913)
				microIsolationProtocalIPv6CarStatResOverLoad(914)
				microIsolationProtocalL2CarStatResOverLoad(915)
				microIsolationProtocalIPv6CarResExceed90ThresHold(916)
				microIsolationProtocalL2CarResExceed90ThresHold(917)
				microIsolationProtocalIPv6CarStatResExceed90ThresHold(918)
				microIsolationProtocalL2CarStatResExceed90ThresHold(919)"

            REVISION "202005251500Z"        --  May 25, 2020 at 15:00 GMT   
            DESCRIPTION
            "modify 5 reasonid for hwFwdResLackReasonId:
                inTM8QueueSqResExhausted(907)
                inTM8QueueEnhanceSqResExhausted(908)
                outTM4QueueSqResExhausted(909)
                outTM8QueueSqResExhausted(910)
                outTM8QueueEnhanceSqResExhausted(911)" 

           REVISION "202005081000Z"        --  May 8, 2020 at 10:00 GMT  
           DESCRIPTION
           "delete hwMlagLinkLocalConflictDetectAlarm"

           REVISION "202004281000Z"        --  April 28, 2020 at 10:00 GMT  
           DESCRIPTION
           "add 1 reasonid for hwFwdResLackReasonId:  
             fibResOverLoad(656)"


            REVISION "202004161500Z"        --  April 16, 2020 at 15:00 GMT
            DESCRIPTION
            "add 15 reasonid for hwWholeFwdResLack, hwWholeFwdResThresholdExceed, hwBoardFwdResLack, hwBoardFwdResThresholdExceed:
                mcidResWarning(875)
                vsiResWarning(876)
                vpResWarning(877)
                macResWarning(878)"


            REVISION "202004132020Z"        --  April 13, 2020 at 20:20 GMT  
            DESCRIPTION
            "modify 15 reasonid for hwFwdResLackReasonId:
                inSlot8QueueSqResExceed90ThresHold(860)
                inSlot8QueueEnhanceSqResExceed90ThresHold(861)
                inTM8QueueSqResExceed90ThresHold(862)
                inTM8QueueEhanceSqResExceed90ThresHold(863)
                outSlot4QueueSqResExceed90ThresHold(864)
                outSlot8QueueSqResExceed90ThresHold(865)
                outSlot8QueueEnhanceSqResExceed90ThresHold(866)
                outTM4QueueSqResExceed90ThresHold(867)
                outTM8QueueSqResExceed90ThresHold(868)
                outTM8QueueEnhanceSqResExceed90ThresHold(869)
                in8QueueSqResExhausted(870)
                in8QueueEnhanceSqResExhausted(871)
                out4QueueSqResExhausted(872)
                out8QueueSqResExhausted(873)
                out8QueueEnhanceSqResExhausted(874)"  

           REVISION "202004071109Z"        -- April 07, 2020 at 11:09 GMT
           DESCRIPTION 
           "Add  hwAutoDiagnoseReasonId 3." 

            REVISION "202003241020Z"        --  March 24, 2020 at 10:20 GMT    
            DESCRIPTION
            "add 15 reasonid for hwFwdResLackReasonId:
                inSlot8QueueSqResOverLoad(860)
                inSlot8QueueEnhanceSqResOverLoad(861)
                inTM8QueueSqResOverLoad(862)
                inTM8QueueEhanceSqResOverLoad(863)
                outSlot4QueueSqResOverLoad(864)
                outSlot8QueueSqResOverLoad(865)
                outSlot8QueueEnhanceSqResOverLoad(866)
                outTM4QueueSqResOverLoad(867)
                outTM8QueueSqResOverLoad(868)
                outTM8QueueEnhanceSqResOverLoad(869)
                in8QueueSqResExceed90ThresHold(870)
                in8QueueEnhanceSqResExceed90ThresHold(871)
                out4QueueSqResExceed90ThresHold(872)
                out8QueueSqResExceed90ThresHold(873)
                out8QueueEnhanceSqResExceed90ThresHold(874)"

            REVISION "202003180900Z"        --  March 18, 2020 at 09:00 GMT
            DESCRIPTION
            "add 1 parameter for hwMlagLinkLocalConflictDetectAlarm:
             hwMlagConflictLinkLocalVpnName"

            REVISION "202003120900Z"        --  March 12, 2020 at 09:00 GMT
            DESCRIPTION
            "add 1 reasonid for hwFwdResLackReasonId:
             vplsMcTable(859)"

             REVISION "202002240900Z"        --  February 24, 2020 at 09:00 GMT
             DESCRIPTION 
             "add 3 reasonid for hwFwdResLackReasonId: 
              arpResOverLoad(856), 
              ndResOverLoad(857),
              fibv4NumPercentOverLoad(858)" 

            REVISION "202002140900Z"        --  February 14, 2020 at 09:00 GMT  
            DESCRIPTION
            "update hwFibDeliverFailed,hwFibDeliverFailedResume,hwFibDeliverSlotId"

            REVISION "202002130900Z"        --  February 13, 2020 at 09:00 GMT  		 
            DESCRIPTION
            "update hwEthernetRouterDownFailed,hwEthernetRouterDownFailedResume,hwEthernetRouteSlotId"

            REVISION "202001220900Z"        --  January 22, 2020 at 09:00 GMT    
            DESCRIPTION
            "update hwMlagLinkLocalConflictDetectAlarm,hwMlagLinkLocalConflictDetectAlarmResume,hwConflictLinkLocalAddress"

            REVISION  "202001211920Z"        --  January 21, 2020 at 19:20 GMT   
            DESCRIPTION   
            "update 2 reasonid  for  IpVpnResOverload:
               ipv4vpnTable(854),
               ipv6vpnTable(855)"       

            REVISION  "202001031920Z"        --  January 3, 2020 at 19:20 GMT 
            DESCRIPTION   
            "add 2 reasonid  for  IpVpnResOverload:
               ipv4vpnTable(854),
               ipv6vpnTable(855)"

            REVISION  "201912102110Z"        --  December 10, 2019 at 21:10 GMT 
            DESCRIPTION   
            "add 4 reasonid  for  Srv6ServChainResOverload:
               srv6ServChainL3ReOverLoad(850),
               srv6ServChainL3ReExceedThreshold(851),
               srv6ServChainL2ReOverLoad(852),
               srv6ServChainL2ReExceedThreshold(853)"

            REVISION  "201912051130Z"        --  December 5, 2019 at 11:30 GMT  
            DESCRIPTION   
            "add 2 reasonid  for  Vxlanv6ResOverload:
               vxlanv6DecapOverLoad(848),
               vxlanv6DecapExceedThreshold(849)"

            REVISION "201910171515Z"        -- Oct 17, 2019 at 15:15GMT 
            DESCRIPTION 
                "add OBJECT hwNvo3VxlanNveMacConflict ." 	

            REVISION "201909282229Z"        -- Sep 28, 2019 at 22:29GMT
            DESCRIPTION 
            "Add hwEcmpMemberLimitOverThresholdAlarm." 

            REVISION  "201909251050Z"        --  Septempber 25, 2019 at 10:50 GMT  
            DESCRIPTION   
            "add 2 reasonid  for  Srv6ResOverload:
               srv6ListOverLoad(844),
               srv6ListExceedThreshold(845),
               srv6PolicyStatResOverLoad(846),
               srv6PolicyStatResExceedThreshold(847)"

            REVISION  "201909241110Z"        --  Septempber 24, 2019 at 11:10 GMT
            DESCRIPTION   
            "del object{} for hwMplsLabelExceedAlarm,hwMplsLabelExceedAlarmResume"

            REVISION  "201909171540Z"        --  Septempber 17, 2019 at 15:40 GMT
            DESCRIPTION   
            "add 10 reasonid  for  Srv6ResOverload:
               localSidOverLoad(653),
               localSidExceedThreshold(835),
               remoteSidOverLoad(836),
               remoteSidExceedThreshold(837),
               teleScan30sOverLoad(838),
               teleScan30sExceedThreshold(839),
               teleScan1sOverLoad(840),
               teleScan1sExceedThreshold(841),
               srv6policyRdrREOverLoad(842),
               srv6policyRdrREExceedThreshold(843)"

            REVISION  "201909171414Z"        --  Septempber 17, 2019 at 14:14 GMT
            DESCRIPTION   
            "add 2 reasonid  for  hwBoardMcResLack, hwBoardMcResLackResume, hwBoardMcResFull:
              l3intflistTable(831),
              mcpmskTable(832)"

            REVISION  "201909101109Z"        --  Septempber 10, 2019 at 11:09 GMT
            DESCRIPTION   
            "add 2 reasonid  for  localArpv6ResOverload:
              localArpv6OverLoad(831),
              localArpv6ExceedThreshold(832)"

            REVISION  "201908291109Z"        --  August 29, 2019 at 11:09 GMT
            DESCRIPTION   
            "add 17 reasonid  for  tmgidResOverload:
              l2TrunkLbTmgidResOverLoad(814),
              vlanL2mcRpTmgidResOverLoad(815),
              vsiL2mcRpTmgidResOverLoad(816),
              bdL2mcRpTmgidResOverLoad(817),
              vsiL2mcBakPwTmgidResOverLoad(818),
              pimFrrTmgidResOverLoad(819),
              vlanL2mcv6RpTmgidResOverLoad(820),
              vsiL2mcv6RpTmgidResOverLoad(821),
              l2mcStkMapTmgidResOverLoad(822),
              brasMcHwTmgidResOverLoad(823),
              mcNatTmgidResOverLoad(824),
              ucDsvpnGroupOverLoad(825),
              bdTmgidResOverLoad(826),
              hwmcTmgidResOverLoad(827),
              vlanTmgidResOverLoad(828),
              l2vpnTmgidResOverLoad(829),
              l2vpnApsTmgidResOverLoad(830)"

            REVISION "201907261109Z"        -- July 21, 2019 at 11:09 GMT
            DESCRIPTION 
            "Add  hwAutoDiagnoseReasonId ( 1 , 2 )." 

            REVISION "201907171109Z"        -- July 21, 2019 at 11:09 GMT
            DESCRIPTION 
            "Add hwAutoDiagnoseAlarm,hwAutoDiagnoseAlarmResume hwAutoDiagnoseReasonId ." 

           REVISION "201906281410Z"        -- June 28, 2019 at 14:10GMT
           DESCRIPTION 
           "Add  srpolicyStatExceedThresHold,srpolicyStatOverLoad."

           REVISION "201906051116Z"        --  June 5, 2019 at 11:16GMT
           DESCRIPTION 
           "add 16 reasonid  for hwLCfwdResourceOverload:                
               inProfSingleCarPre(778),
               outProfSingleCarPre(779),
               inProfSingleCarStatPre(780),
               outProfSingleCarStatPre(781),
               tlmtActCar100ms(800),
               tlmtActCar100msPre(801),
               tlmtActCar1s(802),
               tlmtActCar1Pre(803),
               tlmtActCar30s(804),
               tlmtActCar30Pre(805),
               tlmtPolicy100ms(806),
               tlmtPolicy100msPre(807),
               tlmtPolicy1s(808),
               tlmtPolicy1Pre(809),
               tlmtPolicy30s(810),
               tlmtPolicy30Pre(811)"
           
           REVISION "201905081618Z"        --  May 8, 2019 at 16:18GMT
           DESCRIPTION 
           "add 1 reasonid : vxlanvpTable(777)."

           REVISION "201905061005Z"        --  May 6, 2019 at 10:05GMT
           DESCRIPTION 
           "Add  mcEgressStatOverLoad,mcEgressStatExceedThresHold."

           REVISION "201904191047Z"        --  Apr 19, 2019 at 10:47GMT
           DESCRIPTION   
           "add 7 reasonid  for  hwWholeFwdResLack, hwWholeFwdResThresholdExceed, hwBoardFwdResLack, hwBoardFwdResThresholdExceed:
            mcBierVpnOverLoad(768),
            mcBierTunnelOverLoad(769),
            mcBierTmgidOverLoad(770),
            mcBierVpnExceedThresHold(771),
            mcBierTmgidExceedThresHold(772),
            mcBierBitMaskOverLoad(773),
            mcBierBitMaskExceedThresHold(774)"

            REVISION "201812221247Z"        -- DEC 22, 2018 at 12:47GMT
            DESCRIPTION 
            "Modify hwMplsLabelExceedAlarm,hwMplsLabelExceedAlarmResume" 
			
            REVISION "201812181137Z"        -- DEC 18, 2018 at 11:37 GMT
            DESCRIPTION 
            "Add  hwMplsLabelExceedAlarm,hwMplsLabelExceedAlarmResume" 
			
           REVISION  "201812062200Z"        --  DEC 6, 2018 at 22:00GMT
           DESCRIPTION   
            "add 1 reasonid : ipv6DefipTable(767) "


           REVISION  "201812031600Z"        --  DEC 3, 2018 at 16:00GMT
           DESCRIPTION   
           "add hwMcLeafCfcCheck, hwMcLeafCfcCheckTrap, hwMcLeafCfcCheck, hwMcLeafCfcCheckResume" 
		   
           REVISION  "201811281500Z"        --  DEC 28, 2018 at 15:00GMT
           DESCRIPTION   
           "add 8 reasonid  for hwLCfwdResourceOverload: 
            hqosSessionCaridOverload(759),
            hqosFamilyCaridOverload(760),
            hqosVcpeL2CaridOverload(761),
            hqosVcpeL3CaridOverload(762),
            hqosSessionCarStatidOverload(763),
            hqosFamilyCarStatidOverload(764),
            hqosVcpeL2CarStatidOverload(765),
            hqosVcpeL3CarStatidOverload(766)" 


           REVISION  "201811271600Z"        --  Nov 27, 2018 at 16:00GMT
           DESCRIPTION   
            "add hwBoardMcResLack,hwBoardMcResLackResume"

           REVISION  "201811231500Z"        --  Nov 23, 2018 at 15:00GMT
           DESCRIPTION   
            "add hwEMDIIndicatorOverThreshold,hwEMDIIndicatorOverThresholdResume,hwEMDIReceiveDuplicatePackets,hwEMDIReceiveDuplicatePacketsResume,hwEMDIInstanceId,hwEMDIIndicatorType,hwEMDIIndicatorValue,hwEMDIThreshold" 

           REVISION  "201811091500Z"        --  Nov 09, 2018 at 15:00GMT
           DESCRIPTION   
           "add hwProducerComponentName,hwConsumerComponentName,hwSmoothFailedReasonId,hwFwdComponentSmoothFailed,hwFwdComponentSmoothFailedClear" 

           REVISION  "201810151500Z"        --  Oct 15, 2018 at 15:00GMT
           DESCRIPTION   
           "add 4 reasonid  for hwLCfwdResourceOverload: 
            secV6sessioncarResOverload(738),
            secV6sessioncarRes90Overload(739),
            secV6sessioncarStatOverload(740),
            secV6sessioncarStat90Overload(741)" 

           REVISION  "201810131500Z"        --  Oct 13, 2018 at 15:00GMT
           DESCRIPTION   
           "add new alarm hwBoardMcResFull,hwBoardMplsFwdResFull,hwBoardL3ResFull" 

           REVISION  "201808301530Z"        --  August 30, 2018 at 15:30GMT
           DESCRIPTION   
           "modify reasonid for hwLCfwdResourceOverload :l3mcLeafNumberExceed90OverLoad(736),add reasonid for hwLCfwdResourceOverload :l3mcLeafNumberOverLoad(737)" 

           REVISION  "201808271530Z"        --  August 27, 2018 at 15:30GMT
           DESCRIPTION   
           "add 1 reasonid for hwLCfwdResourceOverload :l3mcLeafNumberOverLoad(733)"  
           
           REVISION  "201808081530Z"        --  August 15, 2018 at 15:30GMT
           DESCRIPTION   
           "add new alarm hwSidResourceThresholdExceed, hwSidResourceThresholdExceedClear, hwSidResourceTotalCountExceed, hwSidResourceTotalCountExceedClear to group"   

           REVISION  "201808071530Z"        --  August 07, 2018 at 15:30GMT
           DESCRIPTION   
           "add new alarm hwSidResourceThresholdExceed, hwSidResourceThresholdExceedClear, hwSidResourceTotalCountExceed, hwSidResourceTotalCountExceedClear"   

           REVISION  "201807091530Z"        --  July 09, 2018 at 15:30GMT
           DESCRIPTION   
           "add 1 reasonid for hwLCfwdResourceOverload and 1 reasonid for hwBoardFwdResThresholdExceed:L3mcV4MreCloneStatResOverLoad(731),
            L3mcV4MreCloneStatResExceedThresHold(732)"     

           REVISION  "201804281600Z"        --  Apr 28, 2018 at 16:00GMT 
           DESCRIPTION    
           "add 3 reasonid for hwLCfwdResourceOverload and 3 reasonid for hwBoardFwdResThresholdExceed: 
           hqosVirtualSQOverLoad(715),hqosVirtualGQOverLoad(716),hqosVirtualVIOverLoad(717),hqosVirtualSQExceedThresHold(718),
           hqosVirtualGQExceedThresHold(719),hqosVirtualVIExceedThresHold(720)" 
           
           REVISION  "201804251940Z"        --  Apr 25, 2018 at 19:40GMT
           DESCRIPTION   
           "add four reasonid for hwLCfwdResourceOverload and four reasonid for hwBoardFwdResThresholdExceed: l3ucVpnSIdIpV6AddrOverLoad(721),
           l3ucNhrpNetworkIdIndexOverLoad(722),
           l3ucVpnSIdIpV6AddrExceedThresHold(723),
           l3ucNhrpNetworkIdIndexExceedThresHold(724)"
           
           REVISION  "201803012007Z"        --  Mar 15, 2018 at 09:00GMT
           DESCRIPTION   
           "add four reasonid for hwLCfwdResourceOverload and four reasonid for hwBoardFwdResThresholdExceed:L3mcV4MreStatResOverLoad(707),
           L3mcV6MreStatResOverLoad(708), L3mcV4MREEXTResOverLoad(709), L3mcV6MREEXTResOverLoad(710), L3mcV4MreStatResExceedThresHold(711),
           L3mcV6MreStatResExceedThresHold(712), L3mcV4MREEXTResExceedThresHold(713), L3mcV6MREEXTResExceedThresHold(714)"

           REVISION  "201803012007Z"        --  Mar 15, 2018 at 09:00GMT
           DESCRIPTION   
           "add one reasonid for SysfwdResourceOverload: l2mcTmgidOverThresHold(605)"

           REVISION  "201803012007Z"        --  Mar 1, 2017 at 20:07 GMT 
           DESCRIPTION   "modify authority for hwTblResInfoTable "

           REVISION  "201802261157Z"        --  Feb 26, 2018 at 11:57GMT
           DESCRIPTION    
           "add hwTrunkWeightExceed" 
		   
           REVISION  "201802091138Z"        --  Feb 9, 2018 at 11:38GMT
           DESCRIPTION    
           "add hwBoardMplsFlowLabelNonSupp" 

           REVISION  "201801040900Z"        --  Jan 15, 2018 at 09:00GMT
           DESCRIPTION  
           "add two reasonid for hwLCfwdResourceOverload and hwBoardFwdResThresholdExceed:mcHotstanbyResOverLoad(700),
           mcHotstanbyResOverLoad(703).
           add four reasonid for SysfwdResourceOverload and hwWholeFwdResThresholdExceed:l3mcV4TmgidResOverLoad(701),
           l3mcV6TmgidResOverLoad(702), l3mcV4TmgidResOverLoad(704), l3mcV6TmgidResOverLoad(705)"

           REVISION  "201801040900Z"        --  Jan 4, 2018 at 09:00GMT
           DESCRIPTION  
           "add hwFwdSessionResUsage and modify hwFwdSessionResLack, hwFwdSessionResLackResume"
          
           REVISION  "201712140900Z"        -- Dec 14, 2017 at 09:00GMT
           DESCRIPTION  
           "modify hwResourceOverwrittenAlarmResume"

           REVISION  "201712091300Z"        --  Dec 9, 2017 at 13:00GMT
           DESCRIPTION  
           "add hwFwdResCongestReasonId, hwFwdResLackFeNodeId, hwFwdResMsgCongestTrap, 
           hwBoardFwdMsgCongest , hwBoardFwdMsgCongestResume.
           add four reasonid for hwFwdResCongestReasonId:FESDetectMsgCongest(1),
           EUMDetectMsgCongest(2),	RMDetectMsgCongest(3), VSTMDetectMsgCongest(4)"

           REVISION  "201712061130Z"        --  Dec 6, 2017 at 11:30GMT
           DESCRIPTION 
           "add reasonid for hwFwdResLackReasonId: NetEapUserResLac(670)"

           REVISION  "201711281650Z"        --  Nov 28, 2017 at 16:50GMT
           DESCRIPTION 
           "add reasonid for hwFwdResLackReasonId: vpnVclabelResExceedThresHold(613)"


           REVISION  "201711221650Z"        --  Nov 22, 2017 at 16:50GMT
           DESCRIPTION 
           "add reasonid for hwFwdResLackReasonId: dsvpnNhrpsulationRes(610), dsvpnResOverLoad(611),dsvpnResExceedThresHold(612)"

           REVISION  "201711161555Z"        --  Nov 16, 2017 at 15:55GMT
           DESCRIPTION  
           "add hwResOverwrittenSlot, hwResOverwrittenResType, hwResourceOverwrittenTrap, hwResourceOverwrittenAlarm, hwResourceOverwrittenAlarmResume"

           REVISION  "201711131018Z"        --  Nov 13, 2017 at 10:18GMT
           DESCRIPTION  
           "add hwFwdResIncomReasonId, hwFwdResIncompTrap, hwFwdDataSyncIncomplete, hwFwdDataSyncIncompleteResume"

            REVISION  "201711032007Z"        --  Nov 3, 2017 at 20:07 GMT 
           DESCRIPTION   "add a table for hwTblResInfoTable "

            REVISION  "201708172108Z"        --  Aug 17, 2017 at 21:08 GMT 
           DESCRIPTION   "modify english description "

           REVISION  "201708081100Z"        --  Aug 8, 2017 at 11:00GMT 
           DESCRIPTION   
           "add two reasonids for hwFwdResLackReasonId : ipv4O6TnlDecapTblResOverLoad(608), ipv4O6TnlIpv6AddrTblResOverLoad(609)"

           REVISION  "201707272006Z"        --  July 27, 2017 at 20:06GMT 
           DESCRIPTION   
           "add hwBoardL3FIBResLack"

           REVISION  "201706222010Z"        --  June 22, 2017 at 20:10GMT 
           DESCRIPTION   
           " add a reasonid for hwFwdResLackReasonId for ecmp resource: ecmpreswarning(579)" 

           REVISION  "201706222010Z"        --  June 22, 2017 at 20:10GMT 
           DESCRIPTION   
           " add a reasonid for hwFwdResLackReasonId for nhp resource: nhpreswarning(580)" 	
	 
           REVISION  "201705181015Z"        --  May 18, 2017 at 10:15GMT 
           DESCRIPTION   
           "add hwBoardL3NDResLack,hwFwdResLackIPStr,hwFwdResLackVrfId"

           REVISION  "201703222010Z"        --  Mar 22, 2017 at 20:10GMT 
           DESCRIPTION   
           " add a reasonid for hwFwdResLackReasonId : userNumberResLack(582)" 

           REVISION  "201703222010Z"        --  Mar 22, 2017 at 20:10GMT 
           DESCRIPTION   
           " add a reasonid for hwFwdResLackReasonId : lacUserNumberResLack(583)" 

           REVISION  "201703222010Z"        --  Mar 22, 2017 at 20:10GMT 
           DESCRIPTION   
           " add a reasonid for hwFwdResLackReasonId : l2VcpeUserNumberResLack(584)" 

           REVISION  "201703222010Z"        --  Mar 22, 2017 at 20:10GMT 
           DESCRIPTION   
           " add a reasonid for hwFwdResLackReasonId : tnlResVcpeUserResLack(585)" 

           REVISION  "201703222010Z"        --  Mar 22, 2017 at 20:10GMT 
           DESCRIPTION   
           " add a reasonid for hwFwdResLackReasonId : fibNumberVcpeUserResLack(586)" 

           REVISION  "201703222010Z"        --  Mar 22, 2017 at 20:10GMT 
           DESCRIPTION   
           " add a reasonid for hwFwdResLackReasonId : card0UserExceed90ThresHold(587)" 

           REVISION  "201703222010Z"        --  Mar 22, 2017 at 20:10GMT 
           DESCRIPTION   
           " add a reasonid for hwFwdResLackReasonId : card1UserExceed90ThresHold(588)" 

           REVISION  "201703222010Z"        --  Mar 22, 2017 at 20:10GMT 
           DESCRIPTION   
           " add a reasonid for hwFwdResLackReasonId : card0UserExceedThresHold(589)" 

           REVISION  "201703222010Z"        --  Mar 22, 2017 at 20:10GMT 
           DESCRIPTION   
           " add a reasonid for hwFwdResLackReasonId : card1UserExceedThresHold(590)" 


           REVISION  "201703100954Z"        --  Mar 10, 2017 at 09:54GMT
           DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId : vfiTable(578)"

           REVISION  "201703031036Z"        --  Mar 03, 2017 at 10:36GMT
           DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId : macAccountingResOverLoad(577)"

           REVISION  "201702281130Z"        --  FEB 28, 2017 at 11:30GMT
           DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId : vllHardPipeResourceOverLoad(497)"

           REVISION "201701131130Z"        --  JAN 13, 2017 at 11:30GMT
           DESCRIPTION  
           "add hwNotsuppDecapVxlanFragPackets,hwNoSuppVxlanFragVni,hwNoSuppVxlanFragSourceIp,hwNoSuppVxlanFragPeerIp,hwBoardVbdifResLack,hwVxlanTnlCfgFailed,hwNotsuppDecapVxlanPackets" 

           REVISION  "201701131130Z"        --  JAN 13, 2017 at 11:30GMT
           DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId : lsL2UserEntryResOverLoad(576)"


           REVISION  "201701131130Z"        --  JAN 13, 2017 at 11:30GMT
           DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId : lsStationTcamResOverLoad(575)"


           REVISION  "201701131130Z"        --  JAN 13, 2017 at 11:30GMT
           DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId : lsEgrL3IntResOverLoad(574)"


           REVISION  "201701131130Z"        --  JAN 13, 2017 at 11:30GMT
           DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId : lsMacResOverLoad(573)"

           REVISION  "201701131130Z"        --  JAN 13, 2017 at 11:30GMT
           DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId : apsOutMirrorResOverLoad(572)"

           REVISION  "201701131130Z"        --  JAN 13, 2017 at 11:30GMT
           DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId : atmIpoaArpResOverLoad(571)"

           REVISION "201701121840Z"        --  JAN 12, 2017 at 18:40GMT
           DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId : ipv6LongerMaskResOverLoad(570)"

           REVISION "201701121540Z"        --  JAN 12, 2017 at 15:40GMT
           DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId : outVIResExceed90ThresHold(569)"

 
           REVISION "201612221000Z"        --  Dec 22, 2016 at 10:00GMT
           DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId : l2tpv3TnlResOverLoad(565)"


           REVISION "201612091137Z"        --  Dec 09, 2016 at 11:37GMT
           DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId : vlanEncapResOverload(556)"


           REVISION "201612081642Z"        -- Dec 08, 2016 at 16:42GMT
           DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId : l2tpv3TunnelResOverLoad(555)"


           REVISION "201611281537Z"        --  Nove  28, 2016 at 15:37GMT
           DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : vplsPwSuppStatOverLoad(553), vplsPwSuppStatExceed90ThresHold(554)"


            REVISION "201611181655Z"      --  Nove  18, 2016 at 16:55GMT 
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: l2ptCarResExceed90ThresHold(551),l2ptCarResOverLoad(552)" 

      
            REVISION "201611171421Z"        --  Nove  17, 2016 at 14:21GMT
            DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : vplspwHqosOverLoad(550)"


             REVISION "201611171421Z"        --  Nove  17, 2016 at 14:21GMT
            DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : vplspwHqosOverLoad"
  
  
           REVISION "201611011125Z"        -- Nov 01, 2016 at 11:25GMT  
           DESCRIPTION  
           "add reasonid for hwFwdResLackReasonId: overlayNhpResOverLoad(549) "

           REVISION "201610201625Z"        -- Oct 20, 2016 at 16:25GMT
           DESCRIPTION 
           "Add  hwFwdSessionResLack,hwFwdSessionResLackResume,hwFwdFastTableResLack,hwFwdFastTableResLackResume." 

           REVISION "201610111125Z"        -- Oct 11, 2016 at 11:25GMT  
           DESCRIPTION  
           "add reasonid for hwFwdResLackReasonId: pwifResOverLoad(548) "

           REVISION "201610091525Z"        -- Oct 09, 2016 at 15:25GMT  
           DESCRIPTION  
           "add reasonid for hwFwdResLackReasonId: insegVrfOverLoad(502),dynldbalStatOverLoad(503),communityeOverLoad(504),ipv4TunnelIndexOverLoad(505), smaAsIndexOverLoad(506),smaFibv6OverLoad(507) "

            REVISION "201609291137Z"        -- Sep 29, 2016 at 11:37GMT  
           DESCRIPTION  
           "add reasonid for hwFwdResLackReasonId: pwifResExceed90ThresHold(501) "

            REVISION "201609280937Z"        -- Sep 28, 2016 at 09:37GMT  
           DESCRIPTION  
           "add reasonid for hwFwdResLackReasonId: e2e1588Res(500) "


            REVISION "201609241804Z"        -- Sep 24, 2016 at 18:04GMT  
           DESCRIPTION  
           "add reasonid for hwFwdResLackReasonId: bfdGidNumOverLoad(498) "

            REVISION "201609231737Z"        -- Sep 23, 2016 at 17:37GMT  
           DESCRIPTION  
           "add reasonid for hwFwdResLackReasonId: vplsPwNhpResourceOverload(499) "

            REVISION "201609091447Z"        -- Sep 9, 2016 at 14:47GMT  
           DESCRIPTION  
           "add reasonid for hwFwdResLackReasonId: tunnelsourceipindex(420) "

            REVISION "201607191633Z"        -- July 19, 2016 at 16:33GMT  
           DESCRIPTION  
           "modify alarm hwFwdEntryInconsistent/hwFwdEntryInconsistentResume index: add index hwServiceIndex2, hwServiceIndex3, hwServiceIndex4 "

            REVISION "201607111201Z"        -- July 11, 2016 at 12:01GMT  
           DESCRIPTION  
           "add reasonid for hwFwdResLackReasonId: VSMIPV6AclTCAMNumFull(418),VSMIPV6AclTCAMNumExhaust(419) "

            REVISION "201606021439Z"        -- June 22, 2016 at 11:09GMT  
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: mcMfibChipEntryHashConflict(411) "

            REVISION "201606021439Z"        -- June 02, 2016 at 11:09GMT  
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: ipv4VXLANVniPeerRes(410) "


            REVISION "201605281109Z"        -- May 28, 2016 at 11:09GMT  
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: tunnelnexthop (408) "

            REVISION "201605241109Z"        -- May 24, 2016 at 11:09GMT  
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId:mcmofrrResourceNumOverLoad (406),mcmofrrResourceExceedThresHold (407) "

            REVISION "201605111109Z"        -- May 11, 2016 at 11:09GMT  
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId:CIRUserQueue(400), EIRUserQueue(401), ShapingFlowqueue (402), ShareShapingFlowqueue (403) "

            REVISION "201604081609Z"        -- Apr 08, 2016 at 16:09GMT  
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: ipv4VXLANDecapsulationRes(399)"
			
            REVISION "201603081041Z"        -- Mar 08, 2016 at 10:41GMT  
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: trunkTableResExceedSlotThresHold(398)"

            REVISION "201603070952Z"        -- Mar 07, 2016 at 09:52GMT  
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: trunkTableResExceedSlotThresHold(398)"

            REVISION "201603031415Z"      --  Mar 03, 2016 at 14:15GMT 
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: ethTestResOverLoad(397)" 

            REVISION "201602261008Z"      --  Feb 26, 2016 at 10:08GMT 
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: l2ptResExceed90ThresHold(354),l2ptResOverLoad(355)" 

            REVISION "201602031459Z"      --  Feb 3, 2016 at 14:59GMT 
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: vxlanResExceed90ThresHold(395),vxlanResOverLoad(396)" 
			   
            REVISION "201602011700Z"      --  Jan 30, 2016 at 17:00GMT 
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: bgpFlowspecReResExceedThresHold(393),bgpFlowspecReResExceed90ThresHold(394)" 

            REVISION "201601282100Z"      --  Jan 30, 2016 at 16:00GMT 
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: glemNumExceedThresHold(391),localLinkEncapExceedThresHold(392)" 
			
             REVISION "201601282100Z"        --  Jan 28, 2016 at 21:00GMT 
             DESCRIPTION   
             "add MPLS_IC_TRAP_NON_SUPPORT_MPLS,MPLS_IC_TRAP_FWD_RESLACK and MPLS_IC_TRAP_FWD_RESLACKRESUME." 

             REVISION "201601262100Z"        --  Jan 26, 2016 at 21:00GMT 
             DESCRIPTION   
             "add hwVpFeatureName table and a trap alarm hwVpresExceed for Virtual Ports." 

             REVISION "201601251500Z"        --  Jan 25, 2016 at 15:00GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: pwSourceTunnelCheckResOverLoad(390)." 

            REVISION "201601041400Z"      --  Jan 4, 2016 at 14:00GMT 
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: spuExtNHPExhaust(381),spuExtNHPExhaustResume(382)" 

            REVISION "201512241320Z"      --  Dec 24, 2015 at 13:20GMT 
            DESCRIPTION  
            "add new alarm hwFpResourceThresholdExceed,hwFpResourceThresholdExceedClear,hwFpResourceTotalCountExceed,hwFpResourceTotalCountExceedClear" 


            REVISION "201512181058Z"      --  Dec 18, 2015 at 10:58GMT 
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: bwLargeBufferExhausted(387),userDefinedFLowAclExceed90ThresHold(388),dynamicLinkProtectionAclExceed90ThresHold(389)" 
            
            REVISION "201512081516Z"      --  Dec 8, 2015 at 15:16GMT 
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: mlidExceed75ThresHold(386)" 


            REVISION "201511021051Z"      --  Nov 02, 2015 at 10:51GMT 
            DESCRIPTION  
            "add reasonid for hwFwdResLackReasonId: pool0FlowWred(353), pool1FlowWred(354), pool0FlowMapping(355),  ...,  pool1SlotGqResExceed90ThresHold(380)" 

            REVISION "201510161355Z"      --  OCT 14, 2015 at 13:55GMT 
            DESCRIPTION   
            "add reasonid for hwFwdResLackReasonId: nhpExceedThresHold(348),nhpNumOverload(349),nstExceedThresHold(350),nstNumOverload(351),mlidExceedThresHold(352)" 



            REVISION "201510141123Z"      --  OCT 14, 2015 at 11:23GMT 
            DESCRIPTION   
            "add reasonid for hwFwdResLackReasonId: mplsSRTELabelStackResLack(347)" 

            REVISION "201510122100Z"      --  OCT 12, 2015 at 21:00GMT 
            DESCRIPTION   
            "add reasonid for hwFwdResLackReasonId: mplsSRTELabelStackResLack(345)" 

            REVISION "201510122100Z"      --  OCT 12, 2015 at 21:00GMT 
            DESCRIPTION   
            "add reasonid for hwFwdResLackReasonId: mplsSRTELabelStackResExceedTresHold(346)" 

            REVISION "201510121500Z"      --  OCT 12, 2015 at 15:00GMT 
            DESCRIPTION   
            "add reasonid for hwFwdResLackReasonId: mplsSRTELabelStackResLack(330)" 

            REVISION "201510121500Z"      --  OCT 12, 2015 at 15:00GMT 
            DESCRIPTION   
            "add reasonid for hwFwdResLackReasonId: mplsSRTELabelStackResExceedTresHold(331)" 
               	   
             REVISION "201510081750Z"        --  OCT 08, 2015 at 17:50GMT 
            DESCRIPTION   
            "add hwFwdResTable table and alarms(hwFwdResOverLimit,hwFwdResOverLimitResume,hwFwdResOverThresh,hwFwdResOverThreshResume)."

            REVISION "201509251750Z"        --  Sep 25, 2015 at 17:50GMT 
            DESCRIPTION   
            "add reasonid for hwFwdResLackReasonId: BoardAclTCAMNumExhaust(342)"
			
            REVISION "201509222010Z"        --  Sep 22, 2015 at 20:10GMT 
            DESCRIPTION   
            "add reasonid for hwFwdResLackReasonId: BoardAclTCAMNumExhaust(342)"

            REVISION "201509221920Z"        --  Sep 17, 2015 at 19:20GMT 
             DESCRIPTION   
             " add some reasonid for hwFwdResLackReasonId:inIPV4UCLTCAMExceedThresHold(334),outIPV4UCLTCAMExceedThresHold(335),inIPV6UCLTCAMExceedThresHold(336),outIPV6UCLTCAMExceedThresHold(337),inIPV4UCLTCAMNumOverload(338),outIPV4UCLTCAMNumOverload(339),inIPV6UCLTCAMNumOverload(340),outIPV6UCLTCAMNumOverload(341)" 

             REVISION "201509171920Z"        --  Sep 17, 2015 at 19:20GMT 
             DESCRIPTION   
             " add a new node hwBoardMplsNonSupport." 


             REVISION "201508041920Z"        --  Augu 04, 2015 at 19:20GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: pbbResExceed90ThresHold(328). pbbResOverLoad(329)." 
   
          REVISION "201506241723Z"        --  June 24, 2015 at 17:23GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId. ReasonId:trillMcOutIfNumOverload(327)." 

             REVISION "201506231432Z"        --  June 23, 2015 at 14:32GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId. ReasonId:ipv4GreDecapsulationRes(325) ipv6GreDecapsulationRes(326)." 

             REVISION "201506171620Z"        --  June 17, 2015 at 16:20GMT 
             DESCRIPTION   
             " add a reasonid for hwWholeFwdResLack. ReasonId: pbbBmacRes(324) ." 
           
             REVISION "201506091520Z"        --  June 09, 2015 at 15:20GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: remoteIntfRes(323) ." 

             REVISION "201505220950Z"        --  May 22, 2015 at 09:50GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: mfibv4NumExceedThresHold(321)  mfibv6NumExceedThresHold(322) ." 

             REVISION "201505080950Z"        --  May 08, 2015 at 09:50GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: fibv4NumExceedThresHold(318)." 

             REVISION "201505080950Z"        --  May 08, 2015 at 09:50GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: fibv6NumExceedThresHold(319)." 

             REVISION "201505080950Z"        --  May 08, 2015 at 09:50GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: ipv6NdExceedThresHold(320)." 

             REVISION "201505051420Z"        --  May 05, 2015 at 14:20GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: vplsResOverLoad(316)." 

             REVISION "201505051420Z"        --  May 05, 2015 at 14:20GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: evpnResOverLoad(317)." 

             REVISION "201504162200Z"        -- APR 16, 2015 at 22:00GMT 
             DESCRIPTION   
             " add a trap info for qos exceed." 

             REVISION "201504162150Z"        -- APR 16, 2015 at 21:50GMT 
             DESCRIPTION   
             " add a trap info for mc exceed." 

             REVISION "201504082150Z"        -- APR 08, 2015 at 21:50GMT 
             DESCRIPTION   
             " add a trap info for php exceed." 

             REVISION "201503312150Z"        --  Mar 31, 2015 at 21:50GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: l2tpv3ResExceed90ThresHold(302)." 

             REVISION "201503312150Z"        --  Mar 31, 2015 at 21:50GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: evpnResExceed90ThresHold(301)." 

             REVISION "201503312150Z"        --  Mar 31, 2015 at 21:50GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: vplsResExceed90ThresHold(300)." 

             REVISION "201503280950Z"        --  Mar 28, 2015 at 09:50GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: multioutlifResExceed90ThresHold(295)." 

             REVISION "201502071011Z"        --  Feb 7, 2015 at 10:11GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: erpsResExceed90ThresHold(285)." 
			 
             REVISION "201411181358Z"        --  Nov 18, 2014 at 13:58GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: ipsecAclResOverLoad(280)." 


             REVISION "201410281846Z"        --  Oct 28, 2014 at 18:46GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: semResOverLoad(279)." 
         
             REVISION "201410231047Z"        --  Oct 23, 2014 at 10:47GMT 
             DESCRIPTION   
             " add a reasonid for hwFwdResLackReasonId: vlanxlateResOverLoad(277)." 

            REVISION "201410231047Z"        --  Oct 23, 2014 at 10:47GMT  
            DESCRIPTION   
            " add a reasonid for hwFwdResLackReasonId: egressvlanxlateResOverLoad(278)."
 
            REVISION "201410171547Z"        --  Oct 17, 2014 at 15:47GMT
            DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId: forwardvpnResOverLoad(276)."
     
            REVISION "201410171547Z"        --  Oct 17, 2014 at 15:47GMT
            DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId: protectgroupResOverLoad(275)."

            REVISION "201409251058Z"        --  Sep 25, 2014 at 10:58GMT
            DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId: outTmSqResExceed90ThresHold(274)."
     
            REVISION "201409251058Z"        --  Sep 25, 2014 at 10:58GMT
            DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId: inSlotSqResExceed90ThresHold(273)."
     
            REVISION "201409251058Z"        --  Sep 25, 2014 at 10:58GMT
            DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId: outTmSqResExceed90ThresHold(272)."
     
            REVISION "201409251058Z"        --  Sep 25, 2014 at 10:58GMT
            DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId: inTmSqResExceed90ThresHold(271)."

            REVISION "201409031501Z"        --  Sep 03, 2014 at 15:01GMT
            DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId: tunnelDecapsulationRes(195),dynLoadbNhpRes(198)."

            REVISION "201408301156Z"        --  Augu  30, 2014 at 11:56GMT
            DESCRIPTION  
           " add a reasonid for hwFwdResLackReasonId: trunkDynAdjRes(176)."

            REVISION "201408221010Z"        --  Augu  22, 2014 at 10:10GMT
            DESCRIPTION  
           " adjust the alarm description ."


            REVISION "201408191001Z"        --  Augu  19, 2014 at 10:01GMT
            DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : tpSlmResExceedThresHold(261),tp1dmResExceedThresHold(262),tp2dmResExceedThresHold(263),tpDlmResExceedThresHold(264),tpSlmResOverLoad(265),tp1dmResOverLoad(266),tp2dmResOverLoad(267),tpDlmResOverLoad(268),tpoamCcResOverLoad(269),apsResOverLoad(270)."

            REVISION "201408061639Z"        --  Augu  06, 2014 at 16:39GMT
            DESCRIPTION  
           " modified for hwFwdProcFailForLCSOperationId,hwFwdLicenseName,hwFwdProcFailForLCS,hwFwdProcFailForLCSResume to keep same with code."


            REVISION "201407311922Z"        --  July  31, 2014 at 19:22GMT
            DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : pwHqosOverLoad(260)."

            
            REVISION "201407281947Z"        --  July  28, 2014 at 19:47GMT
            DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : chipinUserQueue(257) chipouUserQueue(258)."

            REVISION "201407281655Z"        --  July  28, 2014 at 16:55GMT
            DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : l2mcastResExceedThresHold(200),fibResExceedThresHold(201),arpResExceedThresHold(202),l3vpnResExceedThresHold(203),greResExceedThresHold(204),mplsResExceedThresHold(205),ldrResExceedThresHold(206),teResExceedThresHold(207),mplsvllResExceedThresHold(208),vllResExceedThresHold(209),vplsResExceedThresHold(210),hqosResExceedThresHold(211),.etc."



            REVISION "201407261714Z"        --  July  26, 2014 at 17:14GMT
            DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : apsRes(255) oamRes(256)."

            REVISION "201407261538Z"        --  July  26, 2014 at 15:38GMT
            DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : flexRes(177) mainsubifRes(178) dcnRes(179) statRes(180) eoamRes(181) qinqRes(189) l2TrafLmtStat(199)."

            REVISION "201407211554Z"        --  July  21, 2014 at 15:54GMT
            DESCRIPTION  
           " modified for hwFwdProcFailForLCSOperationId,hwFwdLicenseName,hwFwdProcFailForLCS,hwFwdProcFailForLCSResume to keep same with code."

            REVISION "201407162135Z"        --  July  16, 2014 at 21:35GMT
            DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : cpcarQueue(254)."

            REVISION "201407151935Z"        --  July  15, 2014 at 19:35GMT
            DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : popgoRe(253)."

            REVISION "201407110829Z"        --  July  11, 2014 at 08:29GMT
            DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : dp(241) inGQSshaper(242) outGQSshaper(243) inVI(244) outVI(245) inVISshaper(246) outVISshaper(247) inVITemp(248) outVITemp(249)   cqWred(250) incqServiceTemp(251) outcqServiceTemp(252)."

            REVISION "201407081729Z"        --  July  8, 2014 at 17:29GMT
            DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : hqosdp(238) hqosgqshaper(239) hqosvi(240) hqosvishaper(241) hqosvitemplate(242)."

            REVISION "201406090844Z"        --  June 9, 2014 at 08:44GMT
            DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : l2TrafLmt(167)  vlan(184)  bridgeDomain(185)  evcRes(190)."

            REVISION "201406051459Z"        --  June 5, 2014 at 14:59GMT
            DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : l2vpn(183)."

            REVISION "201405301450Z"        --  May 30, 2014 at 14:50GMT
            DESCRIPTION  
           " add some reasonid for hwFwdResLackReasonId : y1564Res(182),vrrpRes(186),twampRes(187),bfdRes(188), ipfpmRes(196), rfc2544Res(197)."

            REVISION "201405211000Z"        --  May 21, 2014 at 10:00GMT
            DESCRIPTION  
           "hwFwdEntryConflict,hwFwdEntryConflictResume,fwdFibCheck(175)."
 
            REVISION "201403081600Z"        --  March 08, 2014 at 16:00GMT
            DESCRIPTION  
            "Add hwFwdProcFailForLCSOperationId,hwFwdProcFailForLCS,hwFwdProcFailForLCSResume."  

            REVISION "201403051526Z"        --  March 05, 2014 at 15:26 GMT
            DESCRIPTION  
            "Add hwBoardIPv6ACLResLack  22."  
            
            REVISION "201401231657Z"        -- Jan 23, 2014 at 16:57 GMT 
            DESCRIPTION 
            " add reasonid     fwdInAc(168)   fwdOutAc(169)      fwdLem(170)      fwdL2Entry(171)        fwdMcMacfibv4(172)   fwdSnoop(173)   fwdArp(174) " 
            
            REVISION "201401211140Z"        -- Jan 21, 2014 at 11:40 GMT
            DESCRIPTION 
            " modified  hwBoardResWarningThresholdExceed,hwBoardResWarningThresholdExceedResume." 
                  
            REVISION "201401142146Z"        -- Jan 14, 2014 at 21:46 GMT
            DESCRIPTION 
            "Add  hwBoardResThresholdExceed,hwBoardResThresholdExceedResume,hwBoardResWarningThresholdExceed,hwBoardResWarningThresholdExceedResume." 
                           
           REVISION "201401061952Z"        -- Jan 06, 2014 at 19:52 GMT  
           DESCRIPTION  
           "Add QPPB alarm type."         
       
           REVISION "201312121728Z" -- Sep 12, 2013 at 17:28 GMT
           DESCRIPTION
            "Add Beavior alarm type."

            REVISION "201311131028Z"        -- Nov 13, 2013 at 10:28 GMT
            DESCRIPTION
            "Add hwFwdResLacTrap 17 "
 
           REVISION "201305141121Z" -- May 14, 2013 at 11:21 GMT
           DESCRIPTION
            "Add alarm type."
          
           REVISION "201305141121Z" -- May 14, 2013 at 11:21 GMT
           DESCRIPTION
            "Add alarm type."

            REVISION "201006041043Z"        -- June 04, 2010 at 10:43 GMT
            DESCRIPTION
                "ver 1.0"  
            ::= { hwDatacomm 227 }       
    
    
--
-- Node definitions
--
    
        -- 1.3.6.1.4.1.2011.5.25.227.1
        hwFwdResTrapObject OBJECT IDENTIFIER ::= { hwFwdResTrapMIB 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.1.1
        hwEntPhysicalindex OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify               
            STATUS current
            DESCRIPTION
                "The index for this entry."
            ::= { hwFwdResTrapObject 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.1.2
        hwFwdResLackSlotStr OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The information for the slot."
            ::= { hwFwdResTrapObject 2 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.1.3
        hwFwdResLackReasonId OBJECT-TYPE
            SYNTAX INTEGER
                {
                mplsLinkOverLoad(1),
                fibv4NumOverLoad(2),
                fibv6NumOverLoad(3),
                arpNumOverLoad(4),
                ipv6NdNumOverLoad(5),
                statNumOverLoad(6),
                qosNumOverLoad(7),
                l2vpnLinkOverLoad(8),
                mcintNumOverLoad(9),
                bfdaclNumOverLoad(10),
                mcfibv4NumOverLoad(11),
                mcfibv6NumOverLoad(12),
                fwdToken(13),
                fvrfIndex(14),
                ndIndex(15),
                tunnelIndex(16),
                bfdIndex(17),
                vplsLearnId(18),
                vsiIndex(19),
                nsIndex(20),
                ringIndex(21),
                mcRepSerNumOverload(22),
                mcOutIfNumOverload(23),
                mcTmgidOverLoad(24),                    
                mcMlidOverLoad(25),                       
                trillNhpIndex(26),                        
                hostTablePrefixTable(27),                  
                routingTablePrefixTable(28),               
                ecmpNextHopTable(29),             
                layer3InterfaceTable(30),                  
                nextHopTable(31),                 
                tunnelDecapsulationTable(32),              
                qvctNumOverload(33),                       
                bfdGlobalIndex(34),
                ipv4FullRull(35), 
                ipv4MaskRull(36), 
                ipv6FullRull(37),
                ipv6MaskRull(38),
                dpiRull(39),
                comRull(40),
                tcpFlagRull(41),
                ccSendNum(42),
                ccRecvNum(43),
                y1731SlmNum(44),
                y17311dmNum(45),
                y17312dmNum(46),
                ipv6RoutingTablePrefixTable(47),
                mcv4StatId(48),
                mcv6StatId(49),
                nhpNum(50),
                nscvmNum(51),
                y1731dlmNum(52), 
                bgpExtNum(53),
                bgp6ExtNum(54),
                linkEncap(55), 
                tunnelEncap(56), 
                largeExactlyMatchTable(57), 
                logicalInterface(58), 
                macMulticastIndex(59), 
                virtualPort(60), 
                aclEntry(61), 
                aclGroup(62), 
                meter(63), 
                counter(64), 
                aclEntryOutbound(65), 
                aclGroupOutbound(66), 
                meterOutbound(67), 
                counterOutbound(68), 
                multicastIndex(69), 
                ipfpmAclResOverLoad(70), 
                dhcpsnpBindTableResOverLoad(71), 
                l3aclFailed(72),
                fibArpFwdModeNumOverLoad(73),
                l2mcindex(74),
                ipmcindex(75),
                arpNumLack(76),
                ipv6NdNumLack(77),
                statNumLack(78),
                qosNumLack(79),
                l2vpnLinkLack(80),
                mcintNumLack(81),
                bfdaclNumLack(82),
                mcfibv4NumLack(83),
                mcfibv6NumLack(84),
                nhpNumLack(85),
                nscvmNumLack(86),
                mplsLinkLack(87),
                fibv4NumLack(88),
                fibv6NumLack(89),
                bgpExtNumLack(90),
                bgp6ExtNumLack(91),
                l2UserEntryOverload(92), 
                fwdGlobal1Token(93),
                fwdBoardToken(94),
                fwdGlobal2Token(95),
                fwdGlobal3Token(96),
                fwdGlobal4Token(97),
                fwdGlobal1ThresHoldToken(98),
                fwdBoardThresHoldToken(99), 
                fwdGlobal2ThresHoldToken(100),
                fwdGlobal3ThresHoldToken(101),
                fwdGlobal4ThresHoldToken(102),
                atIndex(103),
                flexQvctNum(104),
                inFlowWred(105),
                outFlowWred(106),
                inFlowMapping(107),
                outFlowMapping(108),
                inFlowQueueWfq(109),
                outFlowQueueWfq(110),
                inFlowQueueCbs(111),
                outFlowQueueCbs(112),
                inFlowQueuePbs(113),
                outFlowQueuePbs(114),
                inUserQueue(115),
                outUserQueue(116),
                inUserQueueTemp(117),
                outUserQueueTemp(118),
                inServiceTemp(119),
                outServiceTemp(120),
                inGQ(121),
                outGQ(122),
                inGQTemp(123),
                outGQTemp(124),
                inIfCar(125),
                outIfCar(126),
                inCarRemark(127),
                outCarRemark(128),
                gid(129),
                inAclCar(130),
                outAclCar(131),
                aclRe(132),
                aclNhp(133),
                inIPv4Acl(134),
                inIPv6Acl(135),
                outIPv4Acl(136),
                outIPv6Acl(137),
                inQppbCar(138),
                outQppbCar(139),
                inMirror(140),
                outMirror(141),
                inMirrorCapture(142),
                outMirrorCapture(143),
                inSuppressCar(144),
                outSuppressCar(145),
                inMirrorCar(146),
                outMirrorCar(147),
                aclNst(148),
                inProfSuppCar(149),
                outProfSuppCar(150),
                inProfSuppCarStat(151),
                outProfSuppCarStat(152),
                inProfSingleCar(153),
                outProfSingleCar(154),
                inProfSingleCarStat(155),
                outProfSingleCarStat(156),
                inAclStat(157),
                outAclStat(158),
                aclCarStat(159),
                inIfCarStat(160),
                outIfCarStat(161),
                inL2Acl(162),
                outL2Acl(163),
                l2TrafLmt(167),
                inBehaviorSuppCar(191),
                outBehaviorSuppCar(192),
                qppbAcl(193),
                qppbGid(194) ,
                fwdInAc(168),
                fwdOutAc(169),
                fwdLem(170),
                fwdL2Entry(171),
                fwdMcMacfibv4(172),
                fwdSnoop(173),
                fwdArp(174),
                fwdFibCheck(175),
                flexRes(177),
                mainsubifRes(178),
                dcnRes(179),
                statRes(180),
                eoamRes(181),
                y1564Res(182),
                l2vpn(183),
                vlan(184),
                bridgeDomain(185),
                vrrpRes(186),
                twampRes(187),
                bfdRes(188),
                qinqRes(189),
                evcRes(190),
                tunnelDecapsulationRes(195),
                ipfpmRes(196),
                rfc2544Res(197),
                dynLoadbNhpRes(198),
                l2TrafLmtStat(199),
                trunkDynAdjRes(176),
                l2mcastResExceedThresHold(200),
                fibResExceedThresHold(201),
                arpResExceedThresHold(202),
                l3vpnResExceedThresHold(203),
                greResExceedThresHold(204),
                mplsResExceedThresHold(205),
                ldrResExceedThresHold(206),
                teResExceedThresHold(207),
                mplsvllResExceedThresHold(208),
                vllResExceedThresHold(209),
                vplsResExceedThresHold(210),
                hqosResExceedThresHold(211),
                aclResExceedThresHold(212),
                carResExceedThresHold(213),
                diffservResExceedThresHold(214),
                statResExceedThresHold(215),
                resmResExceedThresHold(216),
                fesdrveResExceedThresHold(217),
                atmResExceedThresHold(218),
                cesResExceedThresHold(219),
                mlpppResExceedThresHold(220),
                devmResExceedThresHold(221),
                oamResExceedThresHold(222),
                oam1agResExceedThresHold(223),
                y1731ResExceedThresHold(224),
                oam3ahResExceedThresHold(225),
                nqaResExceedThresHold(226),
                rfc2544ResExceedThresHold(227),
                sdResExceedThresHold(228),
                tpoamResExceedThresHold(229),
                tpapsResExceedThresHold(230),
                ipfpmResExceedThresHold(231),
                ethtestResExceedThresHold(232),
                bfdResExceedThresHold(233),
                oammaxResExceedThresHold(234),
                imsResExceedThresHold(235),
                tcamResExceedThresHold(236),
                dcnResExceedThresHold(237),
                defendResExceedThresHold(238),
                l3mcastResExceedThresHold(239),
                dhcpsnpResExceedThresHold(240),
                dp(241),
                inGQSshaper(242),
                outGQSshaper(243),
                inVI(244),
                outVI(245),
                inVISshaper(246),
                outVISshaper(247),
                inVITemp(248),
                outVITemp(249),
                cqWred(250),
                incqServiceTemp(251),
                outcqServiceTemp(252),
                popgoRe(253),
                cpcarQueue(254),
                apsRes(255),
                oamRes(256),
                chipinUserQueue(257),
                chipouUserQueue(258),
                pwHqosOverLoad(260),
                 tpSlmResExceedThresHold(261),
                tp1dmResExceedThresHold(262),
                tp2dmResExceedThresHold(263),
                tpDlmResExceedThresHold(264),
                tpSlmResOverLoad(265),
                tp1dmResOverLoad(266),
                tp2dmResOverLoad(267),
                tpDlmResOverLoad(268),
                tpoamCcResOverLoad(269),
                apsResOverLoad(270), 
                inTmSqResExceed90ThresHold(271),
                outTmSqResExceed90ThresHold(272),      
                inSlotSqResExceed90ThresHold(273),
                outSlotSqResExceed90ThresHold(274),
                protectgroupResOverLoad(275),      
                forwardvpnResOverLoad(276),   
                vlanxlateResOverLoad(277),
                egressvlanxlateResOverLoad(278),  
                semResOverLoad(279),
                ipsecAclResOverLoad(280),
                erpsResExceed90ThresHold(285),
                multioutlifResExceed90ThresHold(295),
                vplsResExceed90ThresHold(300),
                evpnResExceed90ThresHold(301),
                l2tpv3ResExceed90ThresHold(302),
                multicastGroupExceed95ThresHold(303),
                l2MfibNumExceed95ThresHold(304),
                inIFCarExceedThresHold(305),
               outIFCarExceedThresHold(306),
               gidExceedThresHold(307),
               inRuleStatExceedThresHold(308),
               outRuleStatExceedThresHold(309),
               bhvInCarExceedThresHold(310),
               bhvOutCarExceedThresHold(311),
               inIPV4TCAMExceedThresHold(312),
               outIPV4TCAMExceedThresHold(313),
               inIPV6TCAMExceedThresHold(314),
               outIPV6TCAMExceedThresHold(315),
               vplsResOverLoad(316),
               evpnResOverLoad(317),
               fibv4NumExceedThresHold(318),
               fibv6NumExceedThresHold(319),
               ipv6NdExceedThresHold(320),
               mcfibv4NumExceedThresHold(321),
               mcfibv6NumExceedThresHold(322),
               remoteIntfRes(323),
               pbbBmacRes(324),
               ipv4GreDecapsulationRes(325),
               ipv6GreDecapsulationRes(326),
               trillMcOutIfNumOverload(327),
               pbbResExceed90ThresHold(328),
               pbbResOverLoad(329),
               sourceVpTable(330),
               mplsEntryTable(331),
               mplsVcAndSwapLabelTable(332),
               ipTunnelMplsTable(333),
	       inIPV4UCLTCAMExceedThresHold(334),
               outIPV4UCLTCAMExceedThresHold(335),
               inIPV6UCLTCAMExceedThresHold(336),
               outIPV6UCLTCAMExceedThresHold(337),
	       inIPV4UCLTCAMNumOverload(338),
               outIPV4UCLTCAMNumOverload(339),
               inIPV6UCLTCAMNumOverload(340),
               outIPV6UCLTCAMNumOverload(341),
               boardAclTCAMNumExhaust(342),
			   inGqResExceed90ThresHold(343),
			   outGqResExceed90ThresHold(344),
               mplsSRTELabelStackResLack(345),
               mplsSRTELabelStackResExceedThresHold(346),
               mplsLdpStatResExceedThresHold(347),
               nhpExceedThresHold(348),
               nhpNumOverload(349),
               nstExceedThresHold(350),
               nstNumOverload(351),
               mlidExceedThresHold(352),      
               l2ptResExceed90ThresHold(354),
               l2ptResOverLoad(355),
               pool1FlowMapping(356),                   
               pool0FlowQueueWfq(357),                   
               pool1FlowQueueWfq(358),                  
               pool0FlowQueueCbs(359),                   
               pool1FlowQueueCbs(360),                  
               pool0FlowQueuePbs(361),                   
               pool1FlowQueuePbs(362),                  
               pool0UserQueue(363),                      
               pool1UserQueue(364),                     
               pool0UserQueueTemp(365),                  
               pool1UserQueueTemp(366),                 
               pool0ServiceTemp(367),                    
               pool1ServiceTemp(368),                   
               pool0GQ(369),                             
               pool1GQ(370),                            
               pool0GQTemp(371),                         
               pool1GQTemp(372),                        
               chippool0UserQueue(373),                  
               chippool1UserQueue(374),                  
               pool0TmSqResExceed90ThresHold(375),       
               pool1TmSqResExceed90ThresHold(376),      
               pool0SlotSqResExceed90ThresHold(377),     
               pool1SlotSqResExceed90ThresHold(378),
               pool0SlotGqResExceed90ThresHold(379),     
               pool1SlotGqResExceed90ThresHold(380),
               spuExtNHPExhaust(381),
               spuExtNHPExhaustResume(382),
               pool0FlowWred(383),                       
               pool1FlowWred(384),                      
               pool0FlowMapping(385),
               mlidExceed75ThresHold(386),
               bwLargeBufferExhausted(387),
               userDefinedFLowAclExceed90ThresHold(388),
               dynamicLinkProtectionAclExceed90ThresHold(389),
               pwSourceTunnelCheckResOverLoad(390),
			   glemNumExceedThresHold(391),
			   localLinkEncapExceedThresHold(392),
               bgpFlowspecReResExceedThresHold(393),
               bgpFlowspecReResExceed90ThresHold(394),
			   vxlanResExceed90ThresHold(395),
			   vxlanResOverLoad(396),
               ethTestResOverLoad(397),
               trunkTableResExceedSlotThresHold(398),
			   ipv4VXLANDecapsulationRes(399),
               cirUserQueue(402), 
               eirUserQueue(403), 
               shapingFlowqueue (404), 
               shareShapingFlowqueue (405),
               mcmofrrResourceNumOverLoad (406),
               mcmofrrResourceExceedThresHold (407),
               tunnelnexthop (408),
               ipv4VXLANVniPeerRes(410),
               mcMfibChipEntryHashConflict(411),
               vsmIPV6AclTCAMNumFull(418),
               vsmIPV6AclTCAMNumExhaust(419),
               tunnelsourceipindex(420),
               vllHardPipeResourceOverLoad(497),
               bfdGidNumOverLoad(498),
               vplsPwNhpResourceOverload(499),
               e2e1588Res(500),
               pwifResExceed90ThresHold(501),
               insegVrfOverLoad(502),
               dynldbalStatOverLoad(503),
               communityeOverLoad(504),
               ipv4TunnelIndexOverLoad(505),
               smaAsIndexOverLoad(506),
               smaFibv6OverLoad(507),
               pwifResOverLoad(548),
               overlayNhpResOverLoad(549),
               vplspwHqosOverLoad(550),
               l2ptCarResExceed90ThresHold(551),
               l2ptCarResOverLoad(552),
               vplsPwSuppStatOverLoad(553), 
               vplsPwSuppStatExceed90ThresHold(554),
               l2tpv3TunnelResOverLoad(555),
               vlanEncapResOverload(556),
               l2tpv3TnlResOverLoad(565),
               outVIResExceed90ThresHold(569),
               ipv6LongerMaskResOverLoad(570),
               atmIpoaArpResOverLoad(571),
               apsOutMirrorResOverLoad(572),
               lsMacResOverLoad(573),
               lsEgrL3IntResOverLoad(574),
               lsStationTcamResOverLoad(575),
               lsL2UserEntryResOverLoad(576),
               macAccountingResOverLoad(577),
               vfiTable(578),
               ecmpreswarning(579),
               nhpreswarning(580),
               icibppTable(581),
               icibTable(582),
               isemTable(583),
               ecibTable(587),
               ecibextTable(588),
               fe0UserNumExceed90Threshold(595),
               fe0UserNumExceed100Threshold(596),
               fe1UserNumExceed90Threshold(597),
               fe1UserNumExceed100Threshold(598),
               l2mcTmgidOverThresHold(605),
               ipv4O6TnlDecapTblResOverLoad(608),
               ipv4O6TnlIpv6AddrTblResOverLoad(609),
               fibv6NumWarning(624), 
               arpFastReplyInterface(630),
               level1FECTable(633),
               level2FECTable(634),
               level3FECTable(636),
               fibResOverLoad(656),
               ipv6IgnoreOverLoad(657),
               vxlanv6TrunkResOverLoad(658),
               dsvpnNhrpsulationRes(664),
               dsvpnResOverLoad(665),
               dsvpnResExceedThresHold(666),
               vpnVclabelResExceedThresHold(613),
               mcHotstanbyResLack(700),
               l3mcV4TmgidResLack(701),
               l3mcV6TmgidResLack(702),
               mcHotstanbyResOverLoad(703),
               l3mcV4TmgidResOverLoad(704),
               l3mcV6TmgidResOverLoad(705),
               l3mcV4MreStatResOverLoad(707),
               l3mcV6MreStatResOverLoad(708),
               l3mcV4MreExtResOverLoad(709),
               l3mcV6MreExtResOverLoad(710),
               l3mcV4MreStatResExceedThresHold(711),
               l3mcV6MreStatResExceedThresHold(712),
               l3mcV4MreExtResExceedThresHold(713),
               l3mcV6MreExtResExceedThresHold(714),
               hqosVirtualSQOverLoad(715),
               hqosVirtualGQOverLoad(716),
               hqosVirtualVIOverLoad(717),
               hqosVirtualSQExceedThresHold(718),
               hqosVirtualGQExceedThresHold(719),
               hqosVirtualVIExceedThresHold(720),
               l3ucVpnSIdIpV6AddrOverLoad(721),
               l3ucNhrpNetworkIdIndexOverLoad(722),
               l3ucVpnSIdIpV6AddrExceedThresHold(723),
               l3ucNhrpNetworkIdIndexExceedThresHold(724),
               secSessioncarResExceedOverload(725),
               secSessioncarResExceed90Overload(726),
               secSessioncarStatExceedOverload(727),
               secSessioncarStatExceed90Overload(728),
               l3mcV4MreCloneStatResOverLoad(731),
               l3mcV4MreCloneStatResExceedThresHold(732),
               l3mcLeafNumberExceedThresHold(736),
               l3mcLeafNumberOverLoad(737),
               secV6sessioncarResExceedOverload(738),
               secV6sessioncarResExceed90Overload(739),
               secV6sessioncarStatExceedOverload(740),
               secV6sessioncarStatExceed90Overload(741),
               tunnel6EncapsulationTable(742),
               tunnelEncapsulationTable(743),
               reTable(744),
               aibTable(745),
               nstTable(746),
               vrrpTable(747),
               ipv6amTable(748),
               l2mcTable(749),
               ipmcTable(750),
               ipmcVlanTable(751),
               mlibTable(752),
               elbTable(753),
               fdbTable(754),
               vidxTable(755),
               tcamTable(756),
               lttTable(757),
               mllTable(758),
               hqosSessionCaridOverload(759),
               hqosFamilyCaridOverload(760),
               hqosVcpeL2CaridOverload(761),
               hqosVcpeL3CaridOverload(762),
               hqosSessionCarStatidOverload(763),
               hqosFamilyCarStatidOverload(764),
               hqosVcpeL2CarStatidOverload(765),
               hqosVcpeL3CarStatidOverload(766),
               ipv6DefipTable(767) ,
               mcBierVpnOverLoad(768),
               mcBierTunnelOverLoad(769),
               mcBierTmgidOverLoad(770),
               mcBierVpnExceedThresHold(771),
               mcBierTmgidExceedThresHold(772),
               mcBierBitMaskOverLoad(773),
               mcBierBitMaskExceedThresHold(774),
               mcEgressStatOverLoad(775),
               mcEgressStatExceedThresHold(776),
               vxlanvpTable(777),
               inProfSingleCarPre(778),
               outProfSingleCarPre(779),
               inProfSingleCarStatPre(780),
               outProfSingleCarStatPre(781),
               tlmtActCar100ms(800),
               tlmtActCar100msPre(801),
               tlmtActCar1s(802),
               tlmtActCar1Pre(803),
               tlmtActCar30s(804),
               tlmtActCar30Pre(805),
               tlmtPolicy100ms(806),
               tlmtPolicy100msPre(807),
               tlmtPolicy1s(808),
               tlmtPolicy1Pre(809),
               tlmtPolicy30s(810),
               tlmtPolicy30Pre(811),
               srpolicyStatExceedThresHold(812),
               srpolicyStatOverLoad(813),
               l2TrunkLbTmgidResOverLoad(814),
               vlanL2mcRpTmgidResOverLoad(815),
               vsiL2mcRpTmgidResOverLoad(816),
               bdL2mcRpTmgidResOverLoad(817),
               vsiL2mcBakPwTmgidResOverLoad(818),
               pimFrrTmgidResOverLoad(819),
               vlanL2mcv6RpTmgidResOverLoad(820),
               vsiL2mcv6RpTmgidResOverLoad(821),
               l2mcStkMapTmgidResOverLoad(822),
               brasMcHwTmgidResOverLoad(823),
               mcNatTmgidResOverLoad(824),
               ucDsvpnGroupOverLoad(825),
               bdTmgidResOverLoad(826),
               hwmcTmgidResOverLoad(827),
               vlanTmgidResOverLoad(828),
               l2vpnTmgidResOverLoad(829),
               l2vpnApsTmgidResOverLoad(830),
               localArpv6OverLoad(831),
               localArpv6ExceedThreshold(832),
               l3intflistTable(833),
               mcpmskTable(834),
               localSidOverLoad(653),
               localSidExceedThreshold(835),
               remoteSidOverLoad(836),
               remoteSidExceedThreshold(837),
               teleScan30sOverLoad(838),
               teleScan30sExceedThreshold(839),
               teleScan1sOverLoad(840),
               teleScan1sExceedThreshold(841),
               srv6policyRdrREOverLoad(842),
               srv6policyRdrREExceedThreshold(843),
               srv6ListOverLoad(844),
               srv6ListExceedThreshold(845),
               srv6PolicyStatResOverLoad(846),
               srv6PolicyStatResExceedThreshold(847),
               vxlanv6DecapOverLoad(848),
               vxlanv6DecapExceedThreshold(849),
               srv6ServChainL3ReOverLoad(850),
               srv6ServChainL3ReExceedThreshold(851),
               srv6ServChainL2ReOverLoad(852),
               srv6ServChainL2ReExceedThreshold(853),
               ipv4vpnTable(854),
               ipv6vpnTable(855),
               arpResOverLoad(856),
               ndResOverLoad(857),
               fibv4NumPercentOverLoad(858),
               vplsMcTable(859),
               inSlot8QueueSqResExceed90ThresHold(860),
               inSlot8QueueEnhanceSqResExceed90ThresHold(861),
               inTM8QueueSqResExceed90ThresHold(862),
               inTM8QueueEhanceSqResExceed90ThresHold(863),
               outSlot4QueueSqResExceed90ThresHold(864),
               outSlot8QueueSqResExceed90ThresHold(865),
               outSlot8QueueEnhanceSqResExceed90ThresHold(866),
               outTM4QueueSqResExceed90ThresHold(867),
               outTM8QueueSqResExceed90ThresHold(868),
               outTM8QueueEnhanceSqResExceed90ThresHold(869),
               in8QueueSqResExhausted(870),
               in8QueueEnhanceSqResExhausted(871),
               out4QueueSqResExhausted(872),
               out8QueueSqResExhausted(873),
               out8QueueEnhanceSqResExhausted(874),
               mcidResWarning(875),
               vsiResWarning(876),
               vpResWarning(877),
               macResWarning(878),               			  		   
               inTM8QueueSqResExhausted(907),
               inTM8QueueEnhanceSqResExhausted(908),
               outTM4QueueSqResExhausted(909),
               outTM8QueueSqResExhausted(910),
               outTM8QueueEnhanceSqResExhausted(911),
               cpIPv4AndIPv6AclNum90Overload(920),
               cpIPv4AndIPv6AclNumOverload(921),
               vxlanMcTable(922),
               srv6SliceOportinfoOverLoad(923),
               srv6SliceOportinfoExceedThreshold(924),
               inLabelMaplResOverLoad(925),
               labelTermResOverLoad(926),
               bierv6TmgidOverLoad(927),
               bierv6TmgidExceedThresHold(928),
               bierv6VpnOverLoad(929),
               bierv6Ilmv6OverLoad(930),
               bierv6VpnExceedThresHold(931),
               bierv6Ilmv6ExceedThresHold(932),
               sharedGqResExceed90Threshold(933),
               segmentlistSliceMapOverLoad(934),
               segmentlistSliceMapExceedThresHold(935),
               ifCarAclOverLoad(941),
               pkteventCacheExceedThreshold(942),
               latencyeventCacheExceedThreshold(943),
               anyflowOriCacheExceedThreshold(944),
               anyflowAggreCacheExceedThreshold(945),
               anyflowFLCCacheExceedThreshold(946),
               taCacheExceedThreshold(947),
               bierv6StatCntResOverload(949),
               bierv6StatNseResOverload(950),
               srv6ColorSliceMapOverLoad(951),
               srv6ColorSliceMapExceedThreshold(952),
               userdefinedcpaclNumOverLoad(953),
               userdefinedcpaclNum90PercentOverLoad(954),
               dlpcpaclNumOverLoad(955),
               dlpcpaclNum90PercentOverLoad(956),
               microisoAclNumOverLoad(957),
               microisoAclNum90PercentOverLoad(958),
               microisoLpmNumOverLoad(959),
               microisoLpmNum90PercentOverLoad(960),
               microisoCarNumOverLoad(961),
               microisoCarNum90PercentOverLoad(962),
               microisoCarStatNumOverLoad(963),
               microisoCarStatNum90PercentOverLoad(964),
               cpaclNumOverLoad(965),
               cpaclNum90PercentOverLoad(966),
               fwdLagResourceOverLoad(967),
               bgoflowRefluenceOverLoad(968),
               bgoflowIpv6Int90PercentOverLoad(969),
               bgoflowIpv6IntOverLoad(970),
               ifitNativeIpFlowRes(971),
               fibHardwareNumOverLoad(973),
               fib6HardwareNumOverLoad(974),
               fibSoftwareNumOverLoad(975),
               fib6SoftwareNumOverLoad(976), 
               fibSoftwareExceedThreshold(977), 
               fib6SoftwareNumExceedThreshold(978),
               serviceCarResOverload(979),
               srv6TeFlowGroupClassMapOverLoad(980),
	       srv6TeFlowGroupClassMapExceedThreshold(981),
               inboundInterfaceCar95PercentOverLoad(982),
               outboundInterfaceCar95PercentOverLoad(983),
               srv6Dip90PerNumOverload(984),
               srv6Dip100PerNumOverload(985),
               elineSidTblExt90PerNumOverload(986),
               elineSidTblExt100PerNumOverload(987),
               ifitDynFlowRes(988),
               vxlanVpiOverThreshold(989),
               vxlanVpOverThreshold(990),
               vxlanTunnelOverThreshold(991),
               oam1agvlanbcResourceOverLoad(992),
               tunnelV6DecapsulationRes(993),
	       apn6TrafficSteeringMapOverLoad(994),
       	       apn6InterfaceMapOverLoad(995),
	       apn6VPNPeerMapOverLoad(996),
 	       apn6TrafficIsolationMapOverLoad(997),
	       apn6IsolationStatisticsOverLoad(998),
	       apn6TrafficSteeringMapExceedThreshold(999),
	       apn6InterfaceMapExceedThreshold(1000),
	       apn6VPNPeerMapExceedThreshold(1001),
               apn6TrafficIsolationMapExceedThreshold(1002),
	       apn6IsolationStatisticsExceedThreshold(1003),
               dlbResOverLoad(1004),
               l2tpLacSessionExceed90Threshold(1005),
               l2tpLacSessionExceed100Threshold(1006),
               l2tpLnsSessionExceed90Threshold(1007),
               l2tpLnsSessionExceed100Threshold(1008),
               l2tpLnsTunnelBoardSessionExceed90Threshold(1009),
               l2tpLnsTunnelBoardSessionExceed100Threshold(1010),
               l2tpLacTunnelExceed90Threshold(1011),
               l2tpLacTunnelExceed100Threshold(1012),
               l2tpLnsTunnelExceed90Threshold(1013),
               l2tpLnsTunnelExceed100Threshold(1014),
               ifitAclRes(1015),
               ifitInstanceRes(1016),
               peerGroupResWarning(1017),
               hqosBrasSlotSessionCarOverload(1018),
              hqosBrasNpSessionCarOverload(1019),
              hqosBrasSlotFamilyCarOverload(1020),
              hqosBrasNpFamilyCarOverload(1021),
              hqosBrasSessionCarStatOverload(1022),
              hqosBrasFamilyCarStatOverload(1023),
              nativeIfitFlowIdRes(1024),
              qosDipShapingOverload(1025),
              qosDipShapingStatisticsOverload(1026),
              qosDipShapingExceed90Threshold(1027),
              qosDipShapingStatisticsExceed90Threshold(1028),
              hqosPortWredIdResLac(1029),
              bgpflowMReResExceedThresHold(1030),
              bgpflowMReResExceed90ThresHold(1031),
              bgpflowNstResExceedThresHold(1032),
              bgpflowNstResExceed90ThresHold(1033),
              bgpflowNhpResExceedThresHold(1034),
              bgpflowNhpResExceed90ThresHold(1035),
               fe2UserNumExceed90Threshold(1036),
               fe2UserNumExceed100Threshold(1037),
               fe3UserNumExceed90Threshold(1038),
               fe3UserNumExceed100Threshold(1039),
               cgnAclTcamNumOfNpExceedThreshold(1040), 
               cgnAclTcamNumOfNpExhausted(1041),
              eedbResExceedThresHold(1042),
              sliceResWarning(1043),
              glemResWarning(1044),
              localFec1ResWarning(1045),
              localFec2ResWarning(1046),
              localFec3ResWarning(1047),
              localFecEcmpResWarning(1048),
              hwNdLinkEncapResExceed(1049),
              bgpflowIfBaseV6EmNstExceedThreshold(1052),
              bgpflowIfBaseV6EmNstExceed90Threshold(1053),
              inIfCarAclExceedThreshold(1054),
              inIfCarAclExceed95Threshold(1055),
              l2upstreamAclGroupExceedThreshold(1056),
              l2downstreamAclGroupExceedThreshold(1057),
              ipv4upstreamAclGroupExceedThreshold(1058),
              ipv4downstreamAclGroupExceedThreshold(1059),
              ipv6upstreamAclGroupExceedThreshold(1060),
              ipv6downstreamAclGroupExceedThreshold(1061),
              mplsUpstreamAclGroupExceedThreshold(1062),
              mplsDownstreamAclGroupExceedThreshold(1063),
              ipv4TwampAclGroupExceedThreshold(1064),
              ipv6TwampAclGroupExceedThreshold(1065),
              hwArpLinkEncapResExceed(1070),
              hwInSqExceedPreCfgNum(1071),
              hwOutSqExceedPreCfgNum(1072),
			  bgpepeInStatisticsOverLoad(1073),
			  bgpepeOutStatisticsOverLoad(1074),
			  bgpepeInStatisticsExceedThreshold(1075),
			  bgpepeOutStatisticsExceedThreshold(1076),
			  bgplspInStatisticsOverLoad(1077),
			  bgplspOutStatisticsOverLoad(1078),
			  bgplspInStatisticsExceedThreshold(1079),
			  bgplspOutStatisticsExceedThreshold(1080),
              ipv6MicrocarFlowTableExceedThreshold(1081),
              bgpFlowSpecCommunityExceedThreshold(1082),
              vlanDomainResWarning(1083),
              veResWarning(1084),
              lacpResWarning(1085),
              aibsub1ResWarning(1086),
              aibsub2ResWarning(1087),
              aibsub3ResWarning(1088),
              ecmp2ResWarning(1089),
              mtuResWarning(1090),
              gltpResWarning(1091),
              lstResWarning(1092),
               tlmtActCar300s(1093),
               tlmtActCar300Pre(1094),
               tlmtPolicy300s(1095),
               tlmtPolicy300Pre(1096),
               mplsIlmResWarning(1097),
               rev4NumOverload(1098),
               rev6NumOverload(1099),
               rev4NumExceedThreshold(1100),
               rev6NumExceedThreshold(1101),
               intfCarAclExceedThreshold(1102),
               intfCarAclExceed95Threshold(1103),
               upstreamL2AclGroupExceedThreshold(1104),
               downstreamL2AclGroupExceedThreshold(1105),
               upstreamIpv4AclGroupExceedThreshold(1106),
               downstreamIpv4AclGroupExceedThreshold(1107),
               upstreamIpv6AclGroupExceedThreshold(1108),
               downstreamIpv6AclGroupExceedThreshold(1109),
               upstreamMplsAclGroupExceedThreshold(1110),
               downstreamMplsAclGroupExceedThreshold(1111),
               twampIpv4AclGroupExceedThreshold(1112),
               twampIpv6AclGroupExceedThreshold(1113),
               mcPimBdrStatusResExceedThreshold(1114),
               mcPimBdrStatusResOverLoad(1115),
               y1731SslmNumOverLoad(1116),
               y1731SslmNumExceedThreshold(1117),
               nqaL2RcvEAclGroupExceedThreshold(1118),
               nqaL3RcvEAclGroupExceedThreshold(1119),
               nqaL2RcvIAclGroupExceedThreshold(1120),
               bgpLspNumExceedThreshold(1121),
               ipv4EnhanceCpAclGroupExceedThreshold(1122),
               ipv6EnhanceCpAclGroupExceedThreshold(1123),
               twampInJectAclGroupExceedThreshold(1124),
               mcfibv4NumExceedForwardEngine(1222),
               camResWaring(1223),
               camcountidResWaring(1224),
               netrouteResWaring(1225),
               inlifMplsNumOverload(1226),
               inlifSRv6NumOverload(1227),
               slicePrefixMapNumOverload(1228),
               slicePrefixMapNumExceedingThreshold(1229),
               l2ExtAclGroupResOverload(1230),
               qppbOutCarStatResExceed90Threshold(1231),
               qppbOutCarStatResExceedThreshold(1232)
            }
            MAX-ACCESS accessible-for-notify
            STATUS current 
            DESCRIPTION
                "To describe the type of forwarding engine resource."
            ::= { hwFwdResTrapObject 3 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.4
        hwFwdResThreshold OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The threshold for trap."
            ::= { hwFwdResTrapObject 4 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.5
        hwL3FailedService OBJECT-TYPE
            SYNTAX OCTET STRING(SIZE(0..128))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "Layer 3 services failed to be delivered because of insufficient ACL resource."
            ::= { hwFwdResTrapObject 5 }  
            
        -- 1.3.6.1.4.1.2011.5.25.227.1.6
        hwCommand OBJECT-TYPE
            SYNTAX OCTET STRING(SIZE(0..256))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The Command failed to execute."
            ::= { hwFwdResTrapObject 6 }   
            
        -- 1.3.6.1.4.1.2011.5.25.227.1.7
        hwViewName OBJECT-TYPE
            SYNTAX OCTET STRING(SIZE(0..256))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The specific view of the command."
            ::= { hwFwdResTrapObject 7 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.1.8
        hwReasonDescription OBJECT-TYPE
            SYNTAX OCTET STRING(SIZE(0..256))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The specific description for failed reason."
            ::= { hwFwdResTrapObject 8 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.1.9
        hwFwdResLackVrId OBJECT-TYPE
            SYNTAX  Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The current vrid."
            ::= { hwFwdResTrapObject 9 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.10
        hwFwdProcFailForLCSOperationId OBJECT-TYPE
            SYNTAX INTEGER
            {
                l3vpnFibDownloadFailed(1)
            }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "To describe which operation is failed by reason of the license is not authorized."
            ::= { hwFwdResTrapObject 10 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.11
        hwFwdLicenseName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..31))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "To describe the license name."
            ::= { hwFwdResTrapObject 11 }
        --1.3.6.1.4.1.2011.5.25.227.1.12
        hwFwdResTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwFwdResEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
 	"This table provides the information of forward flow Table."
            ::= { hwFwdResTrapObject 12 }
  	
       --1.3.6.1.4.1.2011.5.25.227.1.12.1
       hwFwdResEntry OBJECT-TYPE
           SYNTAX HwFwdResEntry
           MAX-ACCESS not-accessible
           STATUS current
           DESCRIPTION
  	"Provides the information of a license forward flow entry."
           INDEX { hwFwdResDevName }
           ::= { hwFwdResTable 1 }
        HwFwdResEntry::=
           SEQUENCE { 
              hwFwdResDevName
                  OCTET STRING,
              hwFwdResLimit
 	Unsigned32,
              hwFwdResCurThroughput
  	Counter64
             }
  	 
       -- 1.3.6.1.4.1.2011.5.25.227.1.12.1.1
       hwFwdResDevName OBJECT-TYPE
         SYNTAX OCTET STRING(SIZE (0..31))
         MAX-ACCESS accessible-for-notify
         STATUS current
         DESCRIPTION
  	"The information for the dev name."
         ::= { hwFwdResEntry 1 }	
  
         -- 1.3.6.1.4.1.2011.5.25.227.1.12.1.2
         hwFwdResLimit OBJECT-TYPE
           SYNTAX Unsigned32
           MAX-ACCESS accessible-for-notify
           STATUS current
           DESCRIPTION
  	"The bandwidth configured for the license."
           ::= { hwFwdResEntry 2 }
  	
        -- 1.3.6.1.4.1.2011.5.25.227.1.12.1.3
        hwFwdResCurThroughput OBJECT-TYPE
           SYNTAX Counter64
           MAX-ACCESS accessible-for-notify
           STATUS current
           DESCRIPTION
  	"The current average system throughput."
          ::= { hwFwdResEntry 3 }

        --1.3.6.1.4.1.2011.5.25.227.1.13
        hwFpId OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
 	"The index for Fp."
            ::= { hwFwdResTrapObject 13 }

       -- 1.3.6.1.4.1.2011.5.25.227.1.14
       hwFpResourceType OBJECT-TYPE
           SYNTAX INTEGER
               {
               label(1),
               iid(2),
               unknown(100)
               }
          MAX-ACCESS accessible-for-notify
          STATUS current
          DESCRIPTION
                "To describe the type of Fp resource.
                Options:
                1.label(1)             -Indicates that the resource is label.
                2.iid(2)                 -Indicates that the resource iid.
                3.unknown(100)   -Indicates that the resource type is unknown."
         ::= { hwFwdResTrapObject 14 }	

        -- 1.3.6.1.4.1.2011.5.25.227.1.15
        hwFpResourceCurrentCount OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The value of this object identifies the number of current FP resources."
            ::= { hwFwdResTrapObject 15 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.16
        hwFpResourceTotalCount OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The value of this object identifies the total number of FP resources."
            ::= { hwFwdResTrapObject 16 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.17
        hwFpResourceThresholdUpperLimit OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The value of this object identifies the upper threshold for the number of FP resources."
            ::= { hwFwdResTrapObject 17 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.18
        hwFpResourceThresholdLowerLimit OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The value of this object identifies the lower threshold for the number of FP resources."
            ::= { hwFwdResTrapObject 18 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.19
        hwVpFeatureName OBJECT-TYPE
            SYNTAX OCTET STRING(SIZE(0..64))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The value of this object identifies the feature."
            ::= { hwFwdResTrapObject 19 }
	
        -- 1.3.6.1.4.1.2011.5.25.227.1.20
        hwServiceType OBJECT-TYPE
            SYNTAX INTEGER
            {
                vsi(1),
                arp(2),
                vrrp(3),
                multicast(4)
            }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The type for this service."
            ::= { hwFwdResTrapObject 20 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.21
        hwServiceIndex OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The index for this service."
            ::= { hwFwdResTrapObject 21 }
            
        -- 1.3.6.1.4.1.2011.5.25.227.1.22        
        hwServiceIndex2 OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The second index for this service."
            ::= { hwFwdResTrapObject 22 }
            
        -- 1.3.6.1.4.1.2011.5.25.227.1.23
        hwServiceIndex3 OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The third index for this service."
            ::= { hwFwdResTrapObject 23 }
            
        -- 1.3.6.1.4.1.2011.5.25.227.1.24
        hwServiceIndex4 OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The fourth index for this service."
            ::= { hwFwdResTrapObject 24 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.25
        hwNoSuppVxlanFragVni OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The VXLAN Vni."
            ::= { hwFwdResTrapObject 25 } 
            
        -- 1.3.6.1.4.1.2011.5.25.227.1.26
        hwNoSuppVxlanFragSourceIp OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The VXLAN source ip."
            ::= { hwFwdResTrapObject 26 }  
  
          -- 1.3.6.1.4.1.2011.5.25.227.1.27
        hwNoSuppVxlanFragPeerIp OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The VXLAN peer ip."
            ::= { hwFwdResTrapObject 27 }

          -- 1.3.6.1.4.1.2011.5.25.227.1.28
        hwFwdResLackIPStr OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The ip address."
            ::= { hwFwdResTrapObject 28 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.29
        hwFwdResLackVrfId OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The VRF ID."
            ::= { hwFwdResTrapObject 29 } 
   
       -- 1.3.6.1.4.1.2011.5.25.227.1.30
        hwTblResInfoTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwTblResInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
 	"This table provides the information of table resource information Table."
            ::= { hwFwdResTrapObject 30 }
  	
       -- 1.3.6.1.4.1.2011.5.25.227.1.30.1
       hwTblResInfoEntry OBJECT-TYPE
           SYNTAX HwTblResInfoEntry
           MAX-ACCESS not-accessible
           STATUS current
           DESCRIPTION
  	"Provides the information of table resource information entry."
           INDEX { hwTblResInfoSlotId, hwTblResInfoTblName }
           ::= { hwTblResInfoTable 1 }
        HwTblResInfoEntry::=
           SEQUENCE { 
              hwTblResInfoSlotId
                  OCTET STRING,
              hwTblResInfoTblName
                  OCTET STRING,
               hwTblResInfoTotalNumber
                   Unsigned32,
              hwTblResInfoAllocatedlNumber
                   Unsigned32,			  
              hwTblResInfoFreeNumber
 	           Unsigned32
             }
  	 
       -- 1.3.6.1.4.1.2011.5.25.227.1.30.1.1
       hwTblResInfoSlotId OBJECT-TYPE
         SYNTAX OCTET STRING(SIZE (0..15))
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
  	"The value of this object identifies the slot id."
         ::= { hwTblResInfoEntry 1 }	
  
         -- 1.3.6.1.4.1.2011.5.25.227.1.30.1.2
         hwTblResInfoTblName OBJECT-TYPE
           SYNTAX OCTET STRING(SIZE (0..63))
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
  	"The value of this object identifies the table name."
           ::= { hwTblResInfoEntry 2 }
  	
        -- 1.3.6.1.4.1.2011.5.25.227.1.30.1.3
        hwTblResInfoTotalNumber OBJECT-TYPE
           SYNTAX Unsigned32
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
  	"The value of this object identifies the number of total resource."
          ::= { hwTblResInfoEntry 3 }
		  
	 -- 1.3.6.1.4.1.2011.5.25.227.1.30.1.4
        hwTblResInfoAllocatedlNumber OBJECT-TYPE
           SYNTAX Unsigned32
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
  	"The value of this object identifies the number of allocated resource."
          ::= { hwTblResInfoEntry 4 }
		  
        -- 1.3.6.1.4.1.2011.5.25.227.1.30.1.5
        hwTblResInfoFreeNumber OBJECT-TYPE
           SYNTAX Unsigned32
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
  	"The value of this object identifies the number of free resource."
          ::= { hwTblResInfoEntry 5 }

    -- 1.3.6.1.4.1.2011.5.25.227.1.31
       hwFwdResIncomReasonId OBJECT-TYPE
          SYNTAX INTEGER
               {
	smoothIncomplete(1)
               }
      MAX-ACCESS accessible-for-notify
      STATUS current
      DESCRIPTION
                "To describe the type of data incomplete in forwarding engine resource."
      ::= { hwFwdResTrapObject 31 }

 -- 1.3.6.1.4.1.2011.5.25.227.1.32
       hwResOverwrittenSlot OBJECT-TYPE
           SYNTAX OCTET STRING
      MAX-ACCESS accessible-for-notify
      STATUS current
      DESCRIPTION
                " the slot id of overwritten resource."
      ::= { hwFwdResTrapObject 32 }

-- 1.3.6.1.4.1.2011.5.25.227.1.33
       hwResOverwrittenResType OBJECT-TYPE
       SYNTAX OCTET STRING
      MAX-ACCESS accessible-for-notify
      STATUS current
      DESCRIPTION
                "the resource type of overwritten resource."
      ::= { hwFwdResTrapObject 33 }

     -- 1.3.6.1.4.1.2011.5.25.227.1.34
        hwFwdResCongestReasonId OBJECT-TYPE
            SYNTAX INTEGER
               {
	fesDetectMsgCongest(1),
	eumDetectMsgCongest(2),
	rmDetectMsgCongest(3),
	vstmDetectMsgCongest(4)
               }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "To describe the type of board message congest in forwarding engine resource."
        ::= { hwFwdResTrapObject 34 }

     -- 1.3.6.1.4.1.2011.5.25.227.1.35
        hwFwdResLackFeNodeId OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "The FeNodeId."
        ::= { hwFwdResTrapObject 35 }

     -- 1.3.6.1.4.1.2011.5.25.227.1.36
        hwFwdSessionResUsage OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "Usage of the device session resources."
        ::= { hwFwdResTrapObject 36 }

     -- 1.3.6.1.4.1.2011.5.25.227.1.37
        hwSIDPoolID OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "SID pool ID."
        ::= { hwFwdResTrapObject 37 }
		
     -- 1.3.6.1.4.1.2011.5.25.227.1.38
        hwSIDResourceCurrentCount OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "The value of this object identifies the number of current SID pool."
        ::= { hwFwdResTrapObject 38 }
		
     -- 1.3.6.1.4.1.2011.5.25.227.1.39
        hwSIDResourceTotalCount OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "The value of this object identifies the total number of SID pool."
        ::= { hwFwdResTrapObject 39 }
		
     -- 1.3.6.1.4.1.2011.5.25.227.1.40
        hwSIDResourceThresholdUpperLimit OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "The value of this object identifies the upper threshold for the number of SID pool."
        ::= { hwFwdResTrapObject 40 }
		
     -- 1.3.6.1.4.1.2011.5.25.227.1.41
        hwSIDResourceThresholdLowerLimit OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "UThe value of this object identifies the lower threshold for the number of SID pool."
        ::= { hwFwdResTrapObject 41 }

     -- 1.3.6.1.4.1.2011.5.25.227.1.42
        hwProducerComponentName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "the producer component name."
        ::= { hwFwdResTrapObject 42 }
		
     -- 1.3.6.1.4.1.2011.5.25.227.1.43
        hwConsumerComponentName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "the consumer component name."
        ::= { hwFwdResTrapObject 43 }

    -- 1.3.6.1.4.1.2011.5.25.227.1.44
        hwSmoothFailedReasonId OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "the reason id."
        ::= { hwFwdResTrapObject 44 }

    -- 1.3.6.1.4.1.2011.5.25.227.1.45
        hwEMDIInstanceId OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "the emdi instance id."
        ::= { hwFwdResTrapObject 45 }
           
    -- 1.3.6.1.4.1.2011.5.25.227.1.46
        hwEMDIIndicatorType OBJECT-TYPE
            SYNTAX INTEGER
                {
                    emdiIndicatorRtpLR(1),
                    emdiIndicatorRtpSER(2),
                    emdiIndicatorUPLR(3),
                    emdiIndicatorDPLR(4)

                }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "the emdi alarm type."
            ::= { hwFwdResTrapObject 46 }

    -- 1.3.6.1.4.1.2011.5.25.227.1.47
        hwEMDIIndicatorValue OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "the  value of emdi alarm."
        ::= { hwFwdResTrapObject 47 }
        
    -- 1.3.6.1.4.1.2011.5.25.227.1.48
        hwEMDIThreshold OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "the  threshold of emdi alarm."
        ::= { hwFwdResTrapObject 48 }

    -- 1.3.6.1.4.1.2011.5.25.227.1.49
        hwMcLeafCfcCheckSlot OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "the slot id of mc leaf cfc check error."
        ::= { hwFwdResTrapObject 49 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.50
        hwAutoDiagnoseReasonId OBJECT-TYPE
            SYNTAX INTEGER
        {
            sfuInterruptAlarm(1),
            lpuModifyPacketAlarm(2),
            sfuLinklossAlarm(3)
        }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "Describe the type of faults detected by the AutoDiagnose system."
            ::= { hwFwdResTrapObject 50 }

        hwVxlanTnlPeerIpAddr OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "This object indicates the Peer IP address."
            ::= { hwFwdResTrapObject 51 }
			
        hwVxlanNveMac OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "This object indicates the NVE MAC address."
            ::= { hwFwdResTrapObject 52 }       	

		hwFibDeliverSlotId OBJECT-TYPE
			SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The information for the slot."
            ::= { hwFwdResTrapObject 54 } 

         -- 1.3.6.1.4.1.2011.5.25.227.1.55
        hwSysResChgSlotStr OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The information for the slot."
            ::= { hwFwdResTrapObject 55 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.1.56
        hwSysResChgReasonId OBJECT-TYPE
            SYNTAX INTEGER
                {
                uftResModeChanged(1),
                enpResModeChanged(2),
                arpResAllocationModeChanged(3),
                riotResChanged(4),
                fibv4ResChanged(5),
                l3ResAllocationModeChanged(6),
                l3IfResAllocationModeChanged(7),
                aclExResChanged(8),
                ipv6LongMaskResChanged(9),
                l3ForwardHashResChanged(10),
                uatResAllocationModeChanged(11),
                ipv6VxlanResChanged(12),
                srHashResChanged(13),
                mplsResChanged(14),
                dot1q8021pResChanged(15),
                externalTcamResChanged(16),
                uatHashResModeChanged(17),
                ethtrunkModeChanged(18),
                ingressVlanXlateModeChanged(19),
                egressVlanXlateModeChanged(20),
                qosaifabricdppModeChanged(21),
                qosBuffAutoConfigChanged(22),
                qosLosslessModeChanged(23),
                incConfigChanged(24)
                }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "To describe the type of fowarding engine resource."
            ::= { hwFwdResTrapObject 56 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.57
        hwSysResChgReasonDescription OBJECT-TYPE
            SYNTAX OCTET STRING(SIZE(0..256))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The specific description for failed reason."
            ::= { hwFwdResTrapObject 57 }

     -- 1.3.6.1.4.1.2011.5.25.227.1.58
		hwSessThreshold OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"The threshold of the device session resources."
		::= { hwFwdResTrapObject 58 }

    -- 1.3.6.1.4.1.2011.5.25.227.1.59
        hwAclRuleResUsage OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "Usage of the device acl rule resources."
        ::= { hwFwdResTrapObject 59 }

    -- 1.3.6.1.4.1.2011.5.25.227.1.60
        hwAclRuleThreshold OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "The threshold of the device acl rule resources."
        ::= { hwFwdResTrapObject 60 }
    
    -- 1.3.6.1.4.1.2011.5.25.227.1.61
        hwAclGroupResUsage OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "Usage of the device acl group resources."
        ::= { hwFwdResTrapObject 61 }
    
    -- 1.3.6.1.4.1.2011.5.25.227.1.62
        hwAclGroupThreshold OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "The threshold of the device acl group resources."
        ::= { hwFwdResTrapObject 62 }
   
    -- 1.3.6.1.4.1.2011.5.25.227.1.63
        hwEMDISlotStr OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "The slot of the device emdi resources."
        ::= { hwFwdResTrapObject 63 }

      -- 1.3.6.1.4.1.2011.5.25.227.1.64
        hwEMDIResUsed OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "The used of the device emdi resources."
        ::= { hwFwdResTrapObject 64 }  
     
     -- 1.3.6.1.4.1.2011.5.25.227.1.65
        hwEMDIResTotal OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "The total of the device emdi resources."
        ::= { hwFwdResTrapObject 65 }

        hwPacketChangeInPort OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "This object indicates the changed packet's in port."
            ::= { hwFwdResTrapObject 66 }
			
        hwPacketChangeOutPort OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "This object indicates the changed packet's out port."
            ::= { hwFwdResTrapObject 67 } 
      	
      -- 1.3.6.1.4.1.2011.5.25.227.1.68
        hwSaidPingDetectInterface OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "The detect port of the SAID PING node."
        ::= { hwFwdResTrapObject 68 }
		
    -- 1.3.6.1.4.1.2011.5.25.227.1.69
        hwNetStreamIPv4OriginalFlowUsage OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "Usage of the NetStream IPv4 original flows."
        ::= { hwFwdResTrapObject 69 }

    -- 1.3.6.1.4.1.2011.5.25.227.1.70
        hwNetStreamIPv4OriginalFlowThreshold OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "Threshold of the NetStream IPv4 original flows."
        ::= { hwFwdResTrapObject 70 }		
		
    -- 1.3.6.1.4.1.2011.5.25.227.1.71
        hwNetStreamIPv4FlexibleFlowUsage OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "Usage of the NetStream IPv4 flexible flows."
        ::= { hwFwdResTrapObject 71 }

    -- 1.3.6.1.4.1.2011.5.25.227.1.72
        hwNetStreamIPv4FlexibleFlowThreshold OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "Threshold of the NetStream IPv4 flexible flows."
        ::= { hwFwdResTrapObject 72 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.73
        hwFwmFaultSlotStr OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The information for the slot."
            ::= { hwFwdResTrapObject 73 }    

        -- 1.3.6.1.4.1.2011.5.25.227.1.74
        hwFwmFaultCpuStr OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The information for the cpu."
            ::= { hwFwdResTrapObject 74 }    

        -- 1.3.6.1.4.1.2011.5.25.227.1.75
        hwFwmFaultReasonId OBJECT-TYPE
            SYNTAX INTEGER
            {
                ipv4FibDbNotResponse(1),
                ipv6FibDbNotResponse(2)
            }
            MAX-ACCESS accessible-for-notify
            STATUS current 
            DESCRIPTION
                "To describe the reason id of forwarding manage module fault."
            ::= { hwFwdResTrapObject 75 }

			
        -- 1.3.6.1.4.1.2011.5.25.227.1.76
        hwFwmFaultReasonDescription OBJECT-TYPE
            SYNTAX OCTET STRING(SIZE(0..256))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The specific description for failed reason."
            ::= { hwFwdResTrapObject 76 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.77
        hwFwmSliceInterfaceName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..64))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The physical interface name."
            ::= { hwFwdResTrapObject 77 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.78
        hwFwmSliceId OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "Slice id."
            ::= { hwFwdResTrapObject 78 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.79
        hwFwmSliceTrunkInterfaceName OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The trunk interface name."
            ::= { hwFwdResTrapObject 79 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.80
        hwFwmSliceSrcInterfaceName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..64))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The source physical interface name."
            ::= { hwFwdResTrapObject 80 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.81
        hwFwmSliceResourceReasonId OBJECT-TYPE
            SYNTAX INTEGER
            {
                bandwidthInsufficient(1),
                sliceResourcePerInterfaceInsufficient(2),
                sliceResourcePerChipInsufficient(3),
                chanIfBandwidthInsufficient(4)
            }
            MAX-ACCESS accessible-for-notify
            STATUS current 
            DESCRIPTION
                "To describe the reason id of slice resource fault."
            ::= { hwFwdResTrapObject 81 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.82
        hwFwmSliceFwdReasonId OBJECT-TYPE
            SYNTAX INTEGER
            {
                sliceMapQueueMissMatch(1),
                sliceMapMissMatch(2)
            }
            MAX-ACCESS accessible-for-notify
            STATUS current 
            DESCRIPTION
                "To describe the reason id of slice fowarding fault."
            ::= { hwFwdResTrapObject 82 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.83
        hwFwmSliceSlotStr OBJECT-TYPE
            SYNTAX OCTET STRING
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The information for the slot."
            ::= { hwFwdResTrapObject 83 }

        -- 1.3.6.1.4.1.2011.5.25.227.1.84
        hwFwmSliceReasonDescription OBJECT-TYPE
            SYNTAX OCTET STRING(SIZE(0..256))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The specific description for failed reason."
            ::= { hwFwdResTrapObject 84 }

       -- 1.3.6.1.4.1.2011.5.25.227.1.85
	TopNSourceIpAddress OBJECT-TYPE
	    SYNTAX OCTET STRING(SIZE(0..256))
	    MAX-ACCESS accessible-for-notify
	    STATUS current
	    DESCRIPTION
		"Source IP address with the highest session resource usage. A maximum of three source IP addresses can be displayed. If multiple source IP addresses are displayed, they are separated by commas (,)."
		::= { hwFwdResTrapObject 85 }

       -- 1.3.6.1.4.1.2011.5.25.227.1.86
	hwSessionCurEntryNum OBJECT-TYPE
	    SYNTAX Unsigned32
	    MAX-ACCESS accessible-for-notify
	    STATUS current
	    DESCRIPTION
		"The number of current session entries."
		::= { hwFwdResTrapObject 86 }

       -- 1.3.6.1.4.1.2011.5.25.227.1.87
	hwSessionLeakEntryNum OBJECT-TYPE
	    SYNTAX Unsigned32
	    MAX-ACCESS accessible-for-notify
	    STATUS current
	    DESCRIPTION
		"The number of leak session entries."
		::= { hwFwdResTrapObject 87 }

       -- 1.3.6.1.4.1.2011.5.25.227.1.88
	hwSessionUnrecEntryNum OBJECT-TYPE
	    SYNTAX Unsigned32
	    MAX-ACCESS accessible-for-notify
	    STATUS current
	    DESCRIPTION
		"The number of unrecoverable session entries."
		::= { hwFwdResTrapObject 88 }

       -- 1.3.6.1.4.1.2011.5.25.227.1.89
	hwSessionSpecification OBJECT-TYPE
	    SYNTAX Unsigned32
	    MAX-ACCESS accessible-for-notify
	    STATUS current
	    DESCRIPTION
		"Session specification."
		::= { hwFwdResTrapObject 89 }

       -- 1.3.6.1.4.1.2011.5.25.227.1.90
	hwSessionLeakUsage OBJECT-TYPE
	    SYNTAX Unsigned32
	    MAX-ACCESS accessible-for-notify
	    STATUS current
	    DESCRIPTION
		"The ratio of the number of leaked entries in the current session table to the number of specifications."
		::= { hwFwdResTrapObject 90 }

       -- 1.3.6.1.4.1.2011.5.25.227.1.91
	hwSessionLeakThreshold OBJECT-TYPE
	    SYNTAX Unsigned32
	    MAX-ACCESS accessible-for-notify
	    STATUS current
	    DESCRIPTION
		"Alarm threshold for leaked entries in the session table."
		::= { hwFwdResTrapObject 91 }

       -- 1.3.6.1.4.1.2011.5.25.227.1.92
	hwSessionUnrecUsage OBJECT-TYPE
	    SYNTAX Unsigned32
	    MAX-ACCESS accessible-for-notify
	    STATUS current
	    DESCRIPTION
		"The ratio of the number of unrecoverable entries in the current session table to the number of specifications."
		::= { hwFwdResTrapObject 92 }

       -- 1.3.6.1.4.1.2011.5.25.227.1.93
	hwSessionUnrecThreshold OBJECT-TYPE
	    SYNTAX Unsigned32
	    MAX-ACCESS accessible-for-notify
	    STATUS current
	    DESCRIPTION
		"Alarm threshold for unrecoverable entries in the session table."
		::= { hwFwdResTrapObject 93 }
		
		-- 1.3.6.1.4.1.2011.5.25.227.1.94
    hwL2mcGrpAddress OBJECT-TYPE
        SYNTAX OCTET STRING
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
        "The group address of the L2MC."
        ::= { hwFwdResTrapObject 94 }
		
		-- 1.3.6.1.4.1.2011.5.25.227.1.95
    hwL2mcVlanIdx OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
        "The vlan of the L2MC."
        ::= { hwFwdResTrapObject 95 }

		-- 1.3.6.1.4.1.2011.5.25.227.1.96
    hwMcastElbUsage OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
        "The ratio of the multicast egress interfaces resource to the limit."
        ::= { hwFwdResTrapObject 96 }

		-- 1.3.6.1.4.1.2011.5.25.227.1.97
    hwMcastElbThreshold OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
        "Threshold for multicast egress interfaces resource usage to trigger the alarm or to clear the alarm."
        ::= { hwFwdResTrapObject 97 }

    -- 1.3.6.1.4.1.2011.5.25.227.1.98
    hwEntiyPhysicalindex OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
        "Index of the entity."
        ::= { hwFwdResTrapObject 98 }

    -- 1.3.6.1.4.1.2011.5.25.227.1.99
    hwFwdTableId OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
        "Table ID."
        ::= { hwFwdResTrapObject 99 }

    -- 1.3.6.1.4.1.2011.5.25.227.1.100
    hwFwdTableName OBJECT-TYPE
        SYNTAX OCTET STRING
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
        "Table Name."
        ::= { hwFwdResTrapObject 100 }

    -- 1.3.6.1.4.1.2011.5.25.227.1.101
    hwFwmSliceConflitReasonId OBJECT-TYPE
        SYNTAX INTEGER
        {
            sliceStackConflict(1),
            sameGroupSliceStackConflict(2)
        }
        MAX-ACCESS accessible-for-notify
        STATUS current 
        DESCRIPTION
            "The reason id of slice configuration conflict."
        ::= { hwFwdResTrapObject 101 }

     -- 1.3.6.1.4.1.2011.5.25.227.1.102
        hwEnterModeReasonId OBJECT-TYPE
            SYNTAX INTEGER
               {
	fesEnterSpecialMode(1)
               }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "To describe the type of FES enters the special processing mode."
        ::= { hwFwdResTrapObject 102 }
 
     -- 1.3.6.1.4.1.2011.5.25.227.1.103
        hwEnterModeId OBJECT-TYPE
            SYNTAX Unsigned32
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                 "The SpecialModeId."
        ::= { hwFwdResTrapObject 103 }
		
       -- 1.3.6.1.4.1.2011.5.25.227.2
        hwFwdResTraps OBJECT IDENTIFIER ::= { hwFwdResTrapMIB 2 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.2.1
        hwFwdResLacTrap OBJECT IDENTIFIER ::= { hwFwdResTraps 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.1
        hwWholeFwdResLack NOTIFICATION-TYPE
            OBJECTS { hwEntPhysicalindex, entPhysicalName, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                "The alarm is generated when the system's forwarding engine resources are insufficient."
            ::= { hwFwdResLacTrap 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.2
        hwWholeFwdResLackResume NOTIFICATION-TYPE
            OBJECTS { hwEntPhysicalindex, entPhysicalName, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                "The alarm is generated when the system's forwarding engine resources are no longer insufficient."
            ::= { hwFwdResLacTrap 2 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.3
        hwBoardFwdResLack NOTIFICATION-TYPE
            OBJECTS { hwEntPhysicalindex, entPhysicalName, hwFwdResLackSlotStr, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                "The alarm is generated when a board's forwarding engine resources are insufficient."
            ::= { hwFwdResLacTrap 3 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.4
        hwBoardFwdResLackResume NOTIFICATION-TYPE
            OBJECTS { hwEntPhysicalindex, entPhysicalName, hwFwdResLackSlotStr, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                "The alarm is generated when a board's forwarding engine resources are no longer insufficient."
            ::= { hwFwdResLacTrap 4 }

        -- 1.3.6.1.4.1.2011.5.25.227.2.1.5
        hwBoardL3FwdResLack NOTIFICATION-TYPE
            OBJECTS { hwFwdResThreshold, hwEntPhysicalindex, entPhysicalName, hwFwdResLackSlotStr, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                "The L3 forwarding engine resources were overloaded."
            ::= { hwFwdResLacTrap 5 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.6
        hwBoardL3FwdResLackResume NOTIFICATION-TYPE
            OBJECTS { hwFwdResThreshold, hwEntPhysicalindex, entPhysicalName, hwFwdResLackSlotStr, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                "The L3 forwarding engine resources were resumed."
            ::= { hwFwdResLacTrap 6 }
            
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.7
        hwBoardL3ACLResLack NOTIFICATION-TYPE
            OBJECTS { hwL3FailedService, hwFwdResLackSlotStr, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                "ACL failed to be delivered."
            ::= { hwFwdResLacTrap 7 }
            
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.8
        hwBoardL2mcResLack NOTIFICATION-TYPE
            OBJECTS { hwFwdResThreshold, hwFwdResLackSlotStr, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                "The l2mc index resources were overloaded."
            ::= { hwFwdResLacTrap 8 }    
                    
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.9
        hwBoardL2mcResLackResume NOTIFICATION-TYPE
            OBJECTS { hwFwdResThreshold, hwFwdResLackSlotStr, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                "The l2mc index resources were resumed."
            ::= { hwFwdResLacTrap 9 }        
            
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.10
        hwBoardIpmcResLack NOTIFICATION-TYPE
            OBJECTS { hwFwdResThreshold, hwFwdResLackSlotStr, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                "The ipmc index resources were overloaded."
            ::= { hwFwdResLacTrap 10 }       
                 
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.11
        hwBoardIpmcResLackResume NOTIFICATION-TYPE
            OBJECTS { hwFwdResThreshold, hwFwdResLackSlotStr, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                "The ipmc index resources were resumed."
            ::= { hwFwdResLacTrap 11 }          
            
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.12
        hwBoardServiceFailed NOTIFICATION-TYPE
            OBJECTS { hwCommand, hwViewName, hwFwdResLackReasonId, hwReasonDescription, hwFwdResLackSlotStr }
            STATUS current
            DESCRIPTION 
                "Service failed because resources were overloaded."
            ::= { hwFwdResLacTrap 12 }

        -- 1.3.6.1.4.1.2011.5.25.227.2.1.13
        hwWholeFwdResThresholdExceed NOTIFICATION-TYPE
            OBJECTS { hwEntPhysicalindex, entPhysicalName, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                        "Too many services are configured, and the upper limit of the system's forwarding resources is reached."
            ::= { hwFwdResLacTrap 13 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.14
        hwWholeFwdResThresholdExceedResume NOTIFICATION-TYPE
            OBJECTS { hwEntPhysicalindex, entPhysicalName, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                        "The value of this object identifies an FP resource type.
                         1: Label resources (1)
                         2. IID resources (2)
                         3. Resources of an unknown type (100)."
            ::= { hwFwdResLacTrap 14 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.15
        hwBoardFwdResThresholdExceed NOTIFICATION-TYPE
            OBJECTS { hwEntPhysicalindex, entPhysicalName, hwFwdResLackSlotStr, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                        "The value of this object identifies the number of current FP resources."
            ::= { hwFwdResLacTrap 15 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.16
        hwBoardFwdResThresholdExceedResume NOTIFICATION-TYPE
            OBJECTS { hwEntPhysicalindex, entPhysicalName, hwFwdResLackSlotStr, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                        "The value of this object identifies the total number of FP resources."
            ::= { hwFwdResLacTrap 16 }

        -- 1.3.6.1.4.1.2011.5.25.227.2.1.17
        hwBoardMplsPhpNonsupport NOTIFICATION-TYPE
            OBJECTS { hwFwdResLackSlotStr}
            STATUS current
            DESCRIPTION 
                        "One or more boards do not support MPLS PHP."
            ::= { hwFwdResLacTrap 17 }
            
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.18
        hwBoardResThresholdExceed NOTIFICATION-TYPE
            OBJECTS { hwFwdResLackSlotStr, hwFwdResThreshold, hwFwdResLackReasonId , hwReasonDescription}
            STATUS current
            DESCRIPTION 
                        "The number of forwarding resources reaches the alarm threshold."
            ::= { hwFwdResLacTrap 18 }
            
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.19
        hwBoardResThresholdExceedResume NOTIFICATION-TYPE
            OBJECTS { hwFwdResLackSlotStr,hwFwdResThreshold, hwFwdResLackReasonId , hwReasonDescription }
            STATUS current
            DESCRIPTION 
                        "The number of forwarding engine resources is less than the threshold."
            ::= { hwFwdResLacTrap 19 }
			
	    -- 1.3.6.1.4.1.2011.5.25.227.2.1.20
        hwBoardResWarningThresholdExceed NOTIFICATION-TYPE
            OBJECTS {  hwFwdResLackSlotStr,hwFwdResThreshold,  hwFwdResLackReasonId , hwReasonDescription}
            STATUS current
            DESCRIPTION 
                        "The number of board forwarding engine resources reaches the threshold."
            ::= { hwFwdResLacTrap 20}
            
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.21
        hwBoardResWarningThresholdExceedResume NOTIFICATION-TYPE
            OBJECTS { hwFwdResLackSlotStr,hwFwdResThreshold,  hwFwdResLackReasonId , hwReasonDescription}
            STATUS current
            DESCRIPTION 
                        "The number of board forwarding engine resources is less than the threshold."
            ::= { hwFwdResLacTrap 21 }
           
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.22
        hwBoardIPv6ACLResLack NOTIFICATION-TYPE
            OBJECTS { hwViewName,hwFwdResLackSlotStr}
            STATUS current
            DESCRIPTION 
                        "Service failed because of insufficient resources."
            ::= { hwFwdResLacTrap 22 }
            
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.23
        hwBoardMplsPhpResLack NOTIFICATION-TYPE
            OBJECTS {hwFwdResLackSlotStr}
            STATUS current
            DESCRIPTION 
                        "PHP labels added failed because of insufficient resource."
            ::= { hwFwdResLacTrap 23 }
			
        -- 1.3.6.1.4.1.2011.5.25.227.2.2
        hwFwdProcFailForLCSTrap OBJECT IDENTIFIER ::= { hwFwdResTraps 2 }

        -- 1.3.6.1.4.1.2011.5.25.227.2.2.1
        hwFwdProcFailForLCS NOTIFICATION-TYPE
            OBJECTS { hwFwdLicenseName, hwFwdResLackSlotStr, hwFwdProcFailForLCSOperationId }
            STATUS current
            DESCRIPTION 
                "Operation is failed by reason of the license is not authorized."
            ::= { hwFwdProcFailForLCSTrap 1 }

        -- 1.3.6.1.4.1.2011.5.25.227.2.2.2
        hwFwdProcFailForLCSResume NOTIFICATION-TYPE
            OBJECTS { hwFwdLicenseName, hwFwdResLackSlotStr, hwFwdProcFailForLCSOperationId }
            STATUS current
            DESCRIPTION 
                "The license is authorized."
            ::= { hwFwdProcFailForLCSTrap 2 }

        -- 1.3.6.1.4.1.2011.5.25.227.2.3
        hwFwdEntryConflictTrap OBJECT IDENTIFIER ::= { hwFwdResTraps 3 }

        -- 1.3.6.1.4.1.2011.5.25.227.2.3.1
        hwFwdEntryConflict NOTIFICATION-TYPE
            OBJECTS { hwFwdResLackSlotStr, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                " Table check failed."
            ::= { hwFwdEntryConflictTrap 1 }

        -- 1.3.6.1.4.1.2011.5.25.227.2.3.2
        hwFwdEntryConflictResume NOTIFICATION-TYPE
            OBJECTS { hwFwdResLackSlotStr, hwFwdResLackReasonId }
            STATUS current
            DESCRIPTION 
                "The table check failure was removed."
            ::= { hwFwdEntryConflictTrap 2 }

        -- 1.3.6.1.4.1.2011.5.25.227.2.3.3
        hwFwdEntryInconsistent NOTIFICATION-TYPE
            OBJECTS { hwServiceType, hwServiceIndex, hwServiceIndex2, hwServiceIndex3, hwServiceIndex4, hwReasonDescription }
            STATUS current
            DESCRIPTION 
                " Service table check inconsistent."
            ::= { hwFwdEntryConflictTrap 3 }

        -- 1.3.6.1.4.1.2011.5.25.227.2.3.4
        hwFwdEntryInconsistentResume NOTIFICATION-TYPE
            OBJECTS  { hwServiceType, hwServiceIndex, hwServiceIndex2, hwServiceIndex3, hwServiceIndex4, hwReasonDescription }
            STATUS current
            DESCRIPTION 
                "The service table check inconsistent was removed."
            ::= { hwFwdEntryConflictTrap 4 }		
		
       -- 1.3.6.1.4.1.2011.5.25.227.2.3.7
        hwFibDeliverFailed NOTIFICATION-TYPE
            OBJECTS { hwFibDeliverSlotId }
            STATUS current
            DESCRIPTION 
                        "The route failed to be delivered because of internal error."
            ::= { hwFwdEntryConflictTrap 7 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.2.3.8
        hwFibDeliverFailedResume NOTIFICATION-TYPE
            OBJECTS { hwFibDeliverSlotId }
            STATUS current
            DESCRIPTION 
                        "The route success to be delivered in 24hours."
            ::= { hwFwdEntryConflictTrap 8 }
			
       -- 1.3.6.1.4.1.2011.5.25.227.2.4
       hwFwdResIncompTrap OBJECT IDENTIFIER ::= { hwFwdResTraps 4 }

        -- 1.3.6.1.4.1.2011.5.25.227.2.4.1
        hwFwdDataSyncIncomplete NOTIFICATION-TYPE
            OBJECTS { hwFwdResIncomReasonId }
            STATUS current
            DESCRIPTION 
                        "Data synchronization is incomplete."
            ::= { hwFwdResIncompTrap 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.2.4.2
        hwFwdDataSyncIncompleteResume NOTIFICATION-TYPE
            OBJECTS { hwFwdResIncomReasonId }
            STATUS current
            DESCRIPTION 
                        "Data synchronization is restored."
            ::= { hwFwdResIncompTrap 2 }

       -- 1.3.6.1.4.1.2011.5.25.227.2.5
       hwResourceOverwrittenTrap OBJECT IDENTIFIER ::= { hwFwdResTraps 5 }
        -- 1.3.6.1.4.1.2011.5.25.227.2.5.1
        hwResourceOverwrittenAlarm NOTIFICATION-TYPE
            OBJECTS { hwResOverwrittenSlot,  hwResOverwrittenResType}
            STATUS current
            DESCRIPTION 
                        "Chip resources are overwritten."
            ::= { hwResourceOverwrittenTrap 1 }
        -- 1.3.6.1.4.1.2011.5.25.227.2.5.2
        hwResourceOverwrittenAlarmResume NOTIFICATION-TYPE
            OBJECTS { hwResOverwrittenSlot,  hwResOverwrittenResType}
            STATUS current
            DESCRIPTION 
                        "Overwritten chip resources are recovered."
            ::= { hwResourceOverwrittenTrap 2}

       -- 1.3.6.1.4.1.2011.5.25.227.2.6
       hwFwdResMsgCongestTrap OBJECT IDENTIFIER ::= { hwFwdResTraps 6 }
		
        -- 1.3.6.1.4.1.2011.5.25.227.2.6.1
        hwBoardFwdMsgCongest NOTIFICATION-TYPE
            OBJECTS { hwFwdResLackSlotStr, hwFwdResLackFeNodeId, hwFwdResCongestReasonId }
            STATUS current
            DESCRIPTION 
                        "The message forwarding on the board is congested."
            ::= { hwFwdResMsgCongestTrap 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.2.6.2
        hwBoardFwdMsgCongestResume NOTIFICATION-TYPE
            OBJECTS { hwFwdResLackSlotStr, hwFwdResLackFeNodeId, hwFwdResCongestReasonId }
            STATUS current
            DESCRIPTION 
                        "The message forwarding congestion is resolved."
            ::= { hwFwdResMsgCongestTrap 2 }
			
       -- 1.3.6.1.4.1.2011.5.25.227.2.7
       hwMcLeafCfcCheckTrap OBJECT IDENTIFIER ::= { hwFwdResTraps 7 }
		
        -- 1.3.6.1.4.1.2011.5.25.227.2.7.1
        hwMcLeafCfcCheck NOTIFICATION-TYPE
            OBJECTS {  hwMcLeafCfcCheckSlot }
            STATUS current
            DESCRIPTION 
                        "The multicast leaf count check inconsistent."
            ::= { hwMcLeafCfcCheckTrap 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.2.7.2
        hwMcLeafCfcCheckResume NOTIFICATION-TYPE
            OBJECTS {  hwMcLeafCfcCheckSlot }
            STATUS current
            DESCRIPTION 
                        "The multicast leaf count check inconsistent was removed."
            ::= { hwMcLeafCfcCheckTrap 2 }
    
       -- 1.3.6.1.4.1.2011.5.25.227.2.8
       hwMplsLabelExceedTrap OBJECT IDENTIFIER ::= { hwFwdResTraps 8 }
        -- 1.3.6.1.4.1.2011.5.25.227.2.8.1
        hwMplsLabelExceedAlarm NOTIFICATION-TYPE
            STATUS current
            DESCRIPTION 
                        "The number of labels exceeds the device's encapsulation capability."
            ::= { hwMplsLabelExceedTrap 1 }
        -- 1.3.6.1.4.1.2011.5.25.227.2.8.2
        hwMplsLabelExceedAlarmResume NOTIFICATION-TYPE
            STATUS current
            DESCRIPTION 
                        "The problem that the number of labels exceeds the device's encapsulation capability has been resolved."
            ::= { hwMplsLabelExceedTrap 2}

        hwVxlanNveMacConflictTrap OBJECT IDENTIFIER ::= { hwFwdResTraps 9 }
        hwVxlanNveMacConflict NOTIFICATION-TYPE
            OBJECTS { hwVxlanNveMac, hwVxlanTnlPeerIpAddr}
            STATUS current
            DESCRIPTION
                "MAC addresses of NVE interfaces on distributed VXLAN gateways conflict."
            ::= { hwVxlanNveMacConflictTrap 1 }
        hwVxlanNveMacConflictClear NOTIFICATION-TYPE
            OBJECTS { hwVxlanNveMac, hwVxlanTnlPeerIpAddr}
            STATUS current
            DESCRIPTION
                "MAC addresses of NVE interfaces on distributed VXLAN gateways conflict resolved."
            ::= { hwVxlanNveMacConflictTrap 2 }

        -- 1.3.6.1.4.1.2011.5.25.227.2.10
        hwNsFlowEntryExceedTrap OBJECT IDENTIFIER ::= { hwFwdResTraps 10 }
		
		-- 1.3.6.1.4.1.2011.5.25.227.2.10.1
		hwNsOrigFlexFlowExceedAlarm NOTIFICATION-TYPE
            OBJECTS { hwFwdResLackSlotStr }
            STATUS current
            DESCRIPTION
                "The usage of NetStream original and flexible flow entries exceeded 80%."
            ::= { hwNsFlowEntryExceedTrap 1 }
        -- 1.3.6.1.4.1.2011.5.25.227.2.10.2
        hwNsOrigFlexFlowExceedResume NOTIFICATION-TYPE
            OBJECTS { hwFwdResLackSlotStr }
            STATUS current
            DESCRIPTION
                "The usage of NetStream original and flexible flow entries fell below 70%."
            ::= { hwNsFlowEntryExceedTrap 2 }
        -- 1.3.6.1.4.1.2011.5.25.227.2.10.3
        hwNsAggFlowExceedAlarm NOTIFICATION-TYPE
            OBJECTS { hwFwdResLackSlotStr }
            STATUS current
            DESCRIPTION
                "The usage of NetStream aggregation flow entries exceeded 80%."
            ::= { hwNsFlowEntryExceedTrap 3 }
		-- 1.3.6.1.4.1.2011.5.25.227.2.10.4
        hwNsAggFlowExceedResume NOTIFICATION-TYPE
            OBJECTS { hwFwdResLackSlotStr }
            STATUS current
            DESCRIPTION
                "The usage of NetStream aggregation flow entries fell below 70%."
            ::= { hwNsFlowEntryExceedTrap 4 }

        -- 1.3.6.1.4.1.2011.5.25.227.2.11
        hwNvo3VxlanSrcIpDiffTrap OBJECT IDENTIFIER ::= { hwFwdResTraps 11 }
        -- 1.3.6.1.4.1.2011.5.25.227.2.11.1
        hwNvo3VxlanSrcIpDiffAlarm NOTIFICATION-TYPE
            OBJECTS { hwVxlanTnlPeerIpAddr}
            STATUS current
            DESCRIPTION
                "Multiple VXLAN tunnels have different local IP addresses and the same destination IP address, which may affect traffic forwarding. Change the local IP addresses to be the same."
            ::= { hwNvo3VxlanSrcIpDiffTrap 1 }
        -- 1.3.6.1.4.1.2011.5.25.227.2.11.2
        hwNvo3VxlanSrcIpDiffAlarmResume NOTIFICATION-TYPE
            OBJECTS { hwVxlanTnlPeerIpAddr}
            STATUS current
            DESCRIPTION
                "The alarm caused by different local IP addresses of multiple VXLAN tunnels is cleared."
            ::= { hwNvo3VxlanSrcIpDiffTrap 2 }

        hwPacketChangeTrap OBJECT IDENTIFIER ::= { hwFwdResTraps 12 }
        hwPacketChange NOTIFICATION-TYPE
            OBJECTS { hwPacketChangeInPort, hwPacketChangeOutPort}
            STATUS current
            DESCRIPTION
                "Packets are changed."
            ::= { hwPacketChangeTrap 1 }
        hwPacketChangeClear NOTIFICATION-TYPE
            OBJECTS { hwPacketChangeInPort, hwPacketChangeOutPort}
            STATUS current
            DESCRIPTION
                "Packets are no longer changed."
            ::= { hwPacketChangeTrap 2 }

        -- 1.3.6.1.4.1.2011.5.25.227.2.13
       hwFesEnterSpecialModeTrap OBJECT IDENTIFIER ::= { hwFwdResTraps 13 }
		
        -- 1.3.6.1.4.1.2011.5.25.227.2.13.1
        hwFesEnterSpecialMode NOTIFICATION-TYPE
            OBJECTS { hwEnterModeReasonId, hwEnterModeId }
            STATUS current
            DESCRIPTION 
                        "FES enters the special processing mode."
            ::= { hwFesEnterSpecialModeTrap 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.2.13.2
        hwFesEnterSpecialModeResume NOTIFICATION-TYPE
            OBJECTS { hwEnterModeReasonId, hwEnterModeId }
            STATUS current
            DESCRIPTION 
                        "FES restores to the normal processing mode."
            ::= { hwFesEnterSpecialModeTrap 2 }

        -- 1.3.6.1.4.1.2011.5.25.227.3
        hwFwdResTrapConformance OBJECT IDENTIFIER ::= { hwFwdResTrapMIB 3 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.3.1
        hwFwdResTrapCompliances OBJECT IDENTIFIER ::= { hwFwdResTrapConformance 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.3.1.1
        hwFwdResTrapCompliance MODULE-COMPLIANCE
            STATUS current
            DESCRIPTION 
                "Compliance statement for agents that provide full support for hwBaseTrapMIB."
            MODULE -- this module
                MANDATORY-GROUPS { hwFwdResObjectGroup }
            ::= { hwFwdResTrapCompliances 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.3.2
        hwFwdResTrapGroups OBJECT IDENTIFIER ::= { hwFwdResTrapConformance 2 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.3.2.1
        hwFwdResObjectGroup OBJECT-GROUP
            OBJECTS { hwEntPhysicalindex, hwFwdResLackSlotStr, hwFwdResLackReasonId, hwFwdResThreshold, hwL3FailedService, hwCommand, hwViewName, hwReasonDescription,hwFwdResLackVrId, hwFwdProcFailForLCSOperationId,hwFwdLicenseName, hwFwdResDevName, hwFwdResLimit, hwFwdResCurThroughput,hwFpId,hwFpResourceType,hwFpResourceCurrentCount,hwFpResourceTotalCount,
hwFpResourceThresholdUpperLimit,hwFpResourceThresholdLowerLimit,hwVpFeatureName,hwNoSuppVxlanFragVni,hwNoSuppVxlanFragSourceIp,hwNoSuppVxlanFragPeerIp,hwFwdResLackIPStr,hwFwdResLackVrfId, hwFwdResIncomReasonId, hwResOverwrittenSlot, hwResOverwrittenResType, hwFwdResCongestReasonId, hwFwdResLackFeNodeId, hwFwdSessionResUsage,hwEMDIInstanceId,hwEMDIIndicatorType,hwEMDIIndicatorValue,hwEMDIThreshold,hwAutoDiagnoseReasonId,hwFibDeliverSlotId,hwSysResChgSlotStr,hwSysResChgReasonId,hwSysResChgReasonDescription,hwSessThreshold,hwAclRuleResUsage,hwAclRuleThreshold,hwAclGroupResUsage,hwAclGroupThreshold,hwVxlanTnlPeerIpAddr,hwEMDISlotStr,hwEMDIResUsed,hwEMDIResTotal,hwPacketChangeInPort,hwPacketChangeOutPort ,hwSaidPingDetectInterface,hwNetStreamIPv4OriginalFlowUsage,hwNetStreamIPv4OriginalFlowThreshold,hwNetStreamIPv4FlexibleFlowUsage,hwNetStreamIPv4FlexibleFlowThreshold,TopNSourceIpAddress,hwSessionCurEntryNum,hwSessionLeakEntryNum,hwSessionUnrecEntryNum,hwSessionSpecification,hwSessionLeakUsage,hwSessionLeakThreshold,hwSessionUnrecUsage,hwSessionUnrecThreshold,hwMcastElbUsage,hwMcastElbThreshold,hwEnterModeReasonId,hwEnterModeId}
            STATUS current
            DESCRIPTION 
                "Group for base trap objects."
            ::= { hwFwdResTrapGroups 1 }
        
        -- 1.3.6.1.4.1.2011.5.25.227.3.2.2
        hwFwdResTrapGroup NOTIFICATION-GROUP
            NOTIFICATIONS { hwWholeFwdResLack, hwWholeFwdResLackResume, hwBoardFwdResLack, hwBoardFwdResLackResume, hwBoardL3FwdResLack, hwBoardL3FwdResLackResume, hwBoardL3ACLResLack,
            hwBoardL2mcResLack, hwBoardL2mcResLackResume, hwBoardIpmcResLack, hwBoardIpmcResLackResume, hwBoardServiceFailed, hwWholeFwdResThresholdExceed, 
            hwWholeFwdResThresholdExceedResume, hwBoardFwdResThresholdExceed, hwBoardFwdResThresholdExceedResume,hwBoardMplsPhpNonsupport,
            hwBoardResThresholdExceed,hwBoardResThresholdExceedResume,hwBoardResWarningThresholdExceed,hwBoardResWarningThresholdExceedResume,hwBoardIPv6ACLResLack,
            hwFwdProcFailForLCS, hwFwdProcFailForLCSResume,hwFwdEntryConflict,hwFwdEntryConflictResume, hwFwdResOverLimit, hwFwdResOverLimitResume, hwFwdResOverThresh, hwFwdResOverThreshResume,
            hwFpResourceThresholdExceed,hwFpResourceThresholdExceedClear,hwFpResourceTotalCountExceed,hwFpResourceTotalCountExceedClear, hwVpresExceed, hwBoardMplsNonSupport, hwBoardMplsFwdResLack, hwBoardMplsFwdResLackResume,
            hwFwdSessionResLack, hwFwdSessionResLackResume,hwFwdFastTableResLack, hwFwdFastTableResLackResume,hwNotsuppDecapVxlanFragPackets,hwBoardVbdifResLack,hwVxlanTnlCfgFailed,hwNotsuppDecapVxlanPackets,hwBoardL3NDResLack,hwBoardL3FIBResLack,
            hwFwdDataSyncIncomplete, hwFwdDataSyncIncompleteResume, hwResourceOverwrittenAlarm, hwResourceOverwrittenAlarmResume, 
hwBoardFwdMsgCongest, hwBoardFwdMsgCongestResume , hwBoardMplsFlowLabelNonSupp, hwTrunkWeightExceed, hwTrunkWeightExceedResume,hwSidResourceTotalCountExceed,hwSidResourceTotalCountExceedClear,hwSidResourceThresholdExceed,hwSidResourceThresholdExceedClear,hwBoardMcResFull,hwBoardMplsFwdResFull,hwBoardL3ResFull,hwEMDIIndicatorOverThreshold,hwEMDIIndicatorOverThresholdResume,hwEMDIReceiveDuplicatePackets,hwEMDIReceiveDuplicatePacketsResume,hwBoardMcResLack,hwBoardMcResLackResume, hwMcLeafCfcCheck, hwMcLeafCfcCheckResume,hwMplsLabelExceedAlarm,hwMplsLabelExceedAlarmResume,
hwAutoDiagnoseAlarm,hwAutoDiagnoseAlarmResume,hwEcmpMemberLimitOverThresholdAlarm,hwFibDeliverFailed,hwFibDeliverFailedResume,hwNsOrigFlexFlowExceedAlarm, hwNsOrigFlexFlowExceedResume, hwNsAggFlowExceedAlarm, hwNsAggFlowExceedResume,hwSysResChangedAlarm,hwSysResChangedAlarmResume,hwSessExceed,hwSessExceedClear,hwSessThresholdExceed,hwSessThresholdExceedClear,hwPingfFail,hwAclRuleExceed,hwAclRuleExceedClear,hwAclGroupExceed,hwAclGroupExceedClear,
hwBoardResCriticalThresholdExceed, hwBoardResCriticalThresholdExceedResume,hwNvo3VxlanSrcIpDiffAlarm,hwNvo3VxlanSrcIpDiffAlarmResume,hwEMDIResLack,hwEMDIResLackResume,hwPacketChange,hwPacketChangeClear,hwSaidPingPktModifiedAlarm,hwNetStreamIPv4OriginalFlowExceeded,hwNetStreamIPv4OriginalFlowFellBelow,hwNetStreamIPv4FlexibleFlowExceeded,hwNetStreamIPv4FlexibleFlowFellBelow,
            hwSessLeakEntryNumberThresholdExceed,hwSessLeakEntryNumberThresholdExceedClear,hwSessUnrecEntryNumberThresholdExceed,hwMcastElbExceed,hwMcastElbExceedClear,hwFesEnterSpecialMode,hwFesEnterSpecialModeResume}
            STATUS current
            DESCRIPTION 
                "Group for all base traps."
            ::= { hwFwdResTrapGroups 2 }


       -- 1.3.6.1.4.1.2011.5.25.227.2.1.24
       hwBoardMplsNonSupport NOTIFICATION-TYPE
          OBJECTS { hwFwdResLackSlotStr }
          STATUS current
          DESCRIPTION 
          "The board does not support the MPLS function due to hardware limit, it will be reset."
          ::= { hwFwdResLacTrap 24 }

       -- 1.3.6.1.4.1.2011.5.25.227.2.1.25
        hwBoardMplsFwdResLack NOTIFICATION-TYPE
        OBJECTS { hwEntPhysicalindex, hwFwdResLackSlotStr, hwFwdResLackReasonId, hwFwdResThreshold }
        STATUS current
        DESCRIPTION 
       "The MPLS forwarding engine resources were overloaded."
       ::= { hwFwdResLacTrap 25 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.26
      hwBoardMplsFwdResLackResume NOTIFICATION-TYPE
      OBJECTS { hwEntPhysicalindex, hwFwdResLackSlotStr, hwFwdResLackReasonId, hwFwdResThreshold }
      STATUS current
      DESCRIPTION 
     "The MPLS forwarding engine resources were resumed."
     ::= { hwFwdResLacTrap 26 }
      -- 1.3.6.1.4.1.2011.5.25.227.2.1.27
      hwFwdResOverLimit NOTIFICATION-TYPE
	OBJECTS { hwFwdResLimit, hwFwdResCurThroughput}
	STATUS current
	DESCRIPTION 
		"The current average system throughput exceeded the bandwidth configured for the license."
	::= { hwFwdResLacTrap 27 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.28
      hwFwdResOverLimitResume NOTIFICATION-TYPE
	OBJECTS { hwFwdResLimit, hwFwdResCurThroughput}
	STATUS current
	DESCRIPTION 
		"The current average system throughput decreased below the bandwidth configured for the license."
	::= { hwFwdResLacTrap 28 }
	
      -- 1.3.6.1.4.1.2011.5.25.227.2.1.29
      hwFwdResOverThresh NOTIFICATION-TYPE
	OBJECTS { hwFwdResLimit, hwFwdResCurThroughput}
	STATUS current
	DESCRIPTION 
		"The current average system throughput exceeded 95% of the bandwidth configured for the license."
	::= { hwFwdResLacTrap 29 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.30
      hwFwdResOverThreshResume NOTIFICATION-TYPE
	OBJECTS { hwFwdResLimit, hwFwdResCurThroughput}
	STATUS current
	DESCRIPTION 
		"The current average system throughput decreased below 95% of the bandwidth configured for the license"
	::= { hwFwdResLacTrap 30 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.31
      hwFpResourceThresholdExceed NOTIFICATION-TYPE
	OBJECTS {hwFpId, hwFpResourceType, hwFpResourceCurrentCount, hwFpResourceTotalCount,hwFpResourceThresholdUpperLimit,hwFpResourceThresholdLowerLimit}
	STATUS current
	DESCRIPTION 
		"This object indicates that the number of FP resources has exceeded the upper threshold."
	::= { hwFwdResLacTrap 31 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.32
      hwFpResourceThresholdExceedClear NOTIFICATION-TYPE
	OBJECTS {hwFpId, hwFpResourceType, hwFpResourceCurrentCount, hwFpResourceTotalCount,hwFpResourceThresholdUpperLimit,hwFpResourceThresholdLowerLimit}
	STATUS current
	DESCRIPTION 
		"This object indicates that the number of FP resources has fallen below the lower threshold."
	::= { hwFwdResLacTrap 32 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.33
      hwFpResourceTotalCountExceed NOTIFICATION-TYPE
	OBJECTS {hwFpId, hwFpResourceType, hwFpResourceCurrentCount, hwFpResourceTotalCount}
	STATUS current
	DESCRIPTION 
		"This object indicates that the number of FP resources has reached the maximum number."
	::= { hwFwdResLacTrap 33 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.34
      hwFpResourceTotalCountExceedClear NOTIFICATION-TYPE
	OBJECTS {hwFpId, hwFpResourceType, hwFpResourceCurrentCount, hwFpResourceTotalCount}
	STATUS current
	DESCRIPTION 
		"This object indicates that the number of FP resources fallen below the clear alarm threshold."
	::= { hwFwdResLacTrap 34 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.35
      hwVpresExceed NOTIFICATION-TYPE
      OBJECTS {hwVpFeatureName, hwFwdResLackSlotStr}
      STATUS current
      DESCRIPTION 
        "The number of Virtual Ports exceeded the specification of the forwarding engine resources."
    ::= { hwFwdResLacTrap 35 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.36
      hwFwdSessionResLack NOTIFICATION-TYPE
                     OBJECTS { hwFwdSessionResUsage }
                     STATUS current
                     DESCRIPTION
		"The device session resources were overloaded."
	::= { hwFwdResLacTrap 36 }

       -- 1.3.6.1.4.1.2011.5.25.227.2.1.37      
     hwFwdSessionResLackResume NOTIFICATION-TYPE
                   OBJECTS { hwFwdSessionResUsage }
                   STATUS current
	DESCRIPTION
		"The device session resources were resumed."
	::= { hwFwdResLacTrap 37 }


      -- 1.3.6.1.4.1.2011.5.25.227.2.1.38
      hwFwdFastTableResLack NOTIFICATION-TYPE
	STATUS current
	DESCRIPTION
		"The device fastforwarding table resources were overloadeds."
	::= { hwFwdResLacTrap 38 }


      -- 1.3.6.1.4.1.2011.5.25.227.2.1.39
      hwFwdFastTableResLackResume NOTIFICATION-TYPE
	STATUS current
	DESCRIPTION
	                      "The device fastforwarding table resources were resumed."
	::= { hwFwdResLacTrap 39 }


      -- 1.3.6.1.4.1.2011.5.25.227.2.1.40
      hwNotsuppDecapVxlanFragPackets NOTIFICATION-TYPE
	STATUS current
	DESCRIPTION
	    "The slot does not support decapsulate VXLAN fragments."
	::= { hwFwdResLacTrap 40 }


      -- 1.3.6.1.4.1.2011.5.25.227.2.1.41
      hwBoardVbdifResLack NOTIFICATION-TYPE
	STATUS current
	DESCRIPTION
	    "The current configuration of the number of VBDIF has exceeded the maximum number of this slot can support, which may cause traffic forwarding anomalies."
	::= { hwFwdResLacTrap 41 }


      -- 1.3.6.1.4.1.2011.5.25.227.2.1.42
      hwVxlanTnlCfgFailed NOTIFICATION-TYPE
	STATUS current
	DESCRIPTION
	    "Failed to add VXLAN tunnel table due to hash conflict."
	::= { hwFwdResLacTrap 42 } 

	  
      -- 1.3.6.1.4.1.2011.5.25.227.2.1.43
      hwNotsuppDecapVxlanPackets NOTIFICATION-TYPE
	STATUS current
	DESCRIPTION
	    "The slot does not support to decapsulate VXLAN packets."
	::= { hwFwdResLacTrap 43 }


      -- 1.3.6.1.4.1.2011.5.25.227.2.1.44
      hwBoardL3NDResLack NOTIFICATION-TYPE
                   OBJECTS { hwFwdResLackIPStr, hwFwdResLackVrfId, hwFwdResLackSlotStr }
	STATUS current
	DESCRIPTION
	    "This object indicates that fail to download ND entry because of Hash Collision."
	::= { hwFwdResLacTrap 44 }


      -- 1.3.6.1.4.1.2011.5.25.227.2.1.45
      hwBoardL3FIBResLack NOTIFICATION-TYPE
                   OBJECTS { hwFwdResLackIPStr, hwFwdResLackVrfId, hwFwdResLackSlotStr }
	STATUS current
	DESCRIPTION
	    "This object indicates that fail to download FIB entry because of LPM failure."
	::= { hwFwdResLacTrap 45 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.46
      hwBoardMplsFlowLabelNonSupp NOTIFICATION-TYPE
                   OBJECTS { hwFwdResLackSlotStr}
	STATUS current
	DESCRIPTION
	    "The board does not support MPLS flow label."
	::= { hwFwdResLacTrap 46 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.47
      hwTrunkWeightExceed NOTIFICATION-TYPE
          OBJECTS { hwEntPhysicalindex, entPhysicalName, hwFwdResLackSlotStr, hwFwdResLackReasonId }
          STATUS current
          DESCRIPTION 
              "The sum of all member interfaces' weights of a trunk interface exceeded the maximum value supported by the board."
          ::= { hwFwdResLacTrap 47 }
	 
      -- 1.3.6.1.4.1.2011.5.25.227.2.1.48
      hwTrunkWeightExceedResume NOTIFICATION-TYPE
          OBJECTS { hwEntPhysicalindex, entPhysicalName, hwFwdResLackSlotStr, hwFwdResLackReasonId }
          STATUS current
          DESCRIPTION 
              "The sum of all member interfaces' weights of each trunk interface is less than the maximum value supported by the board."
          ::= { hwFwdResLacTrap 48 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.49
      hwSidResourceThresholdExceed NOTIFICATION-TYPE
	OBJECTS {hwSIDPoolID, hwSIDResourceCurrentCount, hwSIDResourceTotalCount, hwSIDResourceThresholdUpperLimit, hwSIDResourceThresholdLowerLimit}
	STATUS current
	DESCRIPTION 
		"This object indicates that the number of SID pool has fallen below the upper threshol."
	::= { hwFwdResLacTrap 49 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.50
      hwSidResourceThresholdExceedClear NOTIFICATION-TYPE
	OBJECTS {hwSIDPoolID, hwSIDResourceCurrentCount, hwSIDResourceTotalCount, hwSIDResourceThresholdUpperLimit, hwSIDResourceThresholdLowerLimit}
	STATUS current
	DESCRIPTION 
		"This object indicates that the number of SID pool has fallen below the lower threshol."
	::= { hwFwdResLacTrap 50 }		  
	
      -- 1.3.6.1.4.1.2011.5.25.227.2.1.51
      hwSidResourceTotalCountExceed  NOTIFICATION-TYPE
	OBJECTS {hwSIDPoolID, hwSIDResourceCurrentCount, hwSIDResourceTotalCount}
	STATUS current
	DESCRIPTION 
		"This object indicates that the number of SID pool has reached the maximum number."
	::= { hwFwdResLacTrap 51 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.52
      hwSidResourceTotalCountExceedClear NOTIFICATION-TYPE
	OBJECTS {hwSIDPoolID, hwSIDResourceCurrentCount, hwSIDResourceTotalCount}
	STATUS current
	DESCRIPTION 
		"This object indicates that the number of SID pool fallen below the clear alarm threshold."
	::= { hwFwdResLacTrap 52 }			  

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.53
      hwBoardMcResFull NOTIFICATION-TYPE
                   OBJECTS {hwFwdResLackSlotStr, hwFwdResLackReasonId }
	STATUS current
	DESCRIPTION
	    "This object indicates that multicast resource is full."
	::= { hwFwdResLacTrap 53 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.54
      hwBoardMplsFwdResFull NOTIFICATION-TYPE
                   OBJECTS {hwFwdResLackSlotStr, hwFwdResLackReasonId }
	STATUS current
	DESCRIPTION
	    "This object indicates that MPLS resource is full."
	::= { hwFwdResLacTrap 54 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.55
      hwBoardL3ResFull NOTIFICATION-TYPE
                   OBJECTS {hwFwdResLackSlotStr, hwFwdResLackReasonId }
	STATUS current
	DESCRIPTION
	    "This object indicates that l3 resource is full."
	::= { hwFwdResLacTrap 55 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.56
      hwFwdComponentSmoothFailed NOTIFICATION-TYPE
                   OBJECTS { entPhysicalName, hwFwdResLackSlotStr, hwProducerComponentName, hwConsumerComponentName, hwSmoothFailedReasonId}
	STATUS current
	DESCRIPTION
	    "This object indicates that component smooth failed to finish."
	::= { hwFwdResLacTrap 56 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.57
      hwFwdComponentSmoothFailedClear NOTIFICATION-TYPE
                   OBJECTS { entPhysicalName, hwFwdResLackSlotStr, hwProducerComponentName, hwConsumerComponentName, hwSmoothFailedReasonId}
	STATUS current
	DESCRIPTION
	    "This object indicates that component smooth end."
	::= { hwFwdResLacTrap 57 }

    -- 1.3.6.1.4.1.2011.5.25.227.2.1.58
      hwEMDIIndicatorOverThreshold NOTIFICATION-TYPE
                   OBJECTS { hwEMDIInstanceId,hwEMDIIndicatorType,hwEMDIIndicatorValue,hwEMDIThreshold}
	STATUS current
	DESCRIPTION
	    "The monitor indicator exceeded the threshold."
	::= { hwFwdResLacTrap 58 }
    
    -- 1.3.6.1.4.1.2011.5.25.227.2.1.59
      hwEMDIIndicatorOverThresholdResume NOTIFICATION-TYPE
                   OBJECTS { hwEMDIInstanceId,hwEMDIIndicatorType,hwEMDIIndicatorValue,hwEMDIThreshold}
	STATUS current
	DESCRIPTION
	    "The monitor indicator exceeded trap resume."
	::= { hwFwdResLacTrap 59 }
    
    -- 1.3.6.1.4.1.2011.5.25.227.2.1.60
      hwEMDIReceiveDuplicatePackets NOTIFICATION-TYPE
                   OBJECTS { hwEMDIThreshold}
	STATUS current
	DESCRIPTION
	    "The device received duplicate packets."
	::= { hwFwdResLacTrap 60 }
    
    -- 1.3.6.1.4.1.2011.5.25.227.2.1.61
      hwEMDIReceiveDuplicatePacketsResume NOTIFICATION-TYPE
                   OBJECTS { hwEMDIThreshold}
	STATUS current
	DESCRIPTION
	    "The device didn't received duplicate packets."
	::= { hwFwdResLacTrap 61 }
    -- 1.3.6.1.4.1.2011.5.25.227.2.1.62
      hwBoardMcResLack NOTIFICATION-TYPE
                   OBJECTS { hwFwdResThreshold, hwFwdResLackSlotStr, hwFwdResLackReasonId}
	STATUS current
	DESCRIPTION
	    "This object indicates that multicast entry resources were overloaded."
	::= { hwFwdResLacTrap 62 }
    -- 1.3.6.1.4.1.2011.5.25.227.2.1.63
      hwBoardMcResLackResume NOTIFICATION-TYPE
                   OBJECTS { hwFwdResThreshold, hwFwdResLackSlotStr, hwFwdResLackReasonId}
	STATUS current
	DESCRIPTION
	    "This object indicates that multicast entry resources were resumed."
	::= { hwFwdResLacTrap 63 }

       -- 1.3.6.1.4.1.2011.5.25.227.2.1.64
        hwAutoDiagnoseAlarm NOTIFICATION-TYPE
            OBJECTS {hwAutoDiagnoseReasonId, hwReasonDescription}
            STATUS current
            DESCRIPTION 
                        "The AutoDiagnose system detects that the device is faulty."
            ::= { hwFwdResLacTrap 64}
            
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.65
        hwAutoDiagnoseAlarmResume NOTIFICATION-TYPE
            OBJECTS {hwAutoDiagnoseReasonId, hwReasonDescription}
            STATUS current
            DESCRIPTION 
                        "The AutoDiagnose system detects that the faulty device recovers."
            ::= { hwFwdResLacTrap 65 }	

        -- 1.3.6.1.4.1.2011.5.25.227.2.1.66
        hwEcmpMemberLimitOverThresholdAlarm NOTIFICATION-TYPE
            OBJECTS {hwFwdResLackSlotStr}
            STATUS current
            DESCRIPTION 
                        "The number of next hops to which routes recurse exceeds the device capability. During route convergence, load balancing may fail on some links."
            ::= { hwFwdResLacTrap 66}

        -- 1.3.6.1.4.1.2011.5.25.227.2.1.67
        hwSysResChangedAlarm NOTIFICATION-TYPE
            OBJECTS { hwSysResChgSlotStr, hwSysResChgReasonId, hwSysResChgReasonDescription }
            STATUS current
            DESCRIPTION 
                        "The mode of forwarding resourecs was changed."
            ::= { hwFwdResLacTrap 67 }
            
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.68
        hwSysResChangedAlarmResume NOTIFICATION-TYPE
            OBJECTS { hwSysResChgSlotStr, hwSysResChgReasonId, hwSysResChgReasonDescription }
            STATUS current
            DESCRIPTION 
                        "The mode of forwarding resourecs was resumed."
            ::= { hwFwdResLacTrap 68 }

     -- 1.3.6.1.4.1.2011.5.25.227.2.1.69
		hwSessExceed NOTIFICATION-TYPE
			OBJECTS { hwFwdSessionResUsage, hwSessThreshold,TopNSourceIpAddress }
			STATUS current
			DESCRIPTION
				"The number of session resources exceeds the limit."
		::= { hwFwdResLacTrap 69 }

     -- 1.3.6.1.4.1.2011.5.25.227.2.1.70
		hwSessExceedClear NOTIFICATION-TYPE
			OBJECTS { hwFwdSessionResUsage, hwSessThreshold }
			STATUS current
			DESCRIPTION
				"The number of session resources falls below the limit."
		::= { hwFwdResLacTrap 70 }

	 -- 1.3.6.1.4.1.2011.5.25.227.2.1.71
		hwSessThresholdExceed NOTIFICATION-TYPE
			OBJECTS { hwFwdSessionResUsage, hwSessThreshold,TopNSourceIpAddress }
			STATUS current
			DESCRIPTION
				"The number of session resources exceeds the threshold."
		::= { hwFwdResLacTrap 71 }

     -- 1.3.6.1.4.1.2011.5.25.227.2.1.72
		hwSessThresholdExceedClear NOTIFICATION-TYPE
			OBJECTS { hwFwdSessionResUsage, hwSessThreshold }
			STATUS current
			DESCRIPTION
				" The number of session resources falls below the threshold."
		::= { hwFwdResLacTrap 72 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.73
              hwPingfFail NOTIFICATION-TYPE
	           STATUS current
	           DESCRIPTION
	                   "This object indicates that pingf fail."
              ::= { hwFwdResLacTrap 73 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.74
              hwAclRuleExceed NOTIFICATION-TYPE
              OBJECTS { hwAclRuleResUsage, hwAclRuleThreshold }
	           STATUS current
	           DESCRIPTION
	                   "The number of acl rule resource is full."
              ::= { hwFwdResLacTrap 74 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.75
              hwAclRuleExceedClear NOTIFICATION-TYPE
              OBJECTS { hwAclRuleResUsage, hwAclRuleThreshold }
	           STATUS current
	           DESCRIPTION
	                   "The number of acl rule resource falls below the threshold."
              ::= { hwFwdResLacTrap 75 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.76
              hwAclGroupExceed NOTIFICATION-TYPE
              OBJECTS { hwAclGroupResUsage, hwAclGroupThreshold }
	           STATUS current
	           DESCRIPTION
	                   "The number of acl group resource is full."
              ::= { hwFwdResLacTrap 76 }

      -- 1.3.6.1.4.1.2011.5.25.227.2.1.77
              hwAclGroupExceedClear NOTIFICATION-TYPE
              OBJECTS { hwAclGroupResUsage, hwAclGroupThreshold }
	           STATUS current
	           DESCRIPTION
	                   "The number of acl group resource falls below the threshold."
              ::= { hwFwdResLacTrap 77 }

        -- 1.3.6.1.4.1.2011.5.25.227.2.1.78
        hwBoardResCriticalThresholdExceed NOTIFICATION-TYPE
            OBJECTS { hwFwdResLackSlotStr, hwFwdResThreshold, hwFwdResLackReasonId , hwReasonDescription}
            STATUS current
            DESCRIPTION 
                        "The number of forwarding resources reaches the alarm threshold."
            ::= { hwFwdResLacTrap 78 }
            
        -- 1.3.6.1.4.1.2011.5.25.227.2.1.79
        hwBoardResCriticalThresholdExceedResume NOTIFICATION-TYPE
            OBJECTS { hwFwdResLackSlotStr,hwFwdResThreshold, hwFwdResLackReasonId , hwReasonDescription }
            STATUS current
            DESCRIPTION 
                        "The number of forwarding engine resources is less than the threshold."
            ::= { hwFwdResLacTrap 79 }

       -- 1.3.6.1.4.1.2011.5.25.227.2.1.80
        hwEMDIResLack NOTIFICATION-TYPE
            OBJECTS { hwEMDIThreshold,hwEMDISlotStr, hwEMDIResUsed, hwEMDIResTotal}
            STATUS current
            DESCRIPTION 
                        "The number of emdi resources reaches the alarm threshold.."
            ::= { hwFwdResLacTrap 80 }

       -- 1.3.6.1.4.1.2011.5.25.227.2.1.81
        hwEMDIResLackResume NOTIFICATION-TYPE
            OBJECTS { hwEMDIThreshold,hwEMDISlotStr, hwEMDIResUsed, hwEMDIResTotal}
            STATUS current
            DESCRIPTION 
                        "The number of emdi resources is less than the threshold."
            ::= { hwFwdResLacTrap 81 }
       -- 1.3.6.1.4.1.2011.5.25.227.2.1.82
        hwSaidPingPktModifiedAlarm NOTIFICATION-TYPE
            OBJECTS { hwSaidPingDetectInterface}
            STATUS current
            DESCRIPTION 
                        "The SAID PING function detected that the packet modification."
            ::= { hwFwdResLacTrap 82 }
			
	   -- 1.3.6.1.4.1.2011.5.25.227.2.1.83
       hwNetStreamIPv4OriginalFlowExceeded NOTIFICATION-TYPE
              OBJECTS { hwNetStreamIPv4OriginalFlowUsage, hwNetStreamIPv4OriginalFlowThreshold }
	           STATUS current
	           DESCRIPTION
	                   "The number of used NetStream IPv4 original flows exceeded the threshold."
              ::= { hwFwdResLacTrap 83 }

	   -- 1.3.6.1.4.1.2011.5.25.227.2.1.84
       hwNetStreamIPv4OriginalFlowFellBelow NOTIFICATION-TYPE
              OBJECTS { hwNetStreamIPv4OriginalFlowUsage, hwNetStreamIPv4OriginalFlowThreshold }
	           STATUS current
	           DESCRIPTION
	                   "The number of used NetStream IPv4 original flows fell below the threshold."
              ::= { hwFwdResLacTrap 84 }
			  
       -- 1.3.6.1.4.1.2011.5.25.227.2.1.85
       hwNetStreamIPv4FlexibleFlowExceeded NOTIFICATION-TYPE
              OBJECTS { hwNetStreamIPv4FlexibleFlowUsage, hwNetStreamIPv4FlexibleFlowThreshold }
	           STATUS current
	           DESCRIPTION
	                   "The number of used NetStream IPv4 flexible flows exceeded the threshold."
              ::= { hwFwdResLacTrap 85 }

	   -- 1.3.6.1.4.1.2011.5.25.227.2.1.86
       hwNetStreamIPv4FlexibleFlowFellBelow NOTIFICATION-TYPE
              OBJECTS { hwNetStreamIPv4FlexibleFlowUsage, hwNetStreamIPv4FlexibleFlowThreshold }
	           STATUS current
	           DESCRIPTION
	                   "The number of used NetStream IPv4 flexible flows fell below the threshold."
              ::= { hwFwdResLacTrap 86 }

          -- 1.3.6.1.4.1.2011.5.25.227.2.1.87
        hwFwmFaultAlarm NOTIFICATION-TYPE
            OBJECTS { hwFwmFaultSlotStr, hwFwmFaultCpuStr, hwFwmFaultReasonId, hwFwmFaultReasonDescription }
            STATUS current
            DESCRIPTION 
                        "This object indicates that a forwarding manage module encounters a partial failure."
            ::= { hwFwdResLacTrap 87 }
           
          -- 1.3.6.1.4.1.2011.5.25.227.2.1.88
        hwFwmFaultAlarmResume NOTIFICATION-TYPE
            OBJECTS { hwFwmFaultSlotStr, hwFwmFaultCpuStr, hwFwmFaultReasonId, hwFwmFaultReasonDescription }
            STATUS current
            DESCRIPTION 
                        "This object indicates that a forwarding manage module recovers from a partial failure."
            ::= { hwFwdResLacTrap 88 }

          -- 1.3.6.1.4.1.2011.5.25.227.2.1.89
        hwBoardNetworkSliceResourceInsufficient NOTIFICATION-TYPE
            OBJECTS { hwFwmSliceSlotStr, hwFwmSliceInterfaceName, hwFwmSliceId, hwFwmSliceTrunkInterfaceName, hwFwmSliceResourceReasonId, hwFwmSliceReasonDescription }
            STATUS current
            DESCRIPTION 
                        "This object indicates that the service specifications configured for the system exceeded those of the forwarding engine."
            ::= { hwFwdResLacTrap 89 }

          -- 1.3.6.1.4.1.2011.5.25.227.2.1.90
        hwBoardNetworkSliceResourceInsufficientResume NOTIFICATION-TYPE
            OBJECTS { hwFwmSliceSlotStr, hwFwmSliceInterfaceName, hwFwmSliceId, hwFwmSliceTrunkInterfaceName, hwFwmSliceResourceReasonId, hwFwmSliceReasonDescription }
            STATUS current
            DESCRIPTION 
                        "This object indicates that the service specifications configured for the system do not exceed those of the forwarding engine."
            ::= { hwFwdResLacTrap 90 }

          -- 1.3.6.1.4.1.2011.5.25.227.2.1.91
        hwBoardNetworkSliceTrafficAbnormal NOTIFICATION-TYPE
            OBJECTS { hwFwmSliceSlotStr, hwFwmSliceInterfaceName, hwFwmSliceId, hwFwmSliceTrunkInterfaceName, hwFwmSliceSrcInterfaceName, hwFwmSliceFwdReasonId, hwFwmSliceReasonDescription }
            STATUS current
            DESCRIPTION 
                        "This object indicates that the service configured for the system is wrong."
            ::= { hwFwdResLacTrap 91 }

          -- 1.3.6.1.4.1.2011.5.25.227.2.1.92
        hwBoardNetworkSliceTrafficAbnormalResume NOTIFICATION-TYPE
            OBJECTS { hwFwmSliceSlotStr, hwFwmSliceInterfaceName, hwFwmSliceId, hwFwmSliceTrunkInterfaceName, hwFwmSliceSrcInterfaceName, hwFwmSliceFwdReasonId, hwFwmSliceReasonDescription }
            STATUS current
            DESCRIPTION 
                        "This object indicates that the service configured for the system has been configured correctly."
            ::= { hwFwdResLacTrap 92 }

          -- 1.3.6.1.4.1.2011.5.25.227.2.1.93
        hwSessLeakEntryNumberThresholdExceed NOTIFICATION-TYPE
            OBJECTS { hwSessionCurEntryNum, hwSessionLeakEntryNum, hwSessionUnrecEntryNum, hwSessionSpecification, hwSessionLeakUsage, hwSessionLeakThreshold }
	    STATUS current
	    DESCRIPTION
	                "The number of session leak entries exceeds the threshold."
            ::= { hwFwdResLacTrap 93 }

          -- 1.3.6.1.4.1.2011.5.25.227.2.1.94
        hwSessLeakEntryNumberThresholdExceedClear NOTIFICATION-TYPE
            OBJECTS { hwSessionCurEntryNum, hwSessionLeakEntryNum, hwSessionUnrecEntryNum, hwSessionSpecification, hwSessionLeakUsage, hwSessionLeakThreshold }
	    STATUS current
            DESCRIPTION
	                "The number of session leak entries fell below the threshold."
            ::= { hwFwdResLacTrap 94 }

          -- 1.3.6.1.4.1.2011.5.25.227.2.1.95
        hwSessUnrecEntryNumberThresholdExceed NOTIFICATION-TYPE
            OBJECTS { hwSessionCurEntryNum, hwSessionLeakEntryNum, hwSessionUnrecEntryNum, hwSessionSpecification, hwSessionUnrecUsage, hwSessionUnrecThreshold }
	    STATUS current
            DESCRIPTION
	                "The number of session unrecoverable entries exceeds the threshold."
            ::= { hwFwdResLacTrap 95 }
			
		  -- 1.3.6.1.4.1.2011.5.25.227.2.1.96
        hwVlanSrcExeedAlarm NOTIFICATION-TYPE
            OBJECTS { hwL2mcGrpAddress, hwL2mcVlanIdx}
            STATUS current
            DESCRIPTION 
                        "The number of multicast sources of a multicast group reaches the alarm threshold."
            ::= { hwFwdResLacTrap 96 }
			
		  -- 1.3.6.1.4.1.2011.5.25.227.2.1.97
        hwVlanSrcExeedResume NOTIFICATION-TYPE
            OBJECTS { hwL2mcGrpAddress, hwL2mcVlanIdx}
            STATUS current
            DESCRIPTION 
                        "The number of multicast sources of a multicast group is less than the threshold."
            ::= { hwFwdResLacTrap 97 }

                  -- 1.3.6.1.4.1.2011.5.25.227.2.1.98
              hwMcastElbExceed NOTIFICATION-TYPE
              OBJECTS { hwMcastElbUsage, hwMcastElbThreshold }
	           STATUS current
	           DESCRIPTION
	                   "The number of multicast egress interfaces resource is full."
              ::= { hwFwdResLacTrap 98 }

                 -- 1.3.6.1.4.1.2011.5.25.227.2.1.99
              hwMcastElbExceedClear NOTIFICATION-TYPE
              OBJECTS { hwMcastElbUsage, hwMcastElbThreshold }
	           STATUS current
	           DESCRIPTION
	                   "The number of multicast egress interfaces resource falls below the threshold."
              ::= { hwFwdResLacTrap 99 }

                -- 1.3.6.1.4.1.2011.5.25.227.2.1.100
              hwFwdTblmScanHndOverload NOTIFICATION-TYPE
              OBJECTS { hwEntiyPhysicalindex,hwEntPhysicalindex, entPhysicalName, hwFwdTableId, hwFwdTableName }
	           STATUS current
	           DESCRIPTION
	                   "The number of handles traversed in the forwarding resource table exceeded the maximum number supported."
              ::= { hwFwdResLacTrap 100 }

                -- 1.3.6.1.4.1.2011.5.25.227.2.1.101
              hwFwdTblmScanHndThresholdExceed NOTIFICATION-TYPE
              OBJECTS { hwEntiyPhysicalindex,hwEntPhysicalindex, entPhysicalName, hwFwdTableId, hwFwdTableName }
	           STATUS current
	           DESCRIPTION
	                   "The number of handles traversed in the forwarding resource table exceeded the threshold."
              ::= { hwFwdResLacTrap 101 }
			  
                -- 1.3.6.1.4.1.2011.5.25.227.2.1.102
              hwFwdTblmScanHndOverloadClear NOTIFICATION-TYPE
              OBJECTS { hwEntiyPhysicalindex,hwEntPhysicalindex, entPhysicalName, hwFwdTableId, hwFwdTableName }
	           STATUS current
	           DESCRIPTION
	                   "The number of handles traversed in the forwarding resource table is less than the maximum number supported."
              ::= { hwFwdResLacTrap 102 }

                -- 1.3.6.1.4.1.2011.5.25.227.2.1.103
              hwFwdTblmScanHndThresholdExceedClear NOTIFICATION-TYPE
              OBJECTS { hwEntiyPhysicalindex,hwEntPhysicalindex, entPhysicalName, hwFwdTableId, hwFwdTableName }
	           STATUS current
	           DESCRIPTION
	                   "The number of handles traversed in the forwarding resource table is less than the threshold."
              ::= { hwFwdResLacTrap 103 }

                -- 1.3.6.1.4.1.2011.5.25.227.2.1.104
              hwCapwapNoFragmentAlarm NOTIFICATION-TYPE
              OBJECTS { hwFwdResLackSlotStr }
	           STATUS current
	           DESCRIPTION
	                   "There is too much wireless traffic, and some packets cannot be fragmented."
              ::= { hwFwdResLacTrap 104 }

                -- 1.3.6.1.4.1.2011.5.25.227.2.1.105
              hwCapwapDiscardBroadcastAlarm NOTIFICATION-TYPE
              OBJECTS { hwFwdResLackSlotStr }
	           STATUS current
	           DESCRIPTION
	                   "There is too much wireless traffic, and some packets cannot be broadcast."
              ::= { hwFwdResLacTrap 105 }

                -- 1.3.6.1.4.1.2011.5.25.227.2.1.106
              hwBoardNetworkSliceConflict NOTIFICATION-TYPE
             OBJECTS { hwFwmSliceSlotStr, hwFwmSliceInterfaceName, hwFwmSliceId, hwFwmSliceTrunkInterfaceName, hwFwmSliceConflitReasonId, hwFwmSliceReasonDescription }
	           STATUS current
	           DESCRIPTION
	                   "The slice configuration conflicted with other configurations."
              ::= { hwFwdResLacTrap 106 }

                -- 1.3.6.1.4.1.2011.5.25.227.2.1.107
              hwBoardNetworkSliceConflictResume NOTIFICATION-TYPE
              OBJECTS { hwFwmSliceSlotStr, hwFwmSliceInterfaceName, hwFwmSliceId, hwFwmSliceTrunkInterfaceName, hwFwmSliceConflitReasonId, hwFwmSliceReasonDescription }
	           STATUS current
	           DESCRIPTION
	                   "The conflicting slice configuration was deleted."
              ::= { hwFwdResLacTrap 107 }

    END
--
-- HUAWEI-FWD-RES-TRAP-MIB.mib
--
