
-- ==================================================================
-- Copyright (C) 2023 by  HUAWEI TECHNOLOGIES. All rights reserved.
-- Description: This mib which contains objects manages the 
--              SSH server and SSH client configuration. 
-- Reference:  
-- Version: V2.50
-- ==================================================================
-- ==================================================================
-- 
-- Varibles and types are imported
--
-- ==================================================================
    HUAWEI-SSH-MIB DEFINITIONS ::= BEGIN
 
        IMPORTS
            hwDatacomm          
                FROM HUAWEI-MIB         
               OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP         
                FROM SNMPv2-CONF            
            Integer32, Unsigned32, OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE          
                FROM SNMPv2-SMI         
            RowStatus, DisplayString            
                FROM SNMPv2-TC;

        -- 1.3.6.1.4.1.2011.5.25.118
            hwSSH MODULE-IDENTITY 
            LAST-UPDATED "202306010000Z"         
            ORGANIZATION "Huawei Technologies Co.,Ltd."
            CONTACT-INFO                                        
                         "Huawei Industrial Base                
                          Bantian, Longgang                     
                          Shenzhen 518129                       
                          People's Republic of China            
                          Website: http://www.huawei.com        
                          Email: support@huawei.com             
                         "                                      
            DESCRIPTION 
                "This mib which contains objects manages the 
                SSH server and SSH client configuration. 
                "   
--  Revision history
            REVISION    "202306010000Z"
            DESCRIPTION "V2.50, modify dataType for hwEd25519PublicKeyEncodingType ."

            REVISION    "202305250000Z"
            DESCRIPTION "V2.49, add enum for hwEd25519PublicKeyEncodingType ."

            REVISION    "202305100000Z"
            DESCRIPTION "V2.48, add hwEd25519LocalKeyTable and hwEd25519PublicKeyTable ."

            REVISION    "202304100000Z"
            DESCRIPTION "V2.47, add enum keyType ed25519 for hwSftpServerPublicKeyType."

            REVISION    "202301040000Z"
            DESCRIPTION "V2.46, add enum keyTypeX509V3RSA2048SHA256 for hwSSHSessionKeyType ."

            REVISION    "202208110000Z"
            DESCRIPTION "V2.45, delete sensitive information from seninfo."

            REVISION    "202112270000Z"
            DESCRIPTION "V2.44, modify hwSSHServerTimeOut to 1,300."

            REVISION    "202112080000Z"
            DESCRIPTION "V2.43, modify hwSSHUserAuthType."

            REVISION    "202110300000Z"
            DESCRIPTION "V2.42, modify hwSSHUserAssignKeyType, hwSSHSessionKeyType."
     
            REVISION    "202110130000Z"
            DESCRIPTION "V2.41, modify hwSSHUserAuthType."

            REVISION    "202110110000Z"
            DESCRIPTION "V2.40, modify hwSSHClientPublicKeyAlg."            

            REVISION    "202108260000Z"
            DESCRIPTION "V2.37, modify hwSSHServerTimeOut."
            
            REVISION    "202106240000Z"
            DESCRIPTION "V2.38, add x509rsa2048sha256, ed25519."

            REVISION    "202106200000Z"
            DESCRIPTION "V2.37, modify hwRSAPublicKeyCode, hwRSALocalHostPublicKeyCode, hwRSALocalServerPublicKeyCode."
            
            REVISION    "202105280000Z"
            DESCRIPTION "V2.36, modify hwSSHServerCipherAlg, hwSSHClientCipherAlg."

            REVISION    "202103310000Z"
            DESCRIPTION "V2.35, modify hwSSHServerKeyExchangeAlg, hwSSHClientKeyExchangeAlg."

            REVISION    "202101180000Z"
            DESCRIPTION "V2.34, modify hwSSHServerPublicKeyAlg."

            REVISION    "202011230000Z"
            DESCRIPTION "V2.33, add hwSSHServerAlg, hwSSHServerCipherAlg, hwSSHServerHmacAlg, 
                         hwSSHServerKeyExchangeAlg, hwSSHServerDhMinLen, hwSSHServerPublicKeyAlg,
                         hwSSHClientAlg, hwSSHClientCipherAlg, hwSSHClientHmacAlg, hwSSHClientKeyExchangeAlg,
                         hwSSHClientPublicKeyAlg .
                         modify hwSSHServerTimeOut."

            REVISION    "202007140000Z"
            DESCRIPTION "V2.32, modify hwSftpServerName ."
            
            REVISION    "202007100000Z"
            DESCRIPTION "V2.31, modify hwSSHSessionKeyType ."

            REVISION    "202006130000Z"
            DESCRIPTION "V2.30, Add hwSftpClient."

            REVISION    "201912040000Z"
            DESCRIPTION "V2.29, Add alarm."
            
            REVISION    "201905230000Z"
            DESCRIPTION "V2.28, modify hwSSHUserTable."

            REVISION    "201905230000Z"
            DESCRIPTION "V2.27, Add X509V3RSA, X509V3RSAandPASSWORD key authentication."

            REVISION    "201902280000Z"
            DESCRIPTION "V2.26, the description of hwSSHUserTable, hwSSHServerSessionTable, hwRSAPublicKeyTable, hwSSHServerInfoTable,
						hwSSHUserAuthType,hwSSHUserServiceType were modified and supplemented."			
			
            REVISION    "201808040000Z"
            DESCRIPTION "V2.25, modify hwRSAPublicKeyName range 1..40 "

            REVISION    "201807110000Z"
            DESCRIPTION "V2.24, add SM2 key authentication"

            REVISION    "201806070000Z"
            DESCRIPTION "V2.23, modify hwSNetConfMaxUserNum range 0..20 "

            REVISION    "201711220000Z"
            DESCRIPTION "V2.22, delete index of hwRSAPublicKeyTable;" 

            REVISION    "201711100000Z"
            DESCRIPTION "V2.21, modify  hwSSHServerInfoTable    OID:1.3.6.1.4.1.2011.5.25.118.2.2;" 

             REVISION    "201708230000Z"
             DESCRIPTION "V2.20, delete index of hwSSHServerSessionTable." 

            REVISION    "201708170000Z"
            DESCRIPTION "V2.19, 
                          1.modify hwStelnetServerEnable               OID:1.3.6.1.4.1.2011.5.25.118.1.1;
                          2.modify hwSftpServerEnable                    OID:1.3.6.1.4.1.2011.5.25.118.1.2;
                          3.modify hwSNetConfServerEnable         OID:1.3.6.1.4.1.2011.5.25.118.1.15;
                          4.modify hwStelnetIPv4ServerEnable       OID:1.3.6.1.4.1.2011.5.25.118.1.21;
                          5.modify hwStelnetIPv6ServerEnable       OID:1.3.6.1.4.1.2011.5.25.118.1.22;
                          6.modify hwSftpIPv4ServerEnable             OID:1.3.6.1.4.1.2011.5.25.118.1.23;
                          7.modify hwSftpIPv6ServerEnable             OID:1.3.6.1.4.1.2011.5.25.118.1.24;
                          8.modify hwSCPIPv4ServerEnable            OID:1.3.6.1.4.1.2011.5.25.118.1.25;
                          9.modify hwSCPIPv6ServerEnable            OID:1.3.6.1.4.1.2011.5.25.118.1.26;
                          10.modify hwSNetConfIPv4ServerEnable         OID:1.3.6.1.4.1.2011.5.25.118.1.27;
                          11.modify hwSNetConfIPv6ServerEnable         OID:1.3.6.1.4.1.2011.5.25.118.1.28;
                          12.modify hwSSHFirstTimeAuthEnable            OID:1.3.6.1.4.1.2011.5.25.118.2.1;
                          13.modify hwSSHUserName                              OID:1.3.6.1.4.1.2011.5.25.118.1.11.1.2;"

             REVISION    "201705170000Z"
             DESCRIPTION "V2.18, Modify the type of mib-node according to the field type in DOM" 

             REVISION    "201703140000Z"
             DESCRIPTION "V2.17, 
                         1.Add hwSNetConfIPv4ServerEnable          OID:1.3.6.1.4.1.2011.5.25.118.1.27;
                         2.Add hwSNetConfIPv6ServerEnable          OID:1.3.6.1.4.1.2011.5.25.118.1.28;" 

             REVISION    "201701240000Z"
             DESCRIPTION "V2.16, 
                           1.Add hwSSHIPv4ServerPort                OID:1.3.6.1.4.1.2011.5.25.118.1.19;
                           2.Add hwSSHIPv6ServerPort                OID:1.3.6.1.4.1.2011.5.25.118.1.20;
                           3.Add hwStelnetIPv4ServerEnable        OID:1.3.6.1.4.1.2011.5.25.118.1.21;
                           4.Add hwStelnetIPv6ServerEnable        OID:1.3.6.1.4.1.2011.5.25.118.1.22;
                           5.Add hwSftpIPv4ServerEnable             OID:1.3.6.1.4.1.2011.5.25.118.1.23;
                           6.Add hwSftpIPv6ServerEnable             OID:1.3.6.1.4.1.2011.5.25.118.1.24;
                           7.Add hwSCPIPv4ServerEnable            OID:1.3.6.1.4.1.2011.5.25.118.1.25;
                          8.Add hwSCPIPv6ServerEnable            OID:1.3.6.1.4.1.2011.5.25.118.1.26."

             REVISION    "201409260000Z"
             DESCRIPTION "V2.15, default value in the description is updated."


             REVISION    "201406300000Z"
             DESCRIPTION "V2.14, 
                          1. Modify the value range of the node hwSSHServerTimeOut, hwSSHServerPort,hwSftpMaxUserNum,
                             hwSftpOnLineUserNum,hwSSHUserName,hwSSHUserSftpDirectory,hwSSHServerName,hwSSHServerAssignKey.
                          2. Modify the description of the node hwSSHServerTimeOut,hwSSHServerPort,hwSftpMaxUserNum,hwSSHUserName,
                             hwSSHUserAuthorizationCMD,hwSSHSftpUserNumExceedMax.
                          3. Add the following enums of the hwSSHUserAuthType:authDSA(6),authDSAandPASSWORD(7),authAny(8),authECC(9),
                             authECCandPASSWORD(10).
                          4. Add the following enums of the hwSSHUserServiceType:servicetypeSNetConf(5),servicetypeSftpSNetConf(6),
                             servicetypeSTelnetSftp(7),servicetypeSTelnetSNetConf(8).
                          5. Add the following enums of the hwSSHSessionConnectType:none(0),vty15(16),vty16(17),vty17(18),vty18(19),
                             vty19(20),vty20(21).
                          6. modified 'MAX-ACCESS read-only' to 'MAX-ACCESS read-write' of hwSftpMaxUserNum.
                          7. Add hwSSHUserAssignKeyType in hwSSHUserTable.
                          8. Add hwSSHSessionKeyType, hwSSHSessionConnectionIndex, hwSSHSessionCtosCompress, hwSSHSessionStocCompress 
                             in hwSSHServerSessionTable.
                          9. Add hwSNetConfMaxUserNum, hwSNetConfServerEnable, hwSSHKeepAliveEnable, hwSCPServerEnable, hwSCPMaxUserNum
                             in hwSSHServer.
                          10. Add hwSSHServerAssignDSAKey and hwSSHServerAssignECCKey in hwSSHServerInfoTable.
                          11. Add hwSSHKeepAliveInterval and hwSSHKeepAliveMaxCount in hwSSHClient.
                         "

             REVISION    "201405060000Z"
             DESCRIPTION "V1.08, 
                          1. Add hwRSAPublicKeyFingerprint in hwRSAPublicKeyTable.
                          2. Add hwRSALocalKeyTable."
 
             REVISION    "201011090000Z"
             DESCRIPTION "V1.07, The description of this MIB is modified according to the tool."
             
             REVISION    "201008250000Z"
             DESCRIPTION "V1.06, modified the contact-info and the revision history. Modified the description of leaves."
             
             REVISION    "201006170000Z"
             DESCRIPTION "V1.05, the description of hwSSHServerTimeOut, hwSSHServerPort, hwSSHServerKeyTimeOut, hwSSHUserTable, 
                          hwSSHUserEntry, hwSSHUserAuthType and hwSSHUserServiceType were modified and supplemented." 

             REVISION    "201004180000Z"
             DESCRIPTION "V1.04, DT requirements were implemented and the syntax and semantics of SIMPLETEST were changed." 
                          
             REVISION    "201003030000Z"
             DESCRIPTION "V1.03, DT requirements were implemented and the syntax and semantics of SIMPLETEST were changed."
            
             REVISION    "201001290000Z"        
             DESCRIPTION "V1.02, hwRSAPublicKeyTable was added."  
                
             REVISION    "200609050000Z"
             DESCRIPTION "V1.00, completed the draft."
            ::= { hwDatacomm 118}

--
-- Node definitions
--
    
--  Node definitions
-- 
-- ==================================================================
-- 
-- ======================= definition begin =========================
-- 
-- ==================================================================       
        -- 1.3.6.1.4.1.2011.5.25.118.1
        hwSSHServer OBJECT IDENTIFIER ::= { hwSSH 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.1
        hwStelnetServerEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                The object specifies whether the SSH stelnet server is enable.
                Options:
               1. enable(1) -The SSH stelnet server is enable.
               2. disable(2)-The SSH stelnet server is disable.
               The default value is disable.
                "
            ::= { hwSSHServer 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.2
        hwSftpServerEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                The object specifies whether the sftp server is enable. 
                Options:
                1.enable(1) -the sftp server is enable.
                2.disable(2)-the sftp server is disable.
                The default value is disable.
                "
            -- DEFVAL { 2 }
            ::= { hwSSHServer 2 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.3
        hwSSHServerComp1x OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                The object specifies whether the SSH server is compatible with SSH1.x.
                The default is 2.
                Options:
                1. enable(1) -indicates that the version compatibility function of the SSH server is enabled 
                              so that the SSH server is compatible with the SSHv1.x client.
                2. disable(2)-indicates that the version compatibility function of the SSH server is disabled 
                              and therefore the SSH server is incompatible with the SSHv1.x client.
                "
            ::= { hwSSHServer 3 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.4
        hwSSHServerTimeOut OBJECT-TYPE
            SYNTAX Integer32 (1..300)
            UNITS      "second"       
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies the time when SSH authentication times out.
                The unit is the second and the default is 60 seconds."
            ::= { hwSSHServer 4 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.5
        hwSSHServerRetry OBJECT-TYPE
            SYNTAX Integer32 (1..5)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                The object specifies authentication-retry times for SSH user. 
                Default: 3
                "
            ::= { hwSSHServer 5 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.6
        hwSSHServerPort OBJECT-TYPE
            SYNTAX Integer32 (22 | 1025..65535)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies port number for SSH server supporting.
                The default value is 22."
            ::= { hwSSHServer 6 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.7
        hwSSHServerKeyTimeOut OBJECT-TYPE
            SYNTAX Integer32 (0..24)
            UNITS "hour"
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                The interval of updating the SSH server key pair.    
                By default, value is 0 hour, which means server key can't be updated forever.
                Range: 0-24
                Unit: hour
                "
            ::= { hwSSHServer 7 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.8
        hwSSHServerAlarmEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                The object specifies whether send trap information to NMS.
                Options:
                1.enable(1) -Only when its value enable, allowed to send trap informations to NMS.
                2.disable(2)-Can not to send trap informations to NMS.
                "
            ::= { hwSSHServer 8 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.9
        hwSftpMaxUserNum OBJECT-TYPE
            SYNTAX Integer32 (0..15)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies the max number of sftp user that sftp server supporting.
                The default is 5."
            ::= { hwSSHServer 9 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.10
        hwSftpOnLineUserNum OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the number of sftp user that has been connected to sftp server currently.
                "
            ::= { hwSSHServer 10 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.11
        hwSSHUserTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwSSHUserEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                This table is used for querying and setting the information about SSH user.
                "
            ::= { hwSSHServer 11 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.11.1
        hwSSHUserEntry OBJECT-TYPE
            SYNTAX HwSSHUserEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                This table is used for querying and setting the information about SSH user.
                The index of this entry is hwSSHUserIndex.                 
                "
            INDEX { hwSSHUserIndex }
            ::= { hwSSHUserTable 1 }

        
        HwSSHUserEntry ::=
            SEQUENCE { 
                hwSSHUserIndex
                    Integer32,
                hwSSHUserName
                    OCTET STRING,
                hwSSHUserAssignKey
                    OCTET STRING,
                hwSSHUserAuthType
                    INTEGER,
                hwSSHUserServiceType
                    INTEGER,
                hwSSHUserSftpDirectory
                    OCTET STRING,
                hwSSHUserAuthorizationCMD
                    INTEGER,
                hwSSHUserRowStatus
                    RowStatus,
                hwSSHUserAssignKeyType
                    INTEGER
                }

        -- 1.3.6.1.4.1.2011.5.25.118.1.11.1.1
        hwSSHUserIndex OBJECT-TYPE
            SYNTAX Integer32 (1..200)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                The object specifies the index of hwSSHUserTable.
                "
            ::= { hwSSHUserEntry 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.11.1.2
        hwSSHUserName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..255))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The object specifies the name of a SSH user. The maximum length of the node is 255."
            ::= { hwSSHUserEntry 2 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.11.1.3
        hwSSHUserAssignKey OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..64))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "
                The object specifies is a peer public key for a SSH user.
                This peer public key on the SSH server must exist and associate with hwRSAPublicKeyName.
                "
            ::= { hwSSHUserEntry 3 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.11.1.4
        hwSSHUserAuthType OBJECT-TYPE
            SYNTAX INTEGER
                {
                authNULL(1),
                authPASSWORD(2),
                authRSA(3),
                authRSAorPASSWORDorED25519(4),
                authRSAandPASSWORD(5),
                authDSA(6),
                authDSAandPASSWORD(7),
                authAny(8),
                authECC(9),
                authECCandPASSWORD(10),
                authSM2(11),
                authSM2andPASSWORD(12),
                authX509V3RSA(13),
                authX509V3RSAandPASSWORD(14),
                authED25519(15),
                authED25519andPASSWORD(16)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "
                The object specifies the authentication type of SSH user.
                The default authentication type is authPASSWORD.
                Options: 
                1. authNULL(1)           -No authenticate.
                2. authPASSWORD(2)       -Password authentication.
                3. authRSA(3)            -RSA key authentication.
                4. authRSAorPASSWORDorED25519(4)  -Password or RSA key or ED25519 key authentication.
                5. authRSAandPASSWORD(5) -Password and RSA key authentication.
                6. authDSA(6)           -DSA key authentication.
                7. authDSAandPASSWORD(7) -Password or DSA key authentication.
                8. authAny(8)            -Any  authentication.
                9. authECC(9)            -ECC key authentication.
                10.authECCandPASSWORD(10) -Password and ECC key authentication.
				11.authSM2(11)			  -SM2 key authentication.
				12.authSM2andPASSWORD(12) -Password and SM2 key authentication.
                13. authX509V3RSA(13)            -X509V3RSA key authentication.
                14. authX509V3RSAandPASSWORD(14)  -Password and X509V3RSA key authentication.
                15. authED25519(15)             -ED25519 key authentication.
                16. authED25519andPASSWORD(16)  -Password and ED25519 key authentication.
                "
            DEFVAL { authPASSWORD }
            ::= { hwSSHUserEntry 4 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.11.1.5
        hwSSHUserServiceType OBJECT-TYPE
            SYNTAX INTEGER
                {
                servicetypeNULL(1),
                servicetypeSTELNET(2),
                servicetypeSFTP(3),
                servicetypeALL(4),
                servicetypeSNetConf(5),
                servicetypeSftpSNetConf(6),
                servicetypeSTelnetSftp(7),
                servicetypeSTelnetSNetConf(8)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "
                The object specifies the service type of SSH user. 
                Options: 
                1. servicetypeNULL(1)    -default service type.
                2. servicetypeSTELNET(2) -The service type of the SSH user is STELNET.
                3. servicetypeSFTP(3)    -The service type of the SSH user is SFTP.
                4. servicetypeALL(4)     -The service type of the SSH user is all. 
                5. servicetypeSNetConf(5)       -The service type of the SSH user is SNetConf.
                6. servicetypeSftpSNetConf(6)    -The service type of the SSH user is Sftp and SNetConf.
                7. servicetypeSTelnetSftp(7)     -The service type of the SSH user is STelnet and Sftp.
                8. servicetypeSTelnetSNetConf(8) -The service type of the SSH user is STelnet and SNetConf.
				"
            DEFVAL { servicetypeNULL }
            ::= { hwSSHUserEntry 5 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.11.1.6
        hwSSHUserSftpDirectory OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..255))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The object specifies the working directory for the sftp user. 
                The total length of absolute path is 128,the length of single directory is 128."
            ::= { hwSSHUserEntry 6 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.11.1.7
        hwSSHUserAuthorizationCMD OBJECT-TYPE
            SYNTAX INTEGER
                {
                authorizationNULL(1),
                authorizationAAA(2)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "
                The object specifies the authorization type of SSH user. When authorizationAAA is specified,
                the SSH user will be authorizated by HWTACACS server. The default authorization is authorizationNULL,
                indicating SSH user doesn't need to be authorizated by HWTACACS server.
                Options:
                1.authorizationNULL(1)-The default authorization is authorizationNULL,indicating SSH user 
                                       doesn't need to be authorizated by HWTACACS server.
                2.authorizationAAA(2) -When authorizationAAA is specified,the SSH user will be 
                                       authorizated by HWTACACS server. 
                "
            DEFVAL { authorizationNULL }
            ::= { hwSSHUserEntry 7 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.11.1.8
        hwSSHUserRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "
                The object specifies the status of this entry.
                When the status is active(1), hwSSHUserAssignKey, hwSSHUserAuthType, 
                hwSSHUserServiceType, hwSSHUserSftpDirectory, and hwSSHUserAuthorizationCMD's 
                value in the entry are allowed to be modified.
                "
            ::= { hwSSHUserEntry 8 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.11.1.9
        hwSSHUserAssignKeyType OBJECT-TYPE
            SYNTAX INTEGER
                {
                keyTypeNULL(0),
                keyTypeRSA(1),
                keyTypeDSA(2),
                keyTypeECC(3),
                keyTypeSM2(5), 
                keyTypePKI(6),
                keyTypeED25519(7)
                }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The object specifies the public key type of SSH user.
				Options:
				1. keyTypeNULL(0) -The public key type of SSH user is NULL.
				2. keyTypeRSA(1)-The public key type of SSH user is RSA.
				3. keyTypeDSA(2)-The public key type of SSH user is DSA
				4. keyTypeECC(3)-The public key type of SSH user is ECC
				5. keyTypeSM2(5)-The public key type of SSH user is SM2
				6. keyTypePKI(6)-The public key type of SSH user is PKI.
				7.keyTypeED25519(7)-The public key type os SSH user is ED25519.
				"
            ::= { hwSSHUserEntry 9 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12
        hwSSHServerSessionTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwSSHServerSessionEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                The object shows current session information of the SSH server which includes username,
                version information, retry times of online users currently.
                "
            ::= { hwSSHServer 12 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1
        hwSSHServerSessionEntry OBJECT-TYPE
            SYNTAX HwSSHServerSessionEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                The object shows current session information of the SSH server which includes username,
                version information, retry times of online users currently.
                The index of this entry is hwSSHSessionIndex.                
                "
            INDEX { hwSSHSessionIndex }
            ::= { hwSSHServerSessionTable 1 }

        
        HwSSHServerSessionEntry ::=
            SEQUENCE { 
                hwSSHSessionIndex
                    Integer32,
                hwSSHSessionUserName
                    DisplayString,
                hwSSHSessionConnectType
                    INTEGER,
                hwSSHSessionVer
                    DisplayString,
                hwSSHSessionState
                    INTEGER,
                hwSSHSessionRetry
                    Integer32,
                hwSSHSessionCtosCipher
                    DisplayString,
                hwSSHSessionStocCipher
                    DisplayString,
                hwSSHSessionCtosHmac
                    DisplayString,
                hwSSHSessionStocHmac
                    DisplayString,
                hwSSHSessionKex
                    DisplayString,
                hwSSHSessionAuthType
                    DisplayString,
                hwSSHSessionServiceType
                    DisplayString,
                hwSSHSessionKeyType
                    INTEGER,
                hwSSHSessionConnectionIndex
                    Integer32,
                hwSSHSessionCtosCompress
                    DisplayString,
                hwSSHSessionStocCompress
                    DisplayString
                }

        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.1
        hwSSHSessionIndex OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                The object specifies the index of hwSSHServerSessionTable.
                "
            ::= { hwSSHServerSessionEntry 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.2
        hwSSHSessionUserName OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the name of a SSH user,
                which has started a session.
                "
            ::= { hwSSHServerSessionEntry 2 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.3
        hwSSHSessionConnectType OBJECT-TYPE
            SYNTAX INTEGER
                {
                none(0),
                vty0(1),
                vty1(2),
                vty2(3),
                vty3(4),
                vty4(5),
                vty5(6),
                vty6(7),
                vty7(8),
                vty8(9),
                vty9(10),
                vty10(11),
                vty11(12),
                vty12(13),
                vty13(14),
                vty14(15),
                vty15(16),
                vty16(17),
                vty17(18),
                vty18(19),
                vty19(20),
                vty20(21)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the line number supports a connection of SSH 
                user which is in connection with SSH server.
				Options:
				1.none(0) -No specifies the line number.
				2.vty0(1) -The line number is 1.
				3.vty1(2) -The line number is 2.
				4.vty2(3) -The line number is 3.
				5.vty3(4) -The line number is 4.
				6.vty4(5) -The line number is 5.
				7.vty5(6) -The line number is 6.
				8.vty6(7) -The line number is 7.
				9.vty7(8) -The line number is 8.
				10.vty8(9) -The line number is 9.
				11.vty9(10) -The line number is 10.
				12.vty10(11) -The line number is 11.
				13.vty11(12) -The line number is 12.
				14.vty12(13) -The line number is 13.
				15.vty13(14) -The line number is 14.
				16.vty14(15) -The line number is 15.
				17.vty15(16) -The line number is 16.
				18.vty16(17) -The line number is 17.
				19.vty17(18) -The line number is 18.
				20.vty18(19) -The line number is 19.
				21.vty19(20) -The line number is 20.
				22.vty20(21) -The line number is 21.	
                "
            ::= { hwSSHServerSessionEntry 3 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.4
        hwSSHSessionVer OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the version information of a SSH 
                user which is in connection with SSH server.
                "
            ::= { hwSSHServerSessionEntry 4 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.5
        hwSSHSessionState OBJECT-TYPE
            SYNTAX INTEGER { started(1) }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the state of a SSH user 
                which is in connection with SSH server.
                Options:
                1.started(1)-indicates the state is start.
                "
            ::= { hwSSHServerSessionEntry 5 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.6
        hwSSHSessionRetry OBJECT-TYPE
            SYNTAX Integer32 (0..5)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies SSH user's retrying times in authentications.
                "
            ::= { hwSSHServerSessionEntry 6 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.7
        hwSSHSessionCtosCipher OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the cipher of custom to server.
                "
            ::= { hwSSHServerSessionEntry 7 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.8
        hwSSHSessionStocCipher OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the cipher of server to custom.
                "
            ::= { hwSSHServerSessionEntry 8 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.9
        hwSSHSessionCtosHmac OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the hmac of custom to server.
                "
            ::= { hwSSHServerSessionEntry 9 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.10
        hwSSHSessionStocHmac OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the hmac of server to custom.
                "
            ::= { hwSSHServerSessionEntry 10 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.11
        hwSSHSessionKex OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the key exchange.
                "
            ::= { hwSSHServerSessionEntry 11 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.12
        hwSSHSessionAuthType OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the authentication type of SSH session.
                "
            ::= { hwSSHServerSessionEntry 12 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.13
        hwSSHSessionServiceType OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the service type of SSH session.
                "
            ::= { hwSSHServerSessionEntry 13 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.14
        hwSSHSessionKeyType OBJECT-TYPE
            SYNTAX INTEGER
                {
                keyTypeRSA(1),
                keyTypeDSA(2),
                keyTypeECC(3),
                keyTypeSM2(5),
                keyTypePKI(6),
                keyTypeRSASHA256(7),
                keyTypeRSASHA512(8),
                keyTypeED25519(9),
                keyTypeX509V3RSA2048SHA256(10)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The object specifies the public key type of SSH session.
				Options:
				1.keyTypeRSA(1) -The public key type of SSH session is RSA.
				2.keyTypeDSA(2) -The public key type of SSH session is DSA.
				3.keyTypeECC(3) -The public key type of SSH session is ECC.
				4.keyTypeSM2(5) -The public key type of SSH session is SM2.
				5.keyTypePKI(6) -The public key type of SSH session is PKI.
				6.keyTypeRSASHA256(7) -The public key type of SSH session is RSA_SHA2_256.
				7.keyTypeRSASHA512(8) -The public key type of SSH session is RSA_SHA2_512.
				8.keyTypeED25519(9) -The public key type of SSH session is ED25519.
                                9.keyTypeX509V3RSA2048SHA256(10) - The public key type of SSH session is X509V3_RSA2048_SHA25.
				"
            ::= { hwSSHServerSessionEntry 14 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.15
        hwSSHSessionConnectionIndex OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The object specifies the line number supports a connection of SSH user which is in connection with SSH(STelnet/Sftp/SNetConf) server."
            ::= { hwSSHServerSessionEntry 15 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.16
        hwSSHSessionCtosCompress OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The object specifies the Compression algorithm of SSH client to server."
            ::= { hwSSHServerSessionEntry 16 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.12.1.17
        hwSSHSessionStocCompress OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The object specifies the Compression algorithm of SSH Server to client."
            ::= { hwSSHServerSessionEntry 17 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.13
        hwRSAPublicKeyTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwRSAPublicKeyEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                A table of configuration about RSA Public Key.
                hwRSAPublicKeyName is the name of RSA Public Key.              
                "
            ::= { hwSSHServer 13 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.13.1
        hwRSAPublicKeyEntry OBJECT-TYPE
            SYNTAX HwRSAPublicKeyEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                A table of configuration about RSA Public Key.
                The index of this entry is hwRSAPublicKeyName.  
                hwRSAPublicKeyName is the name of RSA Public Key.
                "
            INDEX { hwRSAPublicKeyName }
            ::= { hwRSAPublicKeyTable 1 }

        
        HwRSAPublicKeyEntry ::=
            SEQUENCE { 
                hwRSAPublicKeyName
                    OCTET STRING,
                hwRSAPublicKeyCode
                    OCTET STRING,
                hwRSAPublicKeyRowStatus
                    RowStatus,
                hwRSAPublicKeyFingerprint
                    OCTET STRING
             }

        -- 1.3.6.1.4.1.2011.5.25.118.1.13.1.1
        hwRSAPublicKeyName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..40))
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                The object specifies the name of RSA Public Key.
                "
            ::= { hwRSAPublicKeyEntry 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.13.1.2
        hwRSAPublicKeyCode OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..4096))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "
                The object specifies is RSA Public Key Code that in the format of der, the maximum length of the node is 4096.             
                When the RSA public key is created, the index value is the name of the public key, which uses the ASCII code.
                The public key value must be generated through a tool. Firstly, use the PUTTYGEN.EXE tool to generate the matching 
                public key and private key. Then, use the sshkey.exe tool to convert the generated public key to the required public key value.
                "
            ::= { hwRSAPublicKeyEntry 2 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.13.1.3
        hwRSAPublicKeyRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "
                The object specifies the status of this table entry.
                When the status is active(1), hwRSAPublicKeyName, hwRSAPublicKeyCode's
                value in the entry are allowed to be modified.  
                createAndGo(4) is supplied to create a new instance of a conceptual row.
                destroy(6) is supplied to delete the instances associated with an existing conceptual row.        
                "
            ::= { hwRSAPublicKeyEntry 3 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.13.1.4
        hwRSAPublicKeyFingerprint OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..60))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the fingerprint of RSA Public Key Code,
                that including the public key algorithm, length and fingerprint.
                "
            ::= { hwRSAPublicKeyEntry 4 }

        -- 1.3.6.1.4.1.2011.5.25.118.1.14
        hwSNetConfMaxUserNum OBJECT-TYPE
            SYNTAX Integer32 (0..20)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies the max number of SNetConf user that SNetConf Server supporting.
                The default is 5."
            ::= { hwSSHServer 14 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.15
        hwSNetConfServerEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies whether the SSH SNetConf Server is enable.
				Options:
                1. enable(1) -The SSH SNetConf Server is enable.
                2. disable(2)-The SSH SNetConf Server is disable.					
                The default is disable(2).
				"
            ::= { hwSSHServer 15 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.16
        hwSSHKeepAliveEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies whether the KeepAlive functionality on SSH Server is enable.
				Options:
                1. enable(1) -The KeepAlive functionality on SSH Server is enable.
                2. disable(2)-The KeepAlive functionality on SSH Server is disable.			
                The default is 1.
				"
            ::= { hwSSHServer 16 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.17
        hwSCPServerEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies whether the SSH SCP Server is enable.
				Options:
                1. enable(1) -The SSH  SCP server is enable.
                2. disable(2)-The SSH  SCP server is disable.				
                The default is 2.
				"
            ::= { hwSSHServer 17 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.18
        hwSCPMaxUserNum OBJECT-TYPE
            SYNTAX Integer32 (0..5)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies the max number of SCP user that SCP Server supporting.
                The default is 2."
            ::= { hwSSHServer 18 }

        -- 1.3.6.1.4.1.2011.5.25.118.1.19
        hwSSHIPv4ServerPort OBJECT-TYPE
            SYNTAX Unsigned32 (22 | 1025..65535)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies port number for SSH IPv4 server supporting.
                The default value is 22."
            ::= { hwSSHServer 19 }
            
            
        -- 1.3.6.1.4.1.2011.5.25.118.1.20
        hwSSHIPv6ServerPort OBJECT-TYPE
            SYNTAX Unsigned32 (22 | 1025..65535)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies port number for SSH IPv6 server supporting.
                The default value is 22."
            ::= { hwSSHServer 20 }
            
            
        -- 1.3.6.1.4.1.2011.5.25.118.1.21
        hwStelnetIPv4ServerEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                The object specifies whether the SSH stelnet IPv4 server is enable.
                Options:
                1. enable(1) -The SSH stelnet IPv4 server is enable.
                2. disable(2)-The SSH stelnet IPv4 server is disable.
                The default value is disable.
                "
            ::= { hwSSHServer 21 }
            
            
        -- 1.3.6.1.4.1.2011.5.25.118.1.22
        hwStelnetIPv6ServerEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                The object specifies whether the SSH stelnet IPv6 server is enable.
                Options:
                1. enable(1) -The stelnet IPv6 server is enable.
                2. disable(2)-The stelnet IPv6 server is disable.
                The default value is disable.
                "
            ::= { hwSSHServer 22 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.23
        hwSftpIPv4ServerEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                The object specifies whether the sftp IPv4 server is enable.
                Options:
                1.enable(1) -The sftp IPv4 server is enable
                2.disable(2)-The sftp IPv4 server is disable.
                The default value is disable.
                "
            ::= { hwSSHServer 23 }
            
            
        -- 1.3.6.1.4.1.2011.5.25.118.1.24
        hwSftpIPv6ServerEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                The object specifies whether the sftp IPv6 server is enable.
                Options:
                1.enable(1) -the sftp IPv6 server is enable.
                2.disable(2)-the sftp IPv6 server is disable.
                The default value is disable.
                "
            ::= { hwSSHServer 24 }
            
            
        -- 1.3.6.1.4.1.2011.5.25.118.1.25
        hwSCPIPv4ServerEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies whether the SCP IPv4 Server is enable.
				Options:
                1.enable(1) -the SCP IPv4 Server is enable.
                2.disable(2)-the SCP IPv4 Server is disable.				
                The default value is disable.
				"
            ::= { hwSSHServer 25 }
            
            
        -- 1.3.6.1.4.1.2011.5.25.118.1.26
        hwSCPIPv6ServerEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies whether the SCP IPv6 Server is enable.
				Options:
                1.enable(1) -the SCP IPv6 Server is enable.
                2.disable(2)-the SCP IPv6 Server is disable.
                The default value is disable."
            ::= { hwSSHServer 26 }


         -- 1.3.6.1.4.1.2011.5.25.118.1.27
         hwSNetConfIPv4ServerEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                The object specifies whether the SSH SNetConf IPv4 server is enable.
                Options:
                1.enable(1) -the SSH SNetConf IPv4 server is enable.
                2.disable(2)-the SSH SNetConf IPv4 server is disable.
                The default value is disable.
                "
            ::= { hwSSHServer 27 }

        
         -- 1.3.6.1.4.1.2011.5.25.118.1.28
         hwSNetConfIPv6ServerEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                The object specifies whether the SSH SNetConf IPv6 server is enable.
                Options:
                1. enable(1) -The SSH SNetConf IPv6 server is enable.
                2. disable(2)-The SSH SNetConf IPv6 server is disable.
                The default value is disable.
                "
            ::= { hwSSHServer 28 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.2
        hwSSHClient OBJECT IDENTIFIER ::= { hwSSH 2 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.2.1
        hwSSHFirstTimeAuthEnable OBJECT-TYPE
            SYNTAX INTEGER
                {
                enable(1),
                disable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies whether the SSH client
                supports first-time-authentication.
                Options:
                1.enable(1) -indicates the SSH client supports first-time-authentication.
                2.disable(2)-indicates the SSH client does not support first-time-authentication.
                The default value is disable.
                "
            ::= { hwSSHClient 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.2.2
        hwSSHServerInfoTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwSSHServerInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                A table of configuration about the relation
                between the SSH server and the rsa peerkey.
                "
            ::= { hwSSHClient 2 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.2.2.1
        hwSSHServerInfoEntry OBJECT-TYPE
            SYNTAX HwSSHServerInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                A table of configuration about the relation
                between the SSH server and the rsa peerkey.
                The index of this entry is hwSSHServerIndex.
                "
            INDEX { hwSSHServerIndex }
            ::= { hwSSHServerInfoTable 1 }

        
        HwSSHServerInfoEntry ::=
            SEQUENCE { 
                hwSSHServerIndex
                    Integer32,
                hwSSHServerName
                    OCTET STRING,
                hwSSHServerAssignKey
                    OCTET STRING,
                hwSSHServerRowStatus
                    RowStatus,
                hwSSHServerAssignDSAKey
                    OCTET STRING,
                hwSSHServerAssignECCKey
                    OCTET STRING,
                hwSSHServerAssignSM2Key
                    OCTET STRING
             }

        -- 1.3.6.1.4.1.2011.5.25.118.2.2.1.1
        hwSSHServerIndex OBJECT-TYPE
            SYNTAX Integer32 (1..20)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                The object specifies the index of hwSSHServerInfoTable.
                "
            ::= { hwSSHServerInfoEntry 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.2.2.1.2
        hwSSHServerName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..255))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "
                The object specifies the name of a SSH server.
                "
            ::= { hwSSHServerInfoEntry 2 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.2.2.1.3
        hwSSHServerAssignKey OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..64))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "
                The object specifies a peer public key for a 
                SSH server. This peer public key must exist.
                "
            ::= { hwSSHServerInfoEntry 3 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.2.2.1.4
        hwSSHServerRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "
                The object specifies the status of this entry.
                When the status is active,  
                hwSSHServerAssignKey's value in the entry is 
                allowed to be modified.
                "
            ::= { hwSSHServerInfoEntry 4 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.2.2.1.5
        hwSSHServerAssignDSAKey OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..64))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The object specifies a DSA peer public key for a SSH server.This peer public key must exist."
            ::= { hwSSHServerInfoEntry 5 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.2.2.1.6
        hwSSHServerAssignECCKey OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..64))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The object specifies a ECC peer public key for a SSH server.This peer public key must exist."
            ::= { hwSSHServerInfoEntry 6 }

        -- 1.3.6.1.4.1.2011.5.25.118.2.2.1.7
        hwSSHServerAssignSM2Key OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..64))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The object specifies a SM2 peer public key for a SSH server.This peer public key must exist."
            ::= { hwSSHServerInfoEntry 7 }
			
        -- 1.3.6.1.4.1.2011.5.25.118.2.3
        hwSSHKeepAliveInterval OBJECT-TYPE
            SYNTAX Integer32 (0..3600)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies KeepAlive Timeout interval on SSH Client.
                The default is 0. 0 specify no KeepAlive packet should be sent to Server."
            ::= { hwSSHClient 3 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.2.4
        hwSSHKeepAliveMaxCount OBJECT-TYPE
            SYNTAX Integer32 (1..30)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies maximum KeepAlive packet to send to SSH Server before disconnect.
                The default is 3."
            ::= { hwSSHClient 4 }
        
        -- 1.3.6.1.4.1.2011.5.25.118.1.29
        hwSSHServerInsecureAlgo OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..255))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The insecure algorithm list."
            ::= { hwSSHServer 29 }
        
        hwSSHServerAlg OBJECT IDENTIFIER ::= { hwSSHServer 30 }

        hwSSHServerCipherAlg OBJECT-TYPE
            SYNTAX BITS
            {
                des3cbc(0),
                arcfour128(1),
                arcfour256(2),
                blowfishcbc(3),
                aes128cbc(4),
                aes192cbc(5),
                aes256cbc(6),
                aes128ctr(7),
                aes192ctr(8),
                aes256ctr(9),
                aes128gcm(10),
                aes256gcm(11),
				chacha20poly1305(12)
            }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                List of the SSH server cipher algorithm.
                Through this list, the index can be configured in batches in the format of bit-domain string.
                It can be configured as follows: to configure the index n, set the nth in the bit string to 1, 
                that is,......000100......For example, to configure the index 1, set the first character of 
                the string to 1, and issue 0100 0000, namely, # 0x40 (note that the value of the bit type 
                starts from 0). For example, to configure the index 8, set the eighth character of the string 
                to 1, and issue 0000 0000 1000 0000, namely, # 0x00 0x80.
                "
            ::= { hwSSHServerAlg 1 }

        hwSSHServerHmacAlg OBJECT-TYPE
            SYNTAX BITS
            {
                hmacmd5(0),
                hmacmd596(1),
                hmacsha1(2),
                hmacsha196(3),
                hmacsha2256(4),
                hmacsha225696(5),
                hmacsha2512(6)
            }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                List of the SSH server hmac algorithm.
                Through this list, the index can be configured in batches in the format of bit-domain string.
                "
            ::= { hwSSHServerAlg 2 }

        hwSSHServerKeyExchangeAlg OBJECT-TYPE
            SYNTAX BITS
            {
                dhGroup1Sha1(0),
                dhGroup14Sha1(1),
                dhGroupExchangeSha1(2),
                dhGroupExchangeSha256(3),
                ecdhSha2Nistp256(4),
                ecdhSha2Nistp384(5),
                ecdhSha2Nistp521(6),
                sm2KepSha2Nistp256(7),
                curve25519Sha256(8)
            }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                List of the SSH server key exchange algorithm.
                Through this list, the index can be configured in batches in the format of bit-domain string.
                "
            ::= { hwSSHServerAlg 3 }

        hwSSHServerDhMinLen OBJECT-TYPE
            SYNTAX INTEGER
            {
                modulus1024(1),
                modulus2048(2),
                modulus3072(3),
                modulus4096(4)
            }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                This object indicates the length of DH.
                Options:
                1.modulus1024(1),
                2.modulus2048(2),
                3.modulus3072(3),
                4.modulus4096(4).
                "
            ::= { hwSSHServerAlg 4 }

        hwSSHServerPublicKeyAlg OBJECT-TYPE
            SYNTAX BITS
            {
                rsa(0),
                rsasha2256(1),
                rsasha2512(2),
                x509rsa(3),
                x509rsa2048sha256(4),
                ed25519(5)
            }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                List of the SSH server public key algorithm.
                Through this list, the index can be configured in batches in the format of bit-domain string.
                "
            ::= { hwSSHServerAlg 5 }

        -- 1.3.6.1.4.1.2011.5.25.118.2.5
        hwSSHClientInsecureAlgo OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..255))
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The insecure algorithm list."
            ::= { hwSSHClient 5 }

        hwSSHClientAlg OBJECT IDENTIFIER ::= { hwSSHClient 6 }

        hwSSHClientCipherAlg OBJECT-TYPE
            SYNTAX BITS
            {
                des3cbc(0),
                arcfour128(1),
                arcfour256(2),
                blowfishcbc(3),
                aes128cbc(4),
                aes192cbc(5),
                aes256cbc(6),
                aes128ctr(7),
                aes192ctr(8),
                aes256ctr(9),
                aes128gcm(10),
                aes256gcm(11),
				chacha20poly1305(12)
            }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                List of the SSH client cipher algorithm. However, the blowfishcbc algorithm is not supported.
                Through this list, the index can be configured in batches in the format of bit-domain string.
                It can be configured as follows: to configure the index n, set the nth in the bit string to 1, 
                that is,......000100......For example, to configure the index 1, set the first character of 
                the string to 1, and issue 0100 0000, namely, # 0x40 (note that the value of the bit type 
                starts from 0). For example, to configure the index 8, set the eighth character of the string 
                to 1, and issue 0000 0000 1000 0000, namely, # 0x00 0x80.
                "
            ::= { hwSSHClientAlg 1 }

        hwSSHClientHmacAlg OBJECT-TYPE
            SYNTAX BITS
            {
                hmacmd5(0),
                hmacmd596(1),
                hmacsha1(2),
                hmacsha196(3),
                hmacsha2256(4),
                hmacsha225696(5),
                hmacsha2512(6)
            }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                List of the SSH client hmac algorithm.
                Through this list, the index can be configured in batches in the format of bit-domain string.
                "
            ::= { hwSSHClientAlg 2 }

        hwSSHClientKeyExchangeAlg OBJECT-TYPE
            SYNTAX BITS
            {
                dhGroup1Sha1(0),
                dhGroup14Sha1(1),
                dhGroupExchangeSha1(2),
                dhGroupExchangeSha256(3),
                ecdhSha2Nistp256(4),
                ecdhSha2Nistp384(5),
                ecdhSha2Nistp521(6),
                sm2KepSha2Nistp256(7),
                curve25519Sha256(8)
            }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                List of the SSH client key exchange algorithm.
                Through this list, the index can be configured in batches in the format of bit-domain string.
                "
            ::= { hwSSHClientAlg 3 }

        hwSSHClientPublicKeyAlg OBJECT-TYPE
            SYNTAX BITS
            {
                rsa(0),
                rsasha2256(1),
                rsasha2512(2),
                ed25519(3)
            }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                List of the SSH client public key algorithm.
                Through this list, the index can be configured in batches in the format of bit-domain string.
                "
            ::= { hwSSHClientAlg 4 }
        
        -- 1.3.6.1.4.1.2011.5.25.118.3
        hwSSHNotifications OBJECT IDENTIFIER ::= { hwSSH 3 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.3.1
        hwSSHSftpUserNumExceedMax NOTIFICATION-TYPE
            OBJECTS { hwSftpOnLineUserNum, hwSftpMaxUserNum }
            STATUS current
            DESCRIPTION 
                "This notification was sent when the total number of sftp users requesting sftp service
                exceeds max user number configured."
            ::= { hwSSHNotifications 1 }
            
        -- 1.3.6.1.4.1.2011.5.25.118.3.2
        hwSSHServerUsedInsecureAlgo NOTIFICATION-TYPE
            OBJECTS { hwSSHServerInsecureAlgo }
            STATUS current
            DESCRIPTION 
                "This notification was sent when the insecure algorithm was configured for the SSH server."
            ::= { hwSSHNotifications 2 }
        
        -- 1.3.6.1.4.1.2011.5.25.118.3.3
        hwSSHClientUsedInsecureAlgo NOTIFICATION-TYPE
            OBJECTS { hwSSHClientInsecureAlgo }
            STATUS current
            DESCRIPTION 
                "This notification was sent when the insecure algorithm was configured for the SSH client."
            ::= { hwSSHNotifications 3 }
        -- 1.3.6.1.4.1.2011.5.25.118.3.4
        hwSSHServerUsedInsecureAlgoClear NOTIFICATION-TYPE
            OBJECTS { hwSSHServerInsecureAlgo }
            STATUS current
            DESCRIPTION 
                "This notification was sent when the insecure algorithm was configured for the SSH server."
            ::= { hwSSHNotifications 4 }
        
        -- 1.3.6.1.4.1.2011.5.25.118.3.3
        hwSSHClientUsedInsecureAlgoClear NOTIFICATION-TYPE
            OBJECTS { hwSSHClientInsecureAlgo }
            STATUS current
            DESCRIPTION 
                "This notification was sent when the insecure algorithm was configured for the SSH client."
            ::= { hwSSHNotifications 5 }    
--    Conformance information
        -- 1.3.6.1.4.1.2011.5.25.118.4
        hwSSHMIBConformance OBJECT IDENTIFIER ::= { hwSSH 4 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.4.1
        hwSSHMIBCompliances OBJECT IDENTIFIER ::= { hwSSHMIBConformance 1 }

        
--    this module
        -- 1.3.6.1.4.1.2011.5.25.118.4.1.1
        hwSSHMIBCompliance MODULE-COMPLIANCE
            STATUS current
            DESCRIPTION 
                "
                The compliance statement for systems supporting 
                the HUAWEI-SSH-MIB.
                "
            MODULE -- this module
                MANDATORY-GROUPS { hwSSHServerGroup, hwSSHUserGroup, hwSSHServerSessionGroup, hwSSHClientGroup, hwSSHServerInfoGroup, 
                    hwSSHNotificationGroup }
            ::= { hwSSHMIBCompliances 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.4.2
        hwSSHMIBGroups OBJECT IDENTIFIER ::= { hwSSHMIBConformance 2 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.4.2.1
        hwSSHServerGroup OBJECT-GROUP
            OBJECTS { hwStelnetServerEnable, hwSftpServerEnable, hwSSHServerComp1x, hwSSHServerTimeOut, hwSSHServerRetry, 
                hwSSHServerPort, hwSSHServerKeyTimeOut, hwSSHServerAlarmEnable, hwSftpMaxUserNum, hwSftpOnLineUserNum, 
                hwSNetConfMaxUserNum, hwSNetConfServerEnable, hwSSHKeepAliveEnable, hwSCPServerEnable, 
                hwSCPMaxUserNum, hwSSHServerInsecureAlgo }
            STATUS current
            DESCRIPTION 
                "
                The SSH server attribute group.
                "
            ::= { hwSSHMIBGroups 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.4.2.2
        hwSSHUserGroup OBJECT-GROUP
            OBJECTS { hwSSHUserName, hwSSHUserAssignKey, hwSSHUserAuthType, hwSSHUserServiceType, hwSSHUserSftpDirectory, 
                hwSSHUserAuthorizationCMD, hwSSHUserRowStatus, hwSSHUserAssignKeyType }
            STATUS current
            DESCRIPTION 
                "
                The SSH user's group.
                "
            ::= { hwSSHMIBGroups 2 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.4.2.3
        hwSSHServerSessionGroup OBJECT-GROUP
            OBJECTS { hwSSHSessionUserName, hwSSHSessionConnectType, hwSSHSessionVer, hwSSHSessionState, hwSSHSessionRetry, 
                hwSSHSessionCtosCipher, hwSSHSessionStocCipher, hwSSHSessionCtosHmac, hwSSHSessionStocHmac, hwSSHSessionKex, 
                hwSSHSessionAuthType, hwSSHSessionServiceType, hwSSHSessionKeyType, hwSSHSessionConnectionIndex, hwSSHSessionCtosCompress, 
                hwSSHSessionStocCompress 
                }
            STATUS current
            DESCRIPTION 
                "
                The SSH server's session group.
                "
            ::= { hwSSHMIBGroups 3 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.4.2.4
        hwSSHClientGroup OBJECT-GROUP
            OBJECTS { hwSSHFirstTimeAuthEnable, hwSSHKeepAliveInterval, hwSSHKeepAliveMaxCount, hwSSHClientInsecureAlgo, hwSSHServerUsedInsecureAlgoClear, hwSSHClientUsedInsecureAlgoClear }
            STATUS current
            DESCRIPTION 
                "
                The SSH client's attribute group.
                "
            ::= { hwSSHMIBGroups 4 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.4.2.5
        hwSSHServerInfoGroup OBJECT-GROUP
            OBJECTS { hwSSHServerName, hwSSHServerAssignKey, hwSSHServerRowStatus, hwSSHServerAssignDSAKey }
            STATUS current
            DESCRIPTION 
                "
                The SSH serverInfo's group.
                "
            ::= { hwSSHMIBGroups 5 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.4.2.6
        hwSSHNotificationGroup NOTIFICATION-GROUP
            NOTIFICATIONS { hwSSHSftpUserNumExceedMax, hwSSHServerUsedInsecureAlgo, hwSSHClientUsedInsecureAlgo }
            STATUS current
            DESCRIPTION 
                "
                The SSH Notification group.
                "
            ::= { hwSSHMIBGroups 6 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.5
        hwRSALocalKeyTable OBJECT IDENTIFIER ::= { hwSSH 5 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.5.1
        hwRSALocalHostPublicKeyCode OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..4096))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the local host RSA Public Key Code in the format of der.
                "
            ::= { hwRSALocalKeyTable 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.5.2
        hwRSALocalHostPublicKeyFingerprint OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..60))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the fingerprint of the local host RSA Public Key Code,
                that including the public key algorithm, length and fingerprint.
                "
            ::= { hwRSALocalKeyTable 2 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.5.3
        hwRSALocalServerPublicKeyCode OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..4096))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the local server RSA Public Key Code in the format of der.
                "
            ::= { hwRSALocalKeyTable 3 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.5.4
        hwRSALocalServerPublicKeyFingerprint OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..60))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the fingerprint of the local server RSA Public Key Code,
                that including the public key algorithm, length and fingerprint.
                "
            ::= { hwRSALocalKeyTable 4 }

        -- 1.3.6.1.4.1.2011.5.25.118.6
        hwSftpClient OBJECT IDENTIFIER ::= { hwSSH 6 }

        -- 1.3.6.1.4.1.2011.5.25.118.6.1
        hwSftpServerAuthenticationSwitch OBJECT-TYPE
            SYNTAX INTEGER
                {
                disable(1),
                enable(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The object specifies whether the sftp server authentication switch.
                Options:
                1.disable(1) -indicates the sftp server authentication switch disable.
                2.enable(2)-indicates the sftp server authentication switch enable.
                The default value is enable.
                "
            ::= { hwSftpClient 1 }

        -- 1.3.6.1.4.1.2011.5.25.118.6.2
        hwSftpServerAuthenticationTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwSftpServerAuthenticationEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                A table of configuration about the relation between the ip address
                and the sftp server public key name.
                "
            ::= { hwSftpClient 2 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.6.2.1
        hwSftpServerAuthenticationEntry OBJECT-TYPE
            SYNTAX HwSftpServerAuthenticationEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                A table of configuration about the relation between the ip address
                and the sftp server public key name.
                The index of this entry is hwSftpServerName.
                "
            INDEX { IMPLIED hwSftpServerName }
            ::= { hwSftpServerAuthenticationTable 1 }

        HwSftpServerAuthenticationEntry ::=
            SEQUENCE {
                hwSftpServerName
                    OCTET STRING,
                hwSftpServerPublicKeyType
                    INTEGER,
                hwSftpServerPublicKeyName
                    OCTET STRING, 
                hwSftpServerRowStatus
                    RowStatus
             }
        
        -- 1.3.6.1.4.1.2011.5.25.118.6.2.1.1
        hwSftpServerName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..255))
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                The IPv4 or IPv6 of the SFTP server.
                "
            ::= { hwSftpServerAuthenticationEntry 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.6.2.1.2
        hwSftpServerPublicKeyType OBJECT-TYPE
            SYNTAX INTEGER 
                { 
                    rsa(1),
                    ed25519(2)
                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                The object specifies the sftp server public key type.
                1.rsa(1)
                2.ed25519(2)
                "
            ::= { hwSftpServerAuthenticationEntry 2 }
        
        -- 1.3.6.1.4.1.2011.5.25.118.6.2.1.3
        hwSftpServerPublicKeyName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..40))
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "
                The object specifies a sftp server public key name .
                This public key name must exist.
                "
            ::= { hwSftpServerAuthenticationEntry 3 }

        -- 1.3.6.1.4.1.2011.5.25.118.6.2.1.4
        hwSftpServerRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "
                Row operation object.
                createAndGo(4)is supplied to create a new instance of a conceptual row.  
                destroy(6)is supplied to delete the instances associated with an existing conceptual row.
                "
            ::= { hwSftpServerAuthenticationEntry 4 }

        -- 1.3.6.1.4.1.2011.5.25.118.7
        hwEd25519LocalKeyTable OBJECT IDENTIFIER ::= { hwSSH 7 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.7.1
        hwEd25519LocalPublicKeyCode OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..512))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the local host ED25519 Public Key Code in the format of der.
                "
            ::= { hwEd25519LocalKeyTable 1 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.7.2
        hwEd25519LocalPublicKeyFingerprint OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..60))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the fingerprint of the local host ED25519 Public Key Code,
                that including the public key algorithm, length and fingerprint.
                "
            ::= { hwEd25519LocalKeyTable 2 }

        -- 1.3.6.1.4.1.2011.5.25.118.1.31
        hwEd25519PublicKeyTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwEd25519PublicKeyEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                A table of configuration about Ed25519 Public Key.
                hwEd25519PublicKeyName is the name of Ed25519 Public Key.              
                "
            ::= { hwSSHServer 31 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.31.1
        hwEd25519PublicKeyEntry OBJECT-TYPE
            SYNTAX HwEd25519PublicKeyEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                A table of configuration about Ed25519 Public Key.
                The index of this entry is hwEd25519PublicKeyName.  
                hwEd25519PublicKeyName is the name of Ed25519 Public Key.
                "
            INDEX { hwEd25519PublicKeyName }
            ::= { hwEd25519PublicKeyTable 1 }

        
        HwEd25519PublicKeyEntry ::=
            SEQUENCE { 
                hwEd25519PublicKeyName
                    OCTET STRING,
                hwEd25519PublicKeyEncodingType
                    INTEGER,
                hwEd25519PublicKeyCode
                    OCTET STRING,
                hwEd25519PublicKeyFingerprint
                    OCTET STRING,
                hwEd25519PublicKeyRowStatus
                    RowStatus
             }

        -- 1.3.6.1.4.1.2011.5.25.118.1.31.1.1
        hwEd25519PublicKeyName OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..40))
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "
                The object specifies the name of Ed25519 Public Key.
                "
            ::= { hwEd25519PublicKeyEntry 1 }

        -- 1.3.6.1.4.1.2011.5.25.118.1.31.1.2
        hwEd25519PublicKeyEncodingType OBJECT-TYPE
            SYNTAX INTEGER
            {
             der(1),
             pem(2),
             openssh(3)
            }
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "The object specifies the ED25519 public key encoding format."
            ::= { hwEd25519PublicKeyEntry 2 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.31.1.3
        hwEd25519PublicKeyCode OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (1..512))
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "
                The object specifies is Ed25519 Public Key Code that in the format of der, the maximum length of the node is 512.             
                When the Ed25519 public key is created, the index value is the name of the public key, which uses the ASCII code.
                The public key value must be generated through a tool. Firstly, use the PUTTYGEN.EXE tool to generate the matching 
                public key and private key. Then, use the sshkey.exe tool to convert the generated public key to the required public key value.
                "
            ::= { hwEd25519PublicKeyEntry 3 }

        
        -- 1.3.6.1.4.1.2011.5.25.118.1.31.1.4
        hwEd25519PublicKeyFingerprint OBJECT-TYPE
            SYNTAX OCTET STRING (SIZE (0..60))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "
                The object specifies the fingerprint of Ed25519 Public Key Code,
                that including the public key algorithm, length and fingerprint.
                "
            ::= { hwEd25519PublicKeyEntry 4 }

        -- 1.3.6.1.4.1.2011.5.25.118.1.31.1.10
        hwEd25519PublicKeyRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "
                The object specifies the status of this table entry.
                When the status is active(1), hwEd25519PublicKeyName, hwEd25519PublicKeyCode's
                value in the entry are allowed to be modified.  
                createAndGo(4) is supplied to create a new instance of a conceptual row.
                destroy(6) is supplied to delete the instances associated with an existing conceptual row.        
                "
            ::= { hwEd25519PublicKeyEntry 10 }

    END
