
   VPN-TC-STD-MIB DEFINITIONS ::= BEGIN

   IMPORTS
       MODULE-IDENTITY, mib-2
           FROM SNMPv2-SMI

       TEXTUAL-CONVENTION
           FROM SNMPv2-TC;

   vpnTcMIB MODULE-IDENTITY
       LAST-UPDATED "200511150000Z"  -- 15 November 2005
       ORGANIZATION
           "Layer 3 Virtual Private Networks (L3VPN) Working Group."
       CONTACT-INFO
           "Benson Schliesser
            bensons@savvis.net

            Thomas D. Nadeau
            tnadeau@cisco.com

            This TC MIB is a product of the PPVPN
            http://www.ietf.org/html.charters/ppvpn-charter.html
            and subsequently the L3VPN
            http://www.ietf.org/html.charters/l3vpn-charter.html
            working groups.

            Comments and discussion should be directed to
            l3vpn@ietf.org"
       DESCRIPTION
           "This MIB contains TCs for VPNs.

            Copyright (C) The Internet Society (2005).  This version
            of this MIB module is part of RFC 4265;  see the RFC
            itself for full legal notices."
       -- Revision history.
       REVISION "200511150000Z"  -- 15 November 2005
       DESCRIPTION "Initial version, published as RFC 4265."
       ::= { mib-2 129 }

   -- definition of textual conventions

   VPNId ::= TEXTUAL-CONVENTION
       STATUS current
       DESCRIPTION
           "The purpose of a VPN-ID is to uniquely identify a VPN.
            The Global VPN Identifier format is:
            3 octet VPN Authority, Organizationally Unique Identifier
            followed by 4 octet VPN index identifying VPN according
            to OUI"
       REFERENCE
           "Fox, B. and Gleeson, B., 'Virtual Private Networks
            Identifier', RFC 2685, September 1999."
       SYNTAX    OCTET STRING (SIZE (7))

   VPNIdOrZero ::= TEXTUAL-CONVENTION
       STATUS            current
       DESCRIPTION
           "This textual convention is an extension of the
            VPNId textual convention that defines a non-zero-length
            OCTET STRING to identify a physical entity.  This extension
            permits the additional value of a zero-length OCTET STRING.
            The semantics of the value zero-length OCTET STRING are
            object-specific and must therefore be defined
            as part of the description of any object that uses this
            syntax.  Examples of usage of this extension are
            situations where none or all VPN IDs need to be
            referenced."
       SYNTAX    OCTET STRING (SIZE (0 | 7))

   END
