
Abstract                                                                                        
--------

Each control enclosure ships with an initialization tool for that product, which is supplied on a USB flash drive. The initialization tool is used to perform initial system configuration. It also simplifies other configuration tasks, such as resetting the superuser password and editing the service IP addresses of a system. There is a different initialization tool for each product. Replacement initialization tools can be obtained from your support center. 


Instructions
------------

This tool is supplied pre-installed on a USB flash drive that came with your control enclosure, or it can be obtained from your support center.

If you downloaded this tool from a support website, begin by copying the contents of this zip archive file to the root directory of any USB flash drive formatted with a FAT32, ext2 or ext3 file system. 

To run the tool from the USB flash drive, complete the following steps for your operating system:


Microsoft Windows XP (32-bit) or Microsoft Windows 7 (64-bit)
-------------------------------------------------------------

Run the InitTool.bat file located in the root directory of the USB flash drive.


Apple Mac OS(R) X 10.7, Red Hat Enterprise Server 5 or Ubuntu(R) desktop 11.04
------------------------------------------------------------------------------
Run the InitTool.sh file located in the root directory of the USB flash drive.


For complete instructions on using the initialization tool for your product, see the installation guide that was shipped with your product, or contact your support center.
