# CMMVC8022W

A new system has been initialized or created, but the node canister remains in the `service` state.

#### Explanation

The system has completed the initialize or create system operation. One reason that the node canister remains in the `service` state is when the battery is still charging. The system goes online automatically when the battery charging operation completes.

#### User response

You can only submit service commands to a node canister while the node canister is in the `service` state. See Resolving a problem topics in the Troubleshooting section of the Information Center.