# BGP Peer Group List

The Virtual Router (BGP) – Peer Group page enables you to create collections of peers that enables all members of the peer group to inherit the attributes configured for the group. Route Maps frequently use peer groups. The Virtual Router (BGP) – Peer page displays the following fields:

Group Name: A string that identifies the peer group you want to create.

Entries: Indicates the number of peers included in the peer group created.

Action: Contains either the Add button that enables you to create a new peer group, or the Configure or Remove buttons.

### To Establish a Peer Group

1. Enter a string that identifies the peer group that you want to create.

2. Click Add to save the string.

The group name appears in the list, with Configure and Remove options in the Action column. Click Configure to configure attributes for the peer group. See BGP Peer Group Configuration.

## Other Configurations

From this page, you can perform the following configurations:

### To Configure Basic BGP Parameters

To configure basic BGP settings, see Virtual Router BGP Settings.

### To Configure a Confederation

To configure BGP confederations, see BGP Confederations.

### To Configure Reachable Networks

To configure BGP confederations, see Network Setting Configuration.

### To Configure BGP Communities

To configure BGP communities, see BGP Communities.

### To Configure Redistribution Rules

To configure conditions to redistribute routes to the current BGP router, see BGP Redistribution Rules.

### To Configure an Aggregate Address

To configure an aggregated BGP address, see BGP Aggregation.

### To Configure BGP Neighbors

To configure BGP neighbors, see BGP Neighbors.

### To Configure an AS-Path Value

To configure an AS-Path value, see AS-Path Configuration.