cb#-02-i.01
- 
The two angled lines that are to be created on the Finger 
Guide are shown here as dashed yellow.  
Choose option 
- 
Choose the CREATE option. 
  
Choose option 
- 
Choose the LINE option. 
  
Choose option 
- 
Choose the ANGLE option. 
  
Choose option 
- 
Enter an angle of 8.36 degrees. 
  
Enter angle (30) => 
angle 
- 
Select the highlighted section of the line. 
  
Select a line
line 
- 
Choose the ENDENT option. 
  
Indicate endpoint for angled line  / Cursor-Indicate position
- 
Select the highlighted section of the line. 
  
Indicate endpoint for angled line  / Select entity
line 
- 
Use the BACK-UP option to return two steps and change 
the angle value for creating a line.   
Indicate endpoint for angled line  / Select entity
- 
Use the BACK-UP one more time.
  
Select a line
- 
Enter an angle of -8.36 degrees. 
  
Enter angle (30) => 
angle 
- 
Select the highlighted section of the line. 
  
Select a line
line 
- 
Select the highlighted section of the line to indicate
the endpoint of the line.  
Indicate endpoint for angled line  / Select entity
line 
- 
Press ESCAPE to exit from this function. 
  
Select a line
- 
cb#-02-r.02
-
