bc#-02-i.01
-
bc#-02-i.02
-
Choose the POLAR option from the Menu Options Window.
  
Indicate center  / Select line
-
Choose the CENTER option from the Menu Options Window.
  
Indicate polar origin  / Cursor-indicate position
-
Select the highlighted circle.
  
Indicate polar origin  / Select entity
circle  
-
Enter an angle of 45 degrees for the polar distance.
  
Enter angle (0) => 
angle  
-
Enter the distance of 1.125 for the polar distance.
  
Enter distance (0) => 
distance  
-
bc#-02-i.03
-
Choose the DELTA option from the Menu Options Window.
 
Indicate delta reference position  / Cursor-indicate position
-
Choose the CENTER option from the Menu Options Window.
  
Indicate delta reference position  / Cursor-indicate position
-
Select the highlighted circle for the DELTA reference
position. Its CENTER will be the reference position.
Indicate delta reference position  / Select entity
circle  
-
Enter a distance of -1 along the X axis.
  
dXV = 
dXV
-
Enter a distance of -1 along the Y axis.
  
dXV = -1           dYV = 
dYV
-
Enter a distance of 0 along the Z axis.
  
dXV = -1           dYV = -1            dZV = 
dZV
-
bc#-02-r.04
-
bc#-02-i.05
-
