de#-02-i.01
- 
This is an illustration of the Finger Guide at the end
of this step with the completed drill hole.
Choose option
-
Choose the X-FORM option. 
  
Choose option 
- 
Choose the PROJECT option. 
  
Choose option 
- 
Choose the SKEWED option. 
  
Choose option 
- 
Choose the JOIN option. 
  
Choose option 
- 
Choose the SINGLE option. 
  
Choose option 
- 
Select the highlighted circle as the entity to be 
projected.  
Select entity 1 (Press RETURN when done)
line 
- 
Press <Enter> to accept the selection.
  
Select entity 2 (Press RETURN when done)
- 
de#-02-i.02
-
Choose the 2 LINES option. 
  
Choose option 
- 
Select the highlighted line to indicate the X axis.
  
Select line for X axis
line 
- 
Select the highlighted line to indicate the Y axis.
  
Select line for Y axis
line 
- 
Choose the 2D ENT option. 
  
Choose option 
- 
Select the highlighted circle as the two-dimensional 
entity.  
Select an arc, 2d spline or a conic
circle
- 
The projected circle created a cylindrical hole through 
the part. Press ESCAPE to exit from this function. 
Choose option
- 
de#-02-r.03
-
