bc#-01-i.01
-
bc#-01-i.02
-
Choose the KEY-IN option from the Menu Options Window.
  
Indicate lower-left corner / Cursor-indicate position
-
Enter a value of 0 for X
  
Indicate lower-left corner  / XV = 
XV  
-
Enter a value of 0 for Y
  
Indicate lower-left corner  / YV = 
YV  
-
Enter a value of 0 for Z
  
Indicate lower-left corner  / ZV = 
ZV  
-
A position marker appears and the object is placed
at a coordinate position of (0,0,0).
  
Indicate lower-left corner  / XV = 
-
bc#-01-i.03
-
Choose the CURSOR option from the Menu Options Window.
  
Indicate lower-left corner  / XV = 
-
Indicate in the highlighted box. The circle's center
will be there.
Indicate center  / Cursor-indicate position
-
bc#-01-i.04
-
Choose POINT from the Menu Options Window.
  
Indicate center  / Cursor-indicate position
-
Select the highlighted point entity.
  
Indicate center  / Select point
point  
-
bc#-01-i.05
-
Choose the ENDENT option from the Menu Options Window.
  
Indicate start point  / Select point
-
Select the highlighted line for the first position at 
the line's endpoint.
Indicate start point  / Select entity
line  
-
Choose the CENTER option from the Menu Options Window.
  
Indicate end point  / Select entity
-
Select the highlighted arc.
  
Indicate end point  / Select entity
arc
-
bc#-01-i.06
-
Choose the INTRSC option in the Menu Option Window.
  
Indicate start point  / Select entity
-
Select the highlighted line.
  
Indicate start point  / Select 1st entity
line  
-
Select the highlighted line.
  
Indicate start point  / Select 2nd entity
line
-
Choose the ALONGL option from the Menu Options Window.
  
Indicate end point  / Select 1st entity
-
Select the highlighted line.
  
Indicate end point  / Select line
line
-
Enter a value of .7 as the distance along the line.
  
Enter Distance (2.5) => 
distance
-
bc#-01-i.07
-
