dd#-02-i.01
- 
The lines that are to be trimmed are highlighted in red.
 
Choose option 
-
Use the Immediate Mode command for changing the display 
view, ALT-V. 
Choose option
ALT-V
-
Enter 5 for view number, to switch to the right side view.
 
Enter view number or choose option (1-8) => 
- 
Use the Immediate Mode command ALT-A to autoscale the 
part. 
Choose option
ALT-A
-
dd#-02-i.02
- 
Choose the EDIT option. 
  
Choose option 
- 
Choose the SECTION option. 
  
Choose option 
- 
Choose the TRIM option. 
  
Choose option 
- 
Choose the ALL DSP option. 
  
Choose option 
- 
Choose the ALL option. 
  
Choose option 
- 
Choose the ENTITY option. 
  
Choose option 
- 
Select the highlighted line as the section indicator.
  
Select line, arc or 2d spline
line
- 
Indicate below the line as the section of the part to 
keep.  
Indicate side to preserve  / Cursor-indicate position
- 
dd#-02-i.03
- 
Use the Immediate Mode command ALT-V to switch to a new 
view. 
Choose option
ALT-V
-
Enter 7 for the isometric view.
 
Enter view number or choose option (1-8) => 
- 
Use the Immediate Mode command CTRL-Q to single delete 
the lines. 
Choose option
CTRL-Q
-
Select the highlighted line as one entity to delete.
 
Select entity 1 (Press RETURN when done)
line
-
Select the highlighted line as one entity to delete.
 
Select entity 2 (Press RETURN when done)
line
-
Press <Enter> to accept the selection.
 
Select entity 3 (Press RETURN when done)
-
Press ESCAPE to exit from this function. 
  
Choose option
- 
dd#-02-r.04
-
