ca#-01-i.01 
-  
This is the beginning construction of the Finger Guide 
that you create in this section.         
Choose option   
-  
ca#-01-i.02 
-  
You create this rectangle as four separate line entities  
using the LINE option.        
Choose option   
-  
Choose the CREATE option.
    
Choose option   
-  
Choose the LINE option.  
   
Choose option   
-  
Choose the RECTANG option.   
   
Choose option   
-  
Choose the WID/HT option.   
   
Choose option   
-  
Enter the width of the rectangle as 4.25 inches by typing   
the value (on the Prompt Line) and pressing <Enter>.    
Enter width of rectangle (0.5) => 
width   
-  
Enter the height of the rectangle as 2.5 inches.   
    
Enter height of rectangle (0.5) => 
height   
-  
Choose the KEY-IN option to enter the position of the   
rectangle.   
Indicate lower-left corner  / Cursor-indicate position   
-  
Enter 0.0 for XV.   
   
Indicate lower-left corner / XV = 
XV   
-  
Enter 0.0 for YV.   
    
Indicate lower-left corner / YV = 
YV   
-  
Enter 0.0 for ZV.   
    
Indicate lower-left corner / ZV = 
ZV   
-  
Press ESCAPE to exit from this function.   
    
Indicate lower-left corner / XV = 
-  
ca#-01-r.03 
- 
