AIRBAG BOSCH RENAULT 8200 277 317/---
0285 001 537
AB8.X

CONFIGURATION: 
DRIVER BAG + PASSENGER BAG + SEAT DRIVER BAG + SEAT PASSENGER DRIVER BAG 

CRASH DATA FROM ADDRESS 02C7 -> 038A
--------------------------------------------------------------------------

MCU DATA:

MOTOROLA 68HC912D60 QFP80
MASKSET 0K13J

PIN15: BKGD
PIN34: RESET
PIN9: VDD
PIN10: VSS

FOR PROGRAMMING USE 8.000Mhz OSCILATOR !
Original quartz 4.4..MHz
No ned to pull up any pin.
With UPA23 do not write more than one line,
otherwise MCU change value of one byte on
adress 0007h from 42 to C2 and modul is locked
for diagnose.