- File Descriptions -

MCWIN211.ZIP:
------------
National Instruments NI-488.2 Software for Windows.
Disk 1 of 1

Distribution Disk for the MC-GPIB
Version 2.1.1
Copyright 1992 National Instruments Corporation.
All Rights Reserved.            
P/N:  422756-64

To create an exact copy of the installation diskette, 
please type (at a DOS Prompt):

PKUNZIP MCWIN211.ZIP X: <enter>
    -Where X is the drive letter for your floppy drive.
    -A minimum of 720 KB floppy is required.

At this point all files will be extracted to the floppy.

The NI-488.2 Windows 3 handler is implemented as a Dynamic Link 
Library (DLL).  It works with Windows 3 in both standard and 
386-enhanced modes.  It does not work with Windows 3 in real mode.  
The NI-488.2 Windows 3 handler is shipped with a language interface 
for Microsoft C, Versions 5.1 and later.  This language interface also 
works with Borland C++, Version 2.0.  Please call National Instruments 
at 1-800-IEEE-488 for information about other available language 
interfaces for Windows 3.

You can also access the NI-488.2 Windows 3 handler without a language
interface by using the direct entry functions described in Appendix A
"Windows 3 DLL Direct Entry NI-488 Functions and NI-488.2 Routines" 
of the "Using Your GPIB Software with Microsoft Windows" manual 
(National Instruments part number 320319-01).

The Windows handler does not support the IBSRQ function.

The NI-488.2 Windows handler modules and their approximate disk space 
requirements are as follows:

                                               Approximate
                 Module                    Disk space required
     ------------------------------        -------------------
     Driver and support files                     300K
     Microsoft C language interface                81K
