readme.txt  9.96  Mwave Developers Toolkit      Release 1.31 for OS/2
=====================================================================

MDK Release 1.31 for OS/2 does not include the following items which
are included in MDK 1.31 for Windows:

        o MeioStat, MwMonitor or MwQuery
        o Additional examples and sample applications

Installation:
=============

Assuming your floppy is disk a:, in an OS/2 shell, type

C> a:
A> setup


   This release has been tested with Mwave Manager version 2.101.  Check
the release notes of an updated manager to verify if is compatible with
this toolkit release.  The linker in this release produces a new file
format, it will not work with Mwave managers prior to 2.99.  If you attempt
to use a new file with an old manager, you will get an internal error
return code 0x1.


Release 1.3
===========

 - Bug fixes, see RELEASE.TXT

 - Debugger modifications:

    o The scope control panel screen positions are maintained in
      the configuration file.

    o The bias control now operates with a positive or negative displacement.

 - The debugger !os command is no longer supported due to problems with the OS/2
   "system" call.  The !os command remaines ih the debugger software for
   backward compatibility, however it is no longer documented.  The !os
   command can cause OS/2 to hang if an OS/2 PM application is invoked.
   The !start command should be used instead if you wish to launch an
   OS/2 PM application


Windows 3.1 Version Compatibility
=================================

  - The mwdebug.ini file is a standard OS/2 .ini file and is not
    compatible with the mwdebug.ini file of Windows.  If the OS/2 version
    of the debugger encounters an Windows version of the mwdebug.ini file
    it will be ignored.

  - The OS/2 debugger can read Windows scope configuration files.  Due
    to differences in the coordinate system, fonts and colors between
    OS/2 and Windows, the scope window can not be identically reproduced.



List of supported connections on current Mwave cards
====================================================

MEIO connections for the following cards are listed below:

        o ACE Adapter
        o Audiovation and Eduquest Adapter
        o Multimedia Modem/Spectrum Solo
        o Windsurfer Adapter
        o 2781 PNP/2780 Pro Reference Design card
        o 2781 PNP Modem only Reference Design card
        o Aptiva card
        o 2780 Reference Design card
        o Thinkpad 755 card
        o Thinkpad 760 card

ACE Adapter:
    LineIn_L1   to CdAdc_L1
    LineIn_R1   to CdAdc_R1
    LineIn_S1   to CdAdc_S1
    Mic_L1      to CdAdc_L1
    Mic_R1      to CdAdc_R1
    Mic_S1      to CdAdc_S1
    CddAIn_L1   to CdAdc_L1
    CddAIn_R1   to CdAdc_R1
    CddAIn_S1   to CdAdc_S1
    CdDac_L1    to LineOut_L1
    CdDac_R1    to LineOut_R1
    CdDac_S1    to LineOut_S1
    CdDac_L1    to Head_L1
    CdDac_R1    to Head_R1
    CdDac_S1    to Head_S1
    CdDac_L1    to Head_L2
    Mic_L1      to VoiceAdc_1
    HandIn_1    to VoiceAdc_1
    HandIn_1    to TeleOut_1
    VoiceDac_1  to HandOut_1
    VoiceDac_1  to Head_L2
    VoiceDac_1  to LineOut_L1
    TeleIn_1    to TeleAdc_1
    TeleDac_1   to TeleOut_1
    MidiIn_1    to MidiRx_1
    MidiTx_1    to MidiOut_1
    MidiIn_1    to MidiThruOut_1
    MidiTx_1    to MidiThruOut_1
    CommTx_1    to UartOut_1
    UartIn_1    to CommRx_1

Audiovation and Eduquest Adapter:
    LineIn_L1   to CdAdc_L1
    LineIn_R1   to CdAdc_R1
    LineIn_S1   to CdAdc_S1
    LineIn_L2   to CdAdc_L1
    LineIn_R2   to CdAdc_R1
    LineIn_S2   to CdAdc_S1
    LineIn_L3   to CdAdc_L1
    LineIn_R3   to CdAdc_R1
    LineIn_S3   to CdAdc_S1
    LineIn_L4   to CdAdc_L1
    LineIn_R4   to CdAdc_R1
    LineIn_S4   to CdAdc_S1
    Mic_L1      to CdAdc_L1
    Mic_R1      to CdAdc_R1
    Mic_S1      to CdAdc_S1
    Mic_L2      to CdAdc_L1
    Mic_R2      to CdAdc_R1
    Mic_S2      to CdAdc_S1
    CddAIn_L1   to CdAdc_L1
    CddAIn_R1   to CdAdc_R1
    CddAIn_S1   to CdAdc_S1
    CdDac_L1    to LineOut_L1
    CdDac_R1    to LineOut_R1
    CdDac_S1    to LineOut_S1
    CdDac_L1    to Head_L1
    CdDac_R1    to Head_R1
    CdDac_S1    to Head_S1
    CdDac_L1    to IntSpkrOut_L1
    CdDac_R1    to IntSpkrOut_L1
    CdDac_S1    to IntSpkrOut_L1
    CddAIn_S1   to CdAdc_S1
    MidiIn_1    to MidiRx_1
    MidiTx_1    to MidiOut_1
    MidiIn_1    to MidiThruOut_1
    MidiTx_1    to MidiThruOut_1

Multimedia Modem/Spectrum Solo:
    Mic_L1      to CdAdc_L1
    Mic_R1      to CdAdc_R1
    Mic_S1      to CdAdc_S1
    CddAIn_L1   to CdAdc_L1
    CddAIn_R1   to CdAdc_R1
    CddAIn_S1   to CdAdc_S1
    CdDac_L1    to LineOut_L1
    CdDac_R1    to LineOut_R1
    CdDac_S1    to LineOut_S1
    CdDac_L1    to Head_L1
    CdDac_R1    to Head_R1
    CdDac_S1    to Head_S1
    CdDac_S1    to IntSpkrOut_L1
    Mic_L1      to VoiceAdc_1
    HandIn_1    to VoiceAdc_1
    HandIn_1    to TeleOut_1
    VoiceDac_1  to HandOut_1
    VoiceDac_1  to LineOutL1
    TeleIn1     to HandOut1
    TeleIn_1    to TeleAdc_1
    TeleDac_1   to TeleOut_1
    CommTx_1    to UartOut_1
    UartIn_1    to CommRx_1


Windsurfer Adapter:
    LineIn_L1   to CdAdc_L1
    LineIn_R1   to CdAdc_R1
    LineIn_S1   to CdAdc_S1
    LineIn_L2   to CdAdc_L1
    LineIn_R2   to CdAdc_R1
    LineIn_S2   to CdAdc_S1
    Mic_L1      to CdAdc_L1
    Mic_R1      to CdAdc_R1
    Mic_S1      to CdAdc_S1
    CddAIn_L1   to CdAdc_L1
    CddAIn_R1   to CdAdc_R1
    CddAIn_S1   to CdAdc_S1
    CdDac_L1    to LineOut_L1
    CdDac_R1    to LineOut_R1
    CdDac_S1    to LineOut_S1
    CdDac_L1    to LineOut_L2
    CdDac_R1    to LineOut_R2
    CdDac_S1    to LineOut_S2
    CdDac_L1    to Head_L1
    CdDac_R1    to Head_R1
    CdDac_S1    to Head_S1
    CdDac_L1    to IntSpkrOut_L1
    CdDac_R1    to IntSpkrOut_L1
    CdDac_S1    to IntSpkrOut_L1
    Mic_L1      to VoiceAdc_1
    HandIn_1    to VoiceAdc_1
    HandIn_1    to TeleOut_1
    VoiceDac_1  to HandOut_1
    TeleIn_1    to TeleAdc_1
    TeleDac_1   to TeleOut_1
    MidiIn_1    to MidiRx_1
    MidiTx_1    to MidiOut_1
    MidiIn_1    to MidiThruOut_1
    MidiTx_1    to MidiThruOut_1
    CommTx_1    to UartOut_1
    UartIn_1    to CommRx_1

For the 2781 PNP/2780 Pro Reference card:
    LineInS1    to CdAdcS1
    LineInL1    to CdAdcL1
    LineInR1    to CdAdcR1
    MicS1       to CdAdcS1
    MicL1       to CdAdcL1
    MicR1       to CdAdcR1
    HeadMicL1   to CdAdcL1
    HeadMicR1   to CdAdcR1
    HeadMicS1   to CdAdcS1
    CddAInS1    to CdAdcS1
    CddAInL1    to CdAdcL1
    CddAInR1    to CdAdcR1
    LineOutS1   to CdAdcS
    LineOutL1   to CdAdcL1
    LineOutR1   to CdAdcR1
    LineInS1    to LineOutS1
    LineInL1    to LineOutL1
    LineInR1    to LineOutR1
    CddAInS1    to LineOutS1
    CddAInL1    to LineOutL1
    CddAInR1    to LineOutR1
    LineInS2    to LineOutS1
    LineInL2    to LineOutL1
    LineInR2    to LineOutR1
    CdDacS1     to LineOutS1
    CdDacL1     to LineOutL1
    CdDacR1     to LineOutR1
    MonoIn1     to LineOutS1
    MonoIn1     to MonoOut1
    CdDacS1     to MonoOut1
    CdAdcS1     to CdDacS1
    TeleIn1     to TeleAdc1
    TeleDac1    to TeleOut1
    HandIn1     to TeleOut1
    MicL1       to VoiceAdc1
    HeadMicL1   to VoiceAdc1
    HandIn1     to VoiceAdc1
    VoiceDac1   to HandOut1
    CommTx1     to UartOut1
    UartIn1     to CommRx1
    VoiceDac1   to LineOutL1
    V96Dac1     to LineOutL1
    MicL1       to V96Adc1

For the 2781 PNP Modem only card:
    MicS1       to CdAdcS1
    MicL1       to CdAdcL1
    MicR1       to CdAdcR1
    HeadMicL1   to CdAdcL1
    HeadMicR1   to CdAdcR1
    HeadMicS1   to CdAdcS1
    LineOutS1   to CdAdcS
    LineOutL1   to CdAdcL1
    LineOutR1   to CdAdcR1
    CdDacS1     to LineOutS1
    CdDacL1     to LineOutL1
    CdDacR1     to LineOutR1
    TeleIn1     to TeleAdc1
    TeleDac1    to TeleOut1
    HandIn1     to TeleOut1
    MicL1       to VoiceAdc1
    HeadMicL1   to VoiceAdc1
    HandIn1     to VoiceAdc1
    VoiceDac1   to HandOut1
    CommTx1     to UartOut1
    UartIn1     to CommRx1
    VoiceDac1   to LineOutL1
    V96Dac1     to LineOutL1
    MicL1       to V96Adc1

For the Aptiva card:
    LineInL1    to CdAdcL1
    LineInR1    to CdAdcR1
    LineInS1    to CdAdcS1
    MicL1       to CdAdcL1
    MicL1       to CdAdcR1
    MicL1       to EmulCdAdcR1
    MicR1       to CdAdcR1
    MicS1       to CdAdcS1
    HeadMicL1   to CdAdcL1
    HeadMicL1   to CdAdcR1
    HeadMicR1   to CdAdcR1
    HeadMicS1   to CdAdcS1
    CddAInL1    to CdAdcL1
    CddAInR1    to CdAdcR1
    CddAInS1    to CdAdcS1
    CdDacL1     to LineOutL1
    CdDacR1     to LineOutR1
    CdDacS1     to LineOutS1
    CdDacL1     to HeadL1
    CdDacR1     to HeadR1
    CdDacS1     to HeadS1
    CdDacL1     to HeadSpkrL1
    CdDacR1     to HeadSpkrR1
    CdDacS1     to HeadSpkrS1
    CdDacL1     to IntSpkrOutL1
    CdDacR1     to IntSpkrOutL1
    CdDacS1     to IntSpkrOutL1
    MicL1       to VoiceAdc1
    HeadMicL1   to VoiceAdc1
    HandIn1     to VoiceAdc1
    HandIn1     to TeleOut1
    VoiceDac1   to HandOut1
    TeleIn1     to TeleAdc1
    TeleDac1    to TeleOut1
    MidiIn1     to MidiRx1
    MidiTx1     to MidiOut1
    MidiIn1     to MidiThruOut1
    MidiTx1     to MidiThruOut1
    CommTx1     to UartOut1
    UartIn1     to CommRx1

For the 2780 reference design card:
    LineInL1    to CdAdcL1
    LineInR1    to CdAdcR1
    LineInS1    to CdAdcS1
    MicL1       to CdAdcL1
    MicL1       to CdAdcR1
    MicL1       to EmulCdAdcR1
    MicR1       to CdAdcR1
    MicS1       to CdAdcS1
    HeadMicL1   to CdAdcL1
    HeadMicL1   to CdAdcR1
    HeadMicR1   to CdAdcR1
    HeadMicS1   to CdAdcS1
    CddAInL1    to CdAdcL1
    CddAInR1    to CdAdcR1
    CddAInS1    to CdAdcS1
    CdDacL1     to LineOutL1
    CdDacR1     to LineOutR1
    CdDacS1     to LineOutS1
    CdDacL1     to HeadL1
    CdDacR1     to HeadR1
    CdDacS1     to HeadS1
    CdDacL1     to HeadSpkrL1
    CdDacR1     to HeadSpkrR1
    CdDacS1     to HeadSpkrS1
    CdDacL1     to IntSpkrOutL1
    CdDacR1     to IntSpkrOutL1
    CdDacS1     to IntSpkrOutL1
    MicL1       to VoiceAdc1
    HeadMicL1   to VoiceAdc1
    HandIn1     to VoiceAdc1
    HandIn1     to TeleOut1
    VoiceDac1   to HandOut1
    TeleIn1     to TeleAdc1
    TeleDac1    to TeleOut1
    MidiIn1     to MidiRx1
    MidiTx1     to MidiOut1
    MidiIn1     to MidiThruOut1
    MidiTx1     to MidiThruOut1
    CommTx1     to UartOut1
    UartIn1     to CommRx1

For the Thinkpad 755 card:
    LineInL1    to CdAdcL1
    LineInR1    to CdAdcR1
    LineInS1    to CdAdcS1
    MicL1       to CdAdcL1
    MicR1       to CdAdcR1
    MicS1       to CdAdcS1
    CddAInL1    to CdAdcL1
    CddAInR1    to CdAdcR1
    CddAInS1    to CdAdcS1
    CdDacL1     to LineOutL1
    CdDacR1     to LineOutR1
    CdDacS1     to LineOutS1
    CdDacL1     to HeadL1
    CdDacR1     to HeadR1
    CdDacS1     to HeadS1
    CdDacS1     to IntSpkrOutL1
    CdDacL1     to IntSpkrOutL1
    CdDacR1     to IntSpkrOutL1
    MicL1       to VoiceAdc1
    HandIn1     to VoiceAdc1
    HandIn1     to TeleOut1
    VoiceDac1   to HandOut1
    TeleIn1     to TeleAdc1
    TeleDac1    to TeleOut1
    CommTx1     to UartOut1
    UartIn1     to CommRx1

For the Thinkpad 760 card:
    LineInL1    to CdAdcL1
    LineInR1    to CdAdcR1
    LineInS1    to CdAdcS1
    LineInS1    to LineOutS1
    CddaInS1    to LineOutS1
    MicL1       to CdAdcL1
    MicR1       to CdAdcR1
    MicS1       to CdAdcS1
    CddAInL1    to CdAdcL1
    CddAInR1    to CdAdcR1
    CddAInS1    to CdAdcS1
    CdDacL1     to LineOutL1
    CdDacR1     to LineOutR1
    CdDacS1     to LineOutS1
    CdDacL1     to HeadL1
    CdDacR1     to HeadR1
    CdDacS1     to HeadS1
    CdDacS1     to IntSpkrOutL1
    CdDacL1     to IntSpkrOutL1
    CdDacR1     to IntSpkrOutL1
    MicL1       to VoiceAdc1
    HandIn1     to VoiceAdc1
    HandIn1     to TeleOut1
    VoiceDac1   to HandOut1
    TeleIn1     to TeleAdc1
    TeleDac1    to TeleOut1
    CommTx1     to UartOut1
    UartIn1     to CommRx1
[ End of File ]
