***********************************************************************************
   This directory contains fixes for R/390 Release 4.1.1.1 
***********************************************************************************

General Infomation:
-------------------

  * r390.obj 4.1.1.1 (for AIX 4.1.4, 4.1.5)  

   note: 4111 is the latest level for the MCA P/390 on RS/6000. If installed,
	 you must remove r390.obj.4.1.0.1 and install the r390_4111.installp 
         image provided here (compressed) before picking up any 4111 fixes. 

         When installing, you MUST use P/390 Advanced Diags/LIC version 1.2x.   
	 Contact your R/390 service provider for this diskette.


For Automated Installation of the latest fixes:
-----------------------------------------------
  ALWAYS shutdown the 390 OS, stop390 (END P/390), and exit "R/390 Main Menu"
	 before applying.

   1) Download 4111FIXS.LST (ascii) and 4111FIXS.ZIP (binary) to your R/390
      system in a directory with at least 20MB of free space.

   2) type '/usr/lpp/r390/bin/unzip 4111fixs.zip apply4111' to extract the install script.

   3) type './apply4111'

   4) If prompted "replace xxxx.xxx? " reply with A (upper case).
   
   5) Follow the Special Instructions listed.	

   Note: As of 9/2/98, apply4111 will also update the P/390 LIC files to the
         latest level.   


Fix Methods for Manual Installation: 
------------------------------------
  ALWAYS shutdown the 390 OS, stop390 (END P/390), and exit "R/390 Main Menu"
	 before applying any fix.
  ALWAYS back up the old module before applying any fix module.
  ALWAYS observe the module type (BIN vs. ASC).
  ALWAYS observe the mixed case file names (do not convert).

  See which of these steps to use below for each fix (Patch Steps):
  1) Copy module to /usr/bin/r390 and remove the file extention(s) 
  2) chmod 755 mod_name
  3) ipl390 (IPL P/390) to activate
  4) Copy module to /etc/drivers and remove the file extention
  5) shutdown -Fr (reboot AIX to activate) 
  6) Copy module to /usr/bin/r390 and change the file extention to .EXE
  7) chmod 644 mod_name
  8) Copy module to /usr/bin/r390 as is (ASCII file) 
  9) Modify the ipl390 script file appropriately. See Special Instructions Below! 
 10) Applied automatically by the apply4111 script.  Can be manually applied with
     the licupdte script. 
 11) Copy to /usr/lib/nls/msg/En_US and en_US.


Fixes for 4.1.1.1:         
------------------
                                                                  D S C
                                                                  E Y U
                                                                  V S S
                                                                  T T T
                                                                  E E E
                                                                  T S S
No/Filename         MMDDYY Fix description                        T T T CoReqs   Steps
-----------------   ------ -------------------------------------------- ------   -----
01 dm34xx.Abin      050597 Allow AIX to use drive aft MVS offline Y N Y  None    1-2-3
   dm34xx.Bbin      101497 DDR370 problem on tape changes         Y N N  None    1-2-3
                           Support for IBM 3490-F00 & F01         Y Y N 
   dm34xx.Cbin      101497 MVS IEA435I error msg due to IDRC      Y N Y  None    1-2-3
   dm34xx.Dbin      110797 Fix for ditto using 8MM Exabyte        Y N Y  None    1-2-3
   dm34xx.Ebin      030598 USER process to remove restriction.    Y N Y  NONE    1-2-9-3
                           (Tape no longer required at IPL time !!)
                           Problem detecting eject button fixed.
                           8MM problem using VMFPLC2 on VM fixed.
                           Problem using IBM 3570 Magstar fixed.
                           Problem using IBM 9348 fixed.
                           See Special Instructions Below!
   dm34xx.Fbin      031298 Enhanced Ld Dsply CCW and tape changes Y N Y  NONE    1-2-9-3
                           See Special Instructions Below!
   dm34xx.Gbin      031298 Fixed 8MM prob with VM370 mode VMFPLC2 Y N Y  NONE    1-2-9-3
                           See Special Instructions Below!
   dm34xx.Hbin      032698 Fixes "Read Only" mode of operation    Y N Y  NONE    1-2-9-3
                           Fixes problems with blank 8MM tapes
                           See Special Instructions Below!
   dm34xx.Ibin      032798 Fixes VSE PID tape prob with 4MM DAT   Y N Y  NONE    1-2-9-3
                           FIxes TPF tape problems. 
                           See Special Instructions Below!
   dm34xx.Jbin      040398 Fixes Read Backward problem            Y N Y  NONE    1-2-9-3
                           Improved device claiming algorithm
                           See Special Instructions Below!
   dm34xx.Kbin      040898 Recognize EXABYTE 8505 8MM tape        Y N Y  NONE    1-2-9-3
                           See Special Instructions Below!
   dm34xx.Lbin      041698 Fixes long delay after RUN command     Y N Y  NONE    1-2-9-3
                           Fixes problems with multiple tapes not ready
                           See Special Instructions Below!
   dm34xx.Mbin      042498 Fixes err=11 problem with mult tapes   Y N Y  NONE    1-2-9-3
                           See Special Instructions Below!
   dm34xx.Nbin      042898 Debug logs were not wrapping....       Y N Y  NONE    1-2-9-3
                           See Special Instructions Below!
   dm34xx.Obin      060598 Autoloader detection problem on Fuj    Y N Y  None    1-2-9-3
                           Blank tape handling corrections  
                           See Special Instructions Below!
   dm34xx.Pbin      081398 Increased wait for tape ready (RC=11)  Y N N  None    1-2-9-3
                           See Special Instructions Below!
   dm34xx.Qbin      092398 Removed limit of 7 tape drives         Y N N
                           Now configures 1 device per process to 
                           prevent timeouts during IPL and improve
                           performance when more than 1 drive is in use.
                           See Special Instructions Below!
   dm34xx.Rbin      111198 DLT problem fixed for Ditto Tape Map   Y N N
   dm34xx.Sbin      010699 Fixes uninitialized/void tape problem  Y N N
   dm34xx.Tbin      042299 Fixes missing ERA code on media error  Y N N
   dm34xx.Ubin      060499 Fixes Overland L490E 18 vs 36 trk prob Y N N
   dm34xx.Vbin      082699 Fixes 4/8MM problem "invalid format"   Y Y Y

02 lcs3172rx.Abin   050797 Errors as non-preferred guest under VM Y N N lcs3172tx 1-2-3
   lcs3172tx.Abin   050797 Errors as non-preferred guest under VM Y N N lcs3172rx 1-2-3
   lcs3172rx.Bbin   082597 Fixes INTERLINK problem under OS/390   Y N N
   lcs3172tx.Bbin   082597 Fixes INTERLINK problem under OS/390   Y N N
   lcs3172rx.Cbin   022498 Standard Ethernet problem (OS/390 2.4) Y N Y
   lcs3172tx.Cbin   022498 Standard Ethernet problem (OS/390 2.4) Y N Y
   lcs3172rx.Dbin   042998 Performance enhancement plus log wrap  Y N Y 
   lcs3172tx.Dbin   042998 Performance enhancement plus log wrap  Y N Y
   lcs3172rx.Ebin   060198 Better Performance on busy LANs        Y N Y
   lcs3172tx.Ebin   060198 Better Performance on busy LANs        Y N Y
   lcs3172rx.Fbin   070898 Better performance on outgoing data    Y N N
   lcs3172tx.Fbin   070898 Better performance on outgoing data    Y N N 
   lcs3172rx.Gbin   100698 OS390 2.6 problem with new TCP/IP      Y N Y
   lcs3172tx.Gbin   100698 OS390 2.6 problem with new TCP/IP      Y N Y
   lcs3172tx.Hbin   020899 "End P/390" sometimes takes too long.  Y Y N 
   lcs3172rx.Hbin   020899 "End P/390" sometimes takes too long.  Y Y N 
   lcs3172tx.Ibin   120500 LINUX fix for Token Ring               Y Y Y  none
   lcs3172rx.Ibin   120500 LINUX fix for Token Ring               Y Y Y  none

04 chan.Abin        050197 3174 async problem during file xfer    Y N Y  None    1-2-3
   chan.Bbin        061197 Fixes 370 VMBACKUP running under VMESA Y N Y  None    1-2-3
   chan.Cbin        061897 ASYNC interrupt handling enhancments   Y N Y  None    1-2-3
                    061897 Fixed halt to a suspended device 14786 Y N N  None    1-2-3
   chan.Dbin        062697 5088 fix & more interrupt enhancments  Y Y Y  None    1-2-3 See huron
   chan.Ebin        062797 PVM ESA mode CHAIN-DATA-READ problem   Y Y N  None    1-2-3
   chan.Fbin        070197 PVM ESA mode Invalid Address problem   Y Y N  None    1-2-3
   chan.Gbin        082597 3174 prob (CHAN370 370 guest of VMESA) Y Y N  None    1-2-3
   chan.Hbin        091097 Fixes 370 VMBACKUP running under VMESA Y N N  None    1-2-3
   chan.Ibin        093097 PMR32400 VSE IDCAM restore problem     Y N Y  See 23  1-2-3
   chan.Jbin        101497 DDR370 problem on tape changes	  Y N N  None    1-2-3
		    102497 **DELETED**     
   chan.Kbin        101697 VM/SP IPL problem. Can affect VSE too. Y N Y  None    1-2-3
		    102497 **DELETED**     
   chan.Lbin        102497 Problem handling async interrupts      Y N Y  None    1-2-3
			   NOTE: J and K deleted....bug introduced in J,
   chan.Mbin        102897 3720 probs - fmt 0 CCWs chained w/TICs Y N N  None    1-2-3
   chan.Nbin        111197 Fix fmt 0 CCW prob introduced by Mbin  Y N N  None    1-2-3
                           Fix for VM/ESA IFI004 ABEND (LAN3172 device)
   chan.Obin        111397 ASYNC interrupt performance enhancemnt Y N N  None    1-2-3
   chan.Pbin        120297 More ASYNC enhancemnts (3745 problem)  Y N N  None    1-2-3
   chan.Qbin        022098 Incorrect length problem (PMS 90192)   Y N Y  NONE
                           LAN3172 problem with 2 ethernets       Y N N  NONE
   chan.Rbin        030598 Fixes crash when IPL on AIX 4.3        Y N N  NONE
   chan.Sbin        070898 370 Mode fix for AWSICE CU Busy,CU End Y N Y  13-Bbin 1-2-3
   chan.Tbin        020899 AWSICE start prob with certain LOCALE  Y Y N  13-Bbin 1-2-3
   chan.Ubin        113000 Defered CC=1 on chan PGM check. LINUX  Y Y N
   chan.Vbin        031601 Latest level                           Y Y N

05 dmhuron.Abin     050897 3174 TIO problem (370 mode)            Y Y N  None    1-2-3
   dmhuron.Bbin     062697 5088/GAM-CADM fixes                    Y Y Y  09,10   1-2-3 See chan
   dmhuron.Cbin     081397 Handle Async Unit Check (3174 SNA)     Y N N  09E,10E 1-2-3

06 awssdump.Abin    051497 This version has been deleted          ------------------
   awssdump.Bbin    051497 Snap Shot Dump caused crash            Y N N  None    1-2-3
   awssdump.Cbin    111397 Bring up to same level as in R390.4210 Y Y N  
   awssdump.Dbin    061099 Bring up to same level as in R390.4310 Y Y N 

07 dmx25lcp.Abin    051597 Fixes line drops after several hours   Y N Y  08A     1-2-3
   dmx25lcp.Bbin    061197 Performance enhancement                Y N N  08B     1-2-3
   dmx25lcp.Cbin    060398 After vary inact VSE hangs,must re-IPL Y N Y  08C     1-2-3
08 dmx25bpp.Abin    051597 Fixes line drops after several hours   Y N Y  07A     1-2-3
   dmx25bpp.Bbin    061197 Performance enhancement                Y N N  07B     1-2-3
   dmx25bpp.Cbin    060398 After vary inact VSE hangs,must re-IPL Y N Y  07C     1-2-3

09 huronmain.Abin   051697 Fixes 5088 problem (GAM apps)          Y N N  10      4-2-5
   huronmain.Bbin   061097 Fixes 3480/3420 VM/370 IPL             Y N N  10      4-2-5
   huronmain.Cbin   062697 5088/GAM-CADAM fixes                   Y Y Y  10.05   4-2-5
   huronmain.Dbin   070797 3420 VSE/370 on VM/370-ditto undet err Y Y Y  10.05   4-2-5
   huronmain.Ebin   081397 Handle Async Unit Check (3174 SNA)     Y N N  10E.05C 4-2-5
   huronmain.Fbin   090897 3174-1L SNA TR GTWY "device INOP"      Y Y Y  10F.05C 4-2-5
                           3725 BSNC error "lost data" at 4800    Y Y Y  10F.05C 4-2-5
                           Performance Enhancement                Y Y Y  10F.05C 4-2-5
                           Missing CE/DE on VTAM Startup          Y Y N  10F.05C 4-2-5
   huronmain.Gbin   101697 PMRs 22716,34915 3270 prob & performnc Y Y Y  10G,05C 4-2-5
   huronmain.Hbin   102897 3270 Unit Check problem when Chained   Y N N  10H,05C 4-2-5
   huronmain.Ibin   051198 3174L problem - TR gateway Missing Int Y Y N  10H,05C 4-2-5
   huronmain.Jbin   021799 AIX Hangs due to tracing bug           Y Y N  10J,05C 4-2-5
10 hurondd.Abin     051697 See huronmain                          Y N N  09      4-2-5
   hurondd.Bbin     061097 See huronmain                          Y N N  09      4-2-5
   hurondd.Cbin     062697 See huronmain                          Y Y Y  09,05   4-2-5
   hurondd.Dbin     070797 See huronmain                          Y Y Y  09.05   4-2-5
   hurondd.Ebin     081397 See huronmain                          Y N N  09E.05C 4-2-5
   hurondd.Fbin     090897 See huronmain                          Y N N  09F.05C 4-2-5
   hurondd.Gbin     101697 See huronmain                          Y N N  09G.05C 4-2-5
   hurondd.Hbin     102897 See huronmain                          Y N N  09H.05C 4-2-5
   hurondd.Jbin   	021799 See Huronmain                          Y Y N  09J,05C 4-2-5

11 dmckd.Abin       052197 Added detection of invalid seek arg    Y Y N  None    1-2-3 
   dmckd.Bbin       062697 CMS Format problem (VM 370 ?)          Y Y N  None    1-2-3 
   dmckd.Cbin       102897 Picks up some SYNSORT fixes            Y Y N  None    1-2-3 
   dmckd.Ebin       070698 Second parm not recognized on startup  Y N N  None    1-2-3
                           (only a problem if -ckd3380 specified)
   dmckd.Fbin       081398 Added back awsmount support (got lost) Y N Y
   dmckd.Gbin       081498 awsmount -u problem (crash on EndP390) Y N Y
                           Fixed awsmount -m 
                           Second file of 3390-03 not flushed on terminate
   dmckd.Hbin       110498 Hardware error recovery enhancements   Y N Y
   dmckd.Ibin       051299 VSE SyncSort problem                   Y N Y
   dmckd.Jbin       061099 Locate record problem on latest VSE    Y N Y
   dmckd.Kbin       040400 Prevent lost volumes when bad filename Y N Y
   dmckd.Lbin       011001 Misc EREP, Erase Write, Overflow fixes Y Y Y
                           Fixes for Extended VSAM datasets       Y Y Y
   dmckd.Mbin       030701 3390 Write Data in 0B Domain w/cnt=1   Y Y Y
   dmckd.Nbin       073101 Flush trk buffer on termination.       Y Y N

12 awspbs.Abin      062697 HALT fix for quiecing lines            Y Y N  None    1-2-3 
   awspbs.Bbin      070197 Residual Byte count fix (PVM)          Y Y N  None    1-2-3 
   awspbs.Cbin      070997 Snap Shot Dump Problem (bad ptr)       Y Y N  None    1-2-3 

13 dmlib.Abin       070997 Prevents crash on Snap Shot if bad ptr Y Y N  None    1-2-3
   dmlib.Bbin       070898 370 Mode fix for AWSICE CU Busy,CU End Y N Y  04-Sbin 1-2-3
   dmlib.Cbin       020899 "End P/390" sometimes takes too long.  Y Y N  04-Sbin 1-2-3
   dmlib.Dbin       031601 Latest level                           Y Y N

14 tn3270s.Abin     071697 PSIGDELIVERY err-AWS3274 session drops Y Y N  None    1-2-3
   tn3270s.Bbin     012898 200 users                              Y Y N  
   tn3270s.Cbin     052098 AWS3274 Cons hangs, drops, or prog702  Y Y N  
   tn3270s.Dbin     101999 LU Name support for TN3270E clients    Y Y Y  
15 dm3270.Abin      071697 Bump max number devices from 48 to 64  Y Y N  None    1-2-3
   dm3270.Bbin      012898 200 users                              Y Y N
   dm3270.Cbin      052098 AWS3274 Cons hangs, drops, or prog702  Y Y N 
   dm3270.Dbin      101999 LU Name support for TN3270E clients    Y Y Y  
   dm3270.Ebin      102499 Some LU Names didnt work.              Y Y Y

16 AWS3274.DOC      071697 Bump max number devices from 48 to 64  Y Y N  15      8 
   AWS3274.DOC      101999 LU Name support for TN3270E clients    Y Y Y  

17 awscnf.Abin      072997 Fixed available free space calculation Y Y N  18 19   1-2
   awscnf.Bbin      120297 MMAP failure on multiple large files   Y Y N
   awscnf.Cbin      101698 Latest version                         Y Y N
   awscnf.Dbin      110998 CRS22RA omit DMKRIO on 'new' parameter Y N N
   awscnf.Ebin      111898 Insure msg is seen if error on startup Y N N
   awscnf.Fbin      120498 Cosmetic change to PF definitions      Y Y N
   awscnf.Gbin      051899 Fix 4-digit IPL addr and add awspass   Y Y N
18 alc.Abin         072997 Fixed available free space calculation Y Y N  17 19   1-2
   alc.Bbin         120297 MMAP failure on multiple large files   Y Y N 
   alc.Cbin         101698 Latest version                         Y Y N 
19 ckdalc.Abin      072997 Fixed available free space calculation Y Y N  17 18   1-2
   ckdalc.Bbin      120297 MMAP failure on multiple large files   Y Y N
   ckdalc.Cbin      101698 Latest version                         Y Y N
20 printer.Abin     081397 Fixed CR on 01 Write CCW               Y Y N  None    1-2-3
   printer.Bbin     012398 Fixes SERIAL prtrs. better performance Y Y Y  None    1-2-3
   printer.Cbin     031298 Fixes probs using queue and eoj string Y Y Y  None    1-2-3
                           Enhanced parallel printer int req      Y N Y  None
   printer.Dbin     050198 VMESA wont print when type 3211        Y Y Y  None    1-2-3
   printer.Ebin     070998 1403 Write/Skip Ch 1 not page ejecting Y N Y  None    1-2-3
                           Also added EOJ line 0 wildcard support  
   printer.Fbin     071398 Intermittent intervention req on files Y N Y
   printer.Gbin     072498 Minor architectural corrections        Y Y N
   printer.Hbin     080598 Fixes lost job when queue is busy      Y N Y
   printer.Ibin     082898 Fixes queue file overlay problem       Y N Y
   printer.Jbin     110498 Mult EOJ/QUEUE support.See AWS2821.DOC Y N Y
   printer.Kbin     120998 Put SenseID back in to be same as P390 Y N Y
                           Added -nosid parm to disable Sense ID if needed

21 dm2540.Abin      090497 AWS2540 0 records in file (VM/ESA 2.2) Y Y N  None    1-2-3
   dm2540.Bbin      100197 AWS2540 wild-card problem using /rdr/* Y Y N  
   dm2540.Cbin      091798 AWS2540 Bug when LF or CR in col 81    Y N Y  
                           Also added debug option (-d)
   dm2540.Dbin      092298 VM IPL hangs if too many hot rdr files Y N Y
   dm2540.Fbin      060899 Latest level.  Fixes probs on IPL      Y N Y
22 p390dd.Abin      090497 P390 Device Driver enhancements        Y Y N  None    4-2-5
   p390dd.Bbin      041498 CRS-5RF External Interrupt not working Y Y N 
   p390dd.Cbin      091798 Load microcode failure on 580          Y N Y 
   p390dd.Dbin      110498 Load microcode failure on 580 (092598) Y N Y 
   p390dd.Ebin      010699 Fixed Disabled wait                    Y Y N  39A 
23 dasd.Abin        093097 PMR32400 VSE IDCAM restore to FBA bug  Y N Y  04I     1-2-9-3
   dasd.Bbin        030598 First CCW data transfer problem        Y N Y 
                           See Special Instructions Below!
24 AWS2821.DOC      100297 Clarification of printer set-up        Y N N  none    8
                    070998 EOJ line 0 wildcard support            Y N Y 
                    110498 Multiple EOJ and QUEUE support         Y N Y 
25 dmtape.?bin      102297 VM/370 hang during IPL (TIO BUSY loop) Y N Y  none    1-2-3
   dmtape.Abin      072498 Minor architectural corrections        Y Y N
26 dm3172.Abin      111197 LAN3172 Enhancement..                  Y Y Y  none    1-2-3
27 LAN3172.DOC      010598 Added more examples                    Y N N  none    8
28 dmxcasdlc.Abin   011698 WAN3172 fix for leased line PU 2       Y N N  none    1-2-3
   dmxcasdlc.Bbin   110899 X.21 Leased line support for WAN3172   Y Y Y  None    1-2-3
   WAN3172.DOC      110899 X.21 Leased line support for WAN3172   Y Y Y  None    8

29 AWS34XX.DOC      030598 Clarifications and remove restriction  Y N Y  none    8

30 emul3215.Abin    032798 Fixes TPF msg problems (mult lines)    Y N Y  node    1-2-3  
   dm3215.Bbin      111600 Linux/390 fixes for AWS3215            Y Y N  None    1-2-3
   emul3215.Bbin    111600 Linux/390 fixes for AWS3215            Y Y N  None    1-2-3
   dm3215.Cbin      031601 General Enhancements                   Y Y N  None    1-2-3
   emul3215.Cbin    031601 General Enhancements                   Y Y N  None    1-2-3
   AWS3215.DOC      031601 General Enhancements                   Y Y N  None    8

31 tn3270d.Cbin     052098 AWS3274 Cons hangs, drops, or prog702  Y Y N  
   tn3270d.Dbin     101999 LU Name support for TN3270E clients    Y Y Y  
32 AWS3900.MCP      090298 P/390 370 LIC patch 1.29               Y Y N  none    10 
33 AWS39X0.MCP      090298 P/390 ESA LIC patch 1.29               Y Y N  none    10   
34 licupdte         090298 Script used to apply LIC patchs        N/A    N/A     N/A 

35 dmoma.Abin       102198 AWSOMA Bug when tdf file has no EOL    Y Y N  None    1-2-3
                           Now converts to lower case if MOUNT or 
                           awsmount fileme not found
   dmoma.Bbin       060999 AWSOMA Bug on VMFPLC2 RUN command      Y Y N

36 r390.Abin        102698 Fixes awscnf path restrictions         Y Y N  None    1-2-3
   r390.Bbin        010699 Prevent mult configs, misc enhancments Y Y N 
   r390.Cbin        020899 AWSICE start prob with certain LOCALE  Y Y N 

37 awscfg.Abin      102698 Fixes awscnf path restrictions         Y Y N  None    1-2-3
   awscfg.Bbin      020899 Save devmap.bu in CONFIG_FILE path     Y Y N 

38 startcon         111198 Changed X3270/XANT target to locahost  Y Y N  None    8
39 awsoia.Abin      010699 Fixed Disabled wait, occasional abend  Y Y N  22E     1-2-3
40 dmerror.cat      010699 Latest messages                        Y Y N  None    11

41 stop390.Abin     020899 Occasional crash on "End P/390" on 4.3 Y Y N  None    1-2-3
42 AWSTerm1.Abin    020899 Occasional crash on "End P/390" on 4.3 Y Y N  None    1-2-3
43 AWSTerm.Bbin     020899 Occasional crash on "End P/390" on 4.3 Y Y N  None    1-2-3










Special Instructions: 
---------------------

Running this version of "dasd" and "dm34xx" requires starting them as a user 
process in the ipl390 script. (earlier versions are started as kernel) 

1) Edit the ipl390 script and search for AWSFBA and AWS34XX.  Comment 			
   the kernel sections by inserting a # on these lines:

# ******************************************************************************
#  Note: AWSFBA (dasd) can be started as a USER process if needed (see below)  *
#        If started as a USER process, the following 4 lines must be commented *
# ******************************************************************************
# $DMDIR/AWSStart dasd
# if [ "$?" != 0 ]
# then
#   echo "* FBA DASD device manager failed to start.  Please report this problem."
# fi

# $DMDIR/AWSStart    dm34xx
# if [ "$?" != 0 ]
# then
#   echo "* AWS34XX SCSI Tape device manager failed to start.  Please report this problem."
# fi

2) Search for "Initialize USER processes Only".  

3) Add "$DMDIR/dm34xx &" after the "Initialize USER processes Only"

# ***************************************************************************
# Initialize USER processes Only
# ***************************************************************************

$DMDIR/dm34xx &

4) Enable the user section for AWSFBA by removing the # from the line 
containing "$DMDIR/dasd &" 


# ********************************************************************************
#  Note: AWSFBA (dasd) can be started as a KERNEL process if needed (see above)  *
#        If started as a KERNEL process, the following line must be commented    *
# ********************************************************************************
$DMDIR/dasd &

