# Creating a standby hot-spare drive

Use this action to create a standby hot-spare drive.

1. In the tree, click (ready physical drive) or (hot-spare drive).
2. Right-click Create standby hot-spare drive. The ServeRAID Manager creates the standby hot-spare drive.

## More information

- Choosing to create a standby hot-spare drive
- RAID levels that can use a hot-spare or standby hot-spare drive

Glossary | Index | Contents

x-0310-SRM-00-00-EN