# Novell NetWare considerations

Note to test and NLS: This help panel is still in draft. Do not write defects on this panel or translate the content.

(NetWare 5.x only) If you are preparing to install Novell NetWare 5.x from the startable Novell NetWare 5.x CD, set the write-cache mode only to write-through mode.

Attention: Do not attempt a hot-replace operation on Windows 2000 or NetWare by hot-removing a failed controller and then hot-adding a new controller. Loss of data can occur. If a controller fails on these operating systems, you must shut down the server to replace the controller.

Glossary | Index | Contents

x-1039-SRM-00-00-EN