# Could not set the SCSI initiator ID for controller [number].

## Explanation:

A hardware error occurred.

## Action:

1. Verify that the controller, cables, and physical drives are installed properly.
2. Verify that there is power to the physical drives.
3. Retry the command.
4. If the command still fails, restart the server and retry the command.

5. If the problem persists, contact your IBM service representative.

Note: (Cluster and failover environment only) Verify that the cable from the second system (for clustering) or controller (for failover) is disconnected from the SCSI backplane.

Glossary | Index | Contents

x-0069-SRM-00-00-EN