# Confirming your system configuration

Use the configuration summary to review all the changes that the ServeRAID Manager will apply to your configuration:

1. Review the information that is displayed in the "Configuration summary" window. To change the configuration, click Modify arrays or Modify logical drives.

   Notes:
     1. You can expand the tree for another view of the configuration.
     2. Additional notes and attentions regarding the configuration appear in the event viewer.
     3. Some operating systems have size limitations for logical drives. Before you save the configuration, verify that the size of the logical drive is appropriate for your operating system. For more detailed information, see your operating-system documentation.
2. Click Apply; then, click Yes when asked if you want to apply the new configuration. The configuration is saved in the ServeRAID controller and in the physical drives.

   Note: If you clicked Automatically initialize new logical drives, the ServeRAID Manager will initialize the logical drives automatically.

3. If you have multiple controllers, complete the following steps:
   1. In the tree, click the ServeRAID controller that you want to configure.
   2. Right-click Configure RAID. The Configuration wizard opens.
   3. Choose Express or Custom configuration and continue through the Configuration wizard for each controller.
4. When you have completed configuring your controllers, you can change certain controller settings to fine-tune your configuration.

## More information

- Configuration wizard notes and attentions
- Understanding logical-drive synchronization
- Initializing a logical drive
- Fine-tuning your system

Glossary | Contents

x-0704-SRM-00-04-EN