# Battery controller [number] has exceeded normal operating temperature.

## Explanation:

Battery temperature has exceeded 50 degrees Celsius.

## Action:

Check operating environment: verify that the controller is installed properly, that the server has adequate ventilation, and so on. If the problem persists, the battery may be bad or the server may have a problem. Contact your service representative.

Glossary | Contents

x-0084-SRM-04-00-EN