# Deleting a hot-spare drive

Note: This action is supported on the integrated RAID controller in startable-CD mode only.

Use this action to delete a hot-spare physical drive from your configuration.

1. In the tree, click (hot-spare physical drive).
2. Right-click Delete hot-spare drive. The ServeRAID Manager deletes the hot-spare drive from the configuration by setting the drive state to ready. If you have removed the drive from the server, the ServeRAID Manager removes the drive from the configuration.

Glossary | Contents

x-0336-SRM-00-02-EN