# Deleting a standby hot-spare drive

Note: This action is not supported on the integrated RAID controller.

Use this action to delete a standby hot-spare physical drive from your configuration.

1. In the tree, click (standby hot-spare physical drive).
2. Right-click Delete hot-spare drive. The ServeRAID Manager deletes the standby hot-spare drive from the configuration by setting the drive state to ready. If you have physically removed the drive, the Manager removes the drive from the configuration.

Glossary | Contents

x-0316-SRM-00-02-EN