# This hot-spare drive will not work for any defined array.

# None of the logical drives in the specified array support hot-spare drives.

# The hot-spare drive on controller {0}, channel {1}, SCSI ID {2} is too small to support the array. Replace the specified drive with a larger drive.

## Explanation:

This hot-spare drive will not work for any defined array because of one of the following:

- None of the existing arrays support hot-spare drives.
- The hot-spare drive must have the same capacity as or larger capacity than the smallest physical drive in the array.
- If any of the physical drives in your arrays fail, the specified hot-spare drive cannot replace the failed drive.

## Action:

Remove the specified hot-spare drive and add a drive of the appropriate size.

Glossary | Contents

x-0039-SRM-00-02-EN