# Software and hardware support of RAID levels

RAID level | ServeRAID software* release that supports the RAID level | Hardware levels that support the RAID level
0 | All | ServeRAID on the board, ServeRAID, ServeRAID-II, ServeRAID-3 family, ServeRAID-4 family, ServeRAID-5i, ServeRAID-6M
1 | All | ServeRAID on the board, ServeRAID, ServeRAID-II, ServeRAID-3 family, ServeRAID-4 family, ServeRAID-5i, ServeRAID-6M, integrated RAID controller
1E | All | ServeRAID on the board, ServeRAID, ServeRAID-II, ServeRAID-3 family, ServeRAID-4 family, ServeRAID-5i, ServeRAID-6M
5 | All | ServeRAID on the board, ServeRAID, ServeRAID-II, ServeRAID-3 family, ServeRAID-4 family, ServeRAID-5i, ServeRAID-6M
5E | ServeRAID 3.50 or later | ServeRAID-3 and ServeRAID-4 families.
5EE | ServeRAID 6.00 or later | ServeRAID-4 family except ServeRAID-4H, ServeRAID-6M
x0 | ServeRAID 4.00 or later | ServeRAID-4 family, ServeRAID-5i, ServeRAID-6M

* ServeRAID software refers to BIOS, firmware, device drivers, programs, and so forth.

Glossary | Contents

x-1061-SRM-00-04-EN