# SCSI channel [number] object

Use this object to work with a specified SCSI channel or to display its properties by clicking a specific SCSI channel from the menu.

Notes:
  1. A controller supports a maximum of four SCSI channels.
  2. The ServeRAID-5i controller does not support tape drives and physical drives on the same channel.

## Possible subobject

- (Physical drive)
- (Enclosure)
- (CD-ROM drive)
- (Tape drive)

## Warning and error conditions

- (warning) is displayed if any subobject has a warning or error condition.
- (error) is displayed if all of its subobjects have an error condition.
- (SCSI channel) is displayed if all of its subobjects have no warning or error conditions.

## Actions

- Scan for new or removed ready drives
- Identify all physical drives on SCSI channel [number]

The following action is available only in startable-CD mode:

- Change the SCSI transfer speed

Glossary | Contents

x-0210-SRM-00-03-EN