# SCSI channel [number] on an LSI 1030 object

Use this object to work with a specified SCSI channel or to display its properties by clicking a specific SCSI channel from the menu.

Note: A controller supports a maximum of four SCSI channels.

## Possible subobject

- (Physical drive on an LSI 1030)
- (Enclosure)
- (CD-ROM drive)
- (Tape drive)

## Warning and error conditions

- (warning) is displayed if any subobject has a warning or error condition.
- (error) is displayed if all of its subobjects have an error condition.
- (SCSI channel) is displayed if all of its subobjects have no warning or error conditions.

## Actions

- Identify all physical drives on SCSI channel [number]

Glossary | Contents

x-0227-SRM-00-02-EN