The Kernel Kit Table of Contents | The Kernel Kit Index

# System Information

Declared in: be/kernel/OS.h

Library: libroot.so

The following functions, types, and structures convey information about the system, such as the number of CPUs, when the kernel was built, and whether your computer is on fire.

## System Info Functions

### get_system_info()

status_t `get_system_info(system_info` *info`)`

The `get_system_info()` function tells you more than you want to know about the physical capacities of your computer and other statistics of your operating system. The function copies this information into the `system_info` argument info. You must allocate info before passing it in.

RETURN CODES

`get_system_info()` always returns `B_OK`.

### is_computer_on()

int32`is_computer_on(`void`)`

Returns 1 if the computer is on. If the computer isn't on, the value returned by this function is undefined.

### is_computer_on_fire()

double`is_computer_on_fire(`void`)`

Returns the temperature of the motherboard if the computer is currently on fire. If the computer isn't on fire, the function returns some other value.

## System Info Structures and Constants

### cpu_info

typedef struct { `bigtime_t` active_time; } `cpu_info`

The `cpu_info` structure provides information about your computer's CPU(s). You retrieve the structure by looking in the cpu_infos field of the `system_info` structure. The cpu_infos field is an array that contains one `cpu_info` structure for each CPU on your motherboard.

Field | Meaning
`active_time` | The number of microseconds the CPU has spent doing useful work (i.e. not busy waiting) since the machine was booted.

### cpu_type

typedef enum `cpu_types` { B_CPU_PPC_601, B_CPU_PPC_603, B_CPU_PPC_603e, B_CPU_PPC_604, B_CPU_PPC_604e, B_CPU_PPC_750, B_CPU_PPC_686, B_CPU_AMD_29K, B_CPU_X86, Obsolete B_CPU_MC6502, B_CPU_Z80, B_CPU_ALPHA, B_CPU_MIPS, B_CPU_HPPA, B_CPU_M68K, B_CPU_ARM, B_CPU_SH, B_CPU_SPARC, B_CPU_INTEL_X86 = 0x1000, B_CPU_INTEL_PENTIUM, B_CPU_INTEL_PENTIUM75, B_CPU_INTEL_PENTIUM_486_OVERDRIVE, B_CPU_INTEL_PENTIUM_MMX, B_CPU_INTEL_PENTIUM_MMX_MODEL_4, B_CPU_INTEL_PENTIUM_MMX_MODEL_8, B_CPU_INTEL_PENTIUM75_486_OVERDRIVE, B_CPU_INTEL_PENTIUM_PRO, B_CPU_INTEL_PENTIUM_II, B_CPU_INTEL_PENTIUM_II_MODEL_3, B_CPU_INTEL_PENTIUM_II_MODEL_5, B_CPU_INTEL_CELERON, B_CPU_INTEL_PENTIUM_III, B_CPU_AMD_X86 = 0x1100, B_CPU_AMD_K5_MODEL0, B_CPU_AMD_K5_MODEL1, B_CPU_AMD_K5_MODEL2, B_CPU_AMD_K5_MODEL3, B_CPU_AMD_K6_MODEL6, B_CPU_AMD_K6_MODEL7, B_CPU_AMD_K6_MODEL8, B_CPU_AMD_K6_2, B_CPU_AMD_K6_MODEL9, B_CPU_AMD_K6_III, B_CPU_AMD_ATHLON_MODEL1, B_CPU_CYRIX_X86 = 0x1200, B_CPU_CYRIX_GXm, B_CPU_CYRIX_6x86MX, B_CPU_IDT_X86 = 0x1300, B_CPU_IDT_WINCHIP_C6, B_CPU_IDT_WINCHIP_2, B_CPU_RISE_X86 = 0x1400, B_CPU_RISE_mP6 } `cpu_type`;

| The `B_X86_CPU` constant is obsolete. All x86 CPUs are represented by specific vendor/model constants.

These constants represents different CPU vendors and models. To retrieve the constant that represents the CPU(s) that your computer uses, look in the cpu_type field of the `system_info` structure.

Note that the x86 types are grouped by vendor, where the vendor is identified by the high word, and the model by the low word. Each vendor has its own `cpu_type` constant, as indicated by the explicit values in the list above. If you're only interested in the vendor, mask the `cpu_type` value with `B_CPU_X86_VENDOR_MASK`, thus:

       system_info sysinfo;
       get_system_info( &sysinfo );

       switch ( sysinfo.cpu_type & B_CPU_X86_VENDOR_MASK ) {
          case B_CPU_INTEL_X86: ...
          case B_CPU_AMD_X86: ...
          case B_CPU_CYRIX_x86: ...
          case B_CPU_IDT_X86: ...
          case B_CPU_RISE_X86: ...
          default:
          /* Not x86. */
       }

### B_CPU_X86_VENDOR_MASK

`B_CPU_X86_VENDOR_MASK`

You mask your machine's `cpu_type` value with this constant to retrieve the CPU's vendor id (which is also a `cpu_type` value). If the CPU isn't an breed of x86, applying the mask will yield 0. See the `cpu_type` description for an example.

### machine_id

typedef int32 `machine_id`[2]; Currently unused

`machine_id` is a 64-bit number (encoded as two 32-bit numbers) that uniquely identifies this specific computer. The id number is returned as the id field (currently unused) of the `system_info` structure.

### B_MAX_CPU_COUNT

`B_MAX_CPU_COUNT`

This constant is set to the maximum number of CPUs that the BeOS can take advantage of. The number is machine-dependent.

### platform_type

typedef enum `platform_types` { B_BEBOX_PLATFORM = 0, B_MAC_PLATFORM, B_AT_CLONE_PLATFORM, B_ENIAC_PLATFORM, B_APPLE_II_PLATFORM, B_CRAY_PLATFORM, B_LISA_PLATFORM, B_TI_994A_PLATFORM, B_TIMEX_SINCLAIR_PLATFORM, B_ORAC_1_PLATFORM, B_HAL_PLATFORM, B_BESM_6_PLATFORM, B_MK_61_PLATFORM, B_NINTENDO_64_PLATFORM } `platform_type`;

These constants represent the various computer platforms that the BeOS does, has, should, might, or might not run on. To retrieve the constant for the machine that you're running on, look in the platform_type field of the `system_info` structure.

### system_info

typedef struct { `machine_id` id; Currently unused `bigtime_t` boot_time; int32 cpu_count; `cpu_type` cpu_type; int32 cpu_revision; `cpu_info` cpu_infos[`B_MAX_CPU_NUM`]; int64 cpu_clock_speed; int64 bus_clock_speed; `platform_type` platform_type; int32 max_pages; int32 used_pages; int32 page_faults; int32 max_sems; int32 used_sems; int32 max_ports; int32 used_ports; int32 max_threads; int32 used_threads; int32 max_teams; int32 used_teams; char kernel_name[`B_FILE_NAME_LENGTH`]; char kernel_build_date[`B_OS_NAME_LENGTH`]; char kernel_build_time[`B_OS_NAME_LENGTH`]; int64 kernel_version; } `system_info`;

The `system_info` structure describes your computer's hardware and operating system, and provides information about the availability of kernel resources (such as threads and ports). You retrieve a system_info structure through the `get_system_info()` function.

Field | Meaning
id | A 64-bit number (encoded as two `int32`s) that uniquely identifies this machine. Currently unsed.
boot_time | The time at which the computer was last booted, measured in microseconds since January 1st, 1970. You can also get this information through `system_time()`.
cpu_count | The number of CPUs on your computer's motherboard.
cpu_type | A constant that represents the CPU(s) make and model.
cpu_revision | The revision number of the CPU(s).
cpu_infos | An array of `cpu_info` structures, one for each CPU.
cpu_clock_speed | The speed (in Hz) at which the CPU(s) operate.
bus_clock_speed | The speed (in Hz) at which the bus operates.
platform_type | The platform type constant that reprsents your computer.
max_resource used_resource | These fields give the total number of RAM pages, semaphores, and so on, that the system can create, and the number that are currently in use.
page_faults | The number of times the system has read a page of memory into RAM due to a page fault.
kernel_name | The filename of the kernel (the leaf name, not the path).
kernel_build_date | Fixed-width string that gives the date that the kernel was built; for example:
       Jun  5 1999
kernel_build_time Fixed-width string that gives the time of day that the kernel was built; for example: 10:02:16
kernel_version A Be-assigned number that identifies the kernel version.

The Kernel Kit Table of Contents | The Kernel Kit Index

The B e Book,
...in lovely HTML...
for BeOS Release 5.

Copyright © 2000 Be, Inc. All rights reserved..