megs: 16
romimage: file=../BIOS-bochs-latest
vgaromimage: file=../VGABIOS-elpin-2.40

boot: disk

floppy_bootsig_check: disabled=0
#floppya: 1_2="floppy.img", status=inserted

ata0: enabled=1, ioaddr1=0x1f0, ioaddr2=0x3f0, irq=14
ata0-master: type=disk, mode=flat, translation=auto, path="hd.img", cylinders=900, heads=15, spt=17, biosdetect=auto, model="Generic 1234"
ata1: enabled=0
ata2: enabled=0
ata3: enabled=0

parport1: enabled=0
parport2: enabled=0

com1: enabled=0
com2: enabled=0
com3: enabled=0
com4: enabled=0
usb1: enabled=0

i440fxsupport: enabled=0
vga_update_interval: 40000
vga: extension=none
cpu: count=1, ips=1000000, reset_on_triple_fault=1
text_snapshot_check: enabled=0
private_colormap: enabled=0
clock: sync=realtime, time0=938581955

ne2k: enabled=0
pnic: enabled=0
sb16: enabled=0

user_shortcut: keys=ctrl-alt-del

log: -
logprefix: %t%e%d
debugger_log: -
panic: action=ask
error: action=report
info: action=report
debug: action=ignore
pass: action=fatal
keyboard_type: mf
keyboard_serial_delay: 250
keyboard_paste_delay: 100000
keyboard_mapping: enabled=0, map=
user_shortcut: keys=none
mouse: enabled=0, type=ps2
