SYSPARAM        - SYSTEM PARAMETERS                              22-AUG-1978 00:20:19   VAX-11 MACRO X0.3-11               Page   0

TABLE OF CONTENTS   



   (1)      41  DECLARATIONS

   (1)      62  SYSTEM TIME VARIABLES

   (1)      73  SYSGEN PARAMETERS	

   (1)     139  CONTROL PARAMETERS	

   (1)     164  TERMINAL DRIVER SYSTEM PARAMETERS

SYSPARAM        - SYSTEM PARAMETERS                              22-AUG-1978 00:20:19   VAX-11 MACRO X0.3-11               Page   1

00                                                                                                                               (1)



                                     0000     1 	.TITLE	SYSPARAM - SYSTEM PARAMETERS

                                     0000     2 	.IDENT	/00/

                                     0000     3 

                                     0000     4 ;

                                     0000     5 ; COPYRIGHT (C) 1978

                                     0000     6 ; DIGITAL EQUIPMENT CORPORATION, MAYNARD, MASSACHUSETTS 01754

                                     0000     7 ;

                                     0000     8 ; THIS SOFTWARE IS FURNISHED  UNDER A LICENSE FOR USE ONLY ON A SINGLE

                                     0000     9 ; COMPUTER  SYSTEM AND  MAY BE  COPIED ONLY WITH  THE INCLUSION OF THE

                                     0000    10 ; ABOVE COPYRIGHT NOTICE.  THIS SOFTWARE, OR ANY OTHER COPIES THEREOF,

                                     0000    11 ; MAY NOT BE PROVIDED OR  OTHERWISE MADE AVAILABLE TO ANY OTHER PERSON

                                     0000    12 ; EXCEPT FOR USE ON SUCH SYSTEM AND TO ONE WHO AGREES TO THESE LICENSE

                                     0000    13 ; TERMS.  TITLE TO AND  OWNERSHIP OF THE  SOFTWARE  SHALL AT ALL TIMES

                                     0000    14 ; REMAIN IN DEC.

                                     0000    15 ;

                                     0000    16 ; THE INFORMATION IN THIS SOFTWARE IS SUBJECT TO CHANGE WITHOUT NOTICE

                                     0000    17 ; AND SHOULD  NOT BE CONSTRUED  AS A COMMITMENT  BY DIGITAL  EQUIPMENT

                                     0000    18 ; CORPORATION.

                                     0000    19 ;

                                     0000    20 ; DEC ASSUMES  NO  RESPONSIBILITY  FOR  THE USE OR  RELIABILITY OF ITS

                                     0000    21 ; SOFTWARE ON EQUIPMENT WHICH IS NOT SUPPLIED BY DEC.

                                     0000    22 ;

                                     0000    23 

                                     0000    24 ;++

                                     0000    25 ; FACILITY:  EXECUTIVE DATA BASE

                                     0000    26 ;

                                     0000    27 ; ABSTRACT:

                                     0000    28 ;	SYSPARAM CONTAINS THE EXECUTIVE CONTROL PARAMETERS AND CERTAIN

                                     0000    29 ;	KEY VARIABLES.

                                     0000    30 ;

                                     0000    31 ; ENVIRONMENT:  

                                     0000    32 ;

                                     0000    33 ; AUTHOR:  R. I. HUSTVEDT, CREATION DATE:  09-OCT-1977

                                     0000    34 ;

                                     0000    35 ; MODIFIED BY:

                                     0000    36 ;

                                     0000    37 ; C. A. MONIA, : VERSION 00

                                     0000    38 ; 01	- 	MODIFIED FOR STAND-ALONE SYSTEM

                                     0000    39 ;--

SYSPARAM        - SYSTEM PARAMETERS                              22-AUG-1978 00:20:19   VAX-11 MACRO X0.3-11               Page   2

00              DECLARATIONS                                                                                                     (1)



                                     0000    41 	.SBTTL	DECLARATIONS

                                     0000    42 ;

                                     0000    43 ; INCLUDE FILES:

                                     0000    44 ;

                                     0000    45 	$TTDEF				; DEFINE TERMINAL CHARACTERISTICS

                                     0000    46 

                                     0000    47 ;

                                     0000    48 ; MACROS:

                                     0000    49 ;

                                     0000    50 

                                     0000    51 ;

                                     0000    52 ; EQUATED SYMBOLS:

                                     0000    53 ;

                                     0000    54 

                                     0000    55 ;

                                     0000    56 ; OWN STORAGE:

                                     0000    57 ;

                                 00000000    58 	.PSECT	$$$017,PAGE		; PAGE ALIGNED

                                     0000    59 EXE$A_SYSPARAM::			; SYSTEM PARAMETER BASE

                                     0000    60 

SYSPARAM        - SYSTEM PARAMETERS                              22-AUG-1978 00:20:19   VAX-11 MACRO X0.3-11               Page   3

00              SYSTEM TIME VARIABLES                                                                                            (1)



                                     0000    62 	.SBTTL	SYSTEM TIME VARIABLES

                                     0000    63 ;

                                     0000    64 ;		SYSTEM TIME VARIABLES

                                     0000    65 ;

                                     0000    66 EXE$GQ_TODCBASE::			; TIME OF DAY CLOCK BASE (BOOT TIME)

                           80FBC500  0000    67 	.LONG	^X80FBC500		; 100 NANO-SECOND UNITS

                           00859034  0004    68 	.LONG	^X00859034		; INITIAL TIME 4-JAN-1978 09:58

                                     0008    69 ;

                                     0008    70 EXE$GL_TODR::				; TIME OF DAY REGISTER VALUE CORRESPONDING

                           11C24C88  0008    71 	.LONG	^X11C24C88		; TO EXE$GQ_TODCBASE

SYSPARAM        - SYSTEM PARAMETERS                              22-AUG-1978 00:20:19   VAX-11 MACRO X0.3-11               Page   4

00              SYSGEN PARAMETERS                                                                                                (1)



                                     000C    73 	.SBTTL	SYSGEN PARAMETERS	

                                     000C    74 ;

                                     000C    75 ;	SYSGEN PARAMETERS

                                     000C    76 ;

                                     000C    77 SGN$GW_BALSETCT::			; MAXIMUM BALANCE SET COUNT

                               0000' 000C    78 	.WORD	SGN$C_BALSETCNT		;

                                     000E    79 

                                     000E    80 SGN$GW_DFPFC::				; DEFAULT PAGE FAULT CLUSTER

                               0010  000E    81 	.WORD	16			; 

                                     0010    82 

                                     0010    83 SGN$GW_GBLSECNT::			; MAXIMUM COUNT OF GLOBAL SECTIONS

                               0000' 0010    84 	.WORD	SGN$C_GBLSECCNT		;

                                     0012    85 

                                     0012    86 SGN$GW_MAXGPGCT::			; MAXIMUM COUNT OF GLOBAL PAGES

                               0000' 0012    87 	.WORD	SGN$C_MAXGPGCNT		;

                                     0014    88 

                                     0014    89 SGN$GW_MAXPRCCT::			; MAXIMUM PROCESS COUNT

                               0000' 0014    90 	.WORD	SCH$C_MAXPIX		;

                                     0016    91 

                                     0016    92 SGN$GW_MAXPSTCT::			; GUARANTEED COUNT OF PST ENTRIES

                               0000' 0016    93 	.WORD	SGN$C_MAXPSTCNT		;

                                     0018    94 

                                     0018    95 SGN$GW_MAXPIX::				; MAXIMUM PROCESS INDEX

                               0000' 0018    96 	.WORD	SCH$C_MAXPIX		;

                                     001A    97 

                                     001A    98 SGN$GW_MAXVPGCT::			; MAXIMUM VIRTUAL ADDRESS SPACE

                               0000' 001A    99 	.WORD	SGN$C_MAXVPGCNT		;

                                     001C   100 

                                     001C   101 SGN$GW_MINWSCNT::			; MINIMUM WORKING SET COUNT

                               0000' 001C   102 	.WORD	SGN$C_MINWSCNT		;

                                     001E   103 

                                     001E   104 SGN$GW_NPROCS::				; MAXIMUM PROCESSES

                               0000' 001E   105 	.WORD	SGN$C_NPROCS		;

                                     0020   106 

                                     0020   107 SGN$GW_PAGFILCT::			; COUNT OF ALLOWED PAGING FILES

                               0000  0020   108 	.WORD	0			;

                                     0022   109 

                                     0022   110 SGN$GW_PFLIBAS::			; PAGE FAULT INDEX BASE

                               0000  0022   111 	.WORD	0			;

                                     0024   112 

                                     0024   113 SGN$GW_SFTMAX::				; NUMBER OF SWAP FILE TABLE SLOTS

                               0000' 0024   114 	.WORD	SGN$C_SFTMAX		; 

                                     0026   115 

                                     0026   116 SGN$GW_SYSVECPG::			; COUNT OF SYSTEM VECTOR PAGES

                               0000' 0026   117 	.WORD	SGN$C_SYSVECPGS		;

                                     0028   118 

                                     0028   119 SGN$GW_SYSDWSCT::			; DEFAULT SYSTEM WORKING SET COUNT

                               0000' 0028   120 	.WORD	SGN$C_SYSDWSCNT		;

                                     002A   121 

                                     002A   122 SGN$GW_SYSWSCNT::			; MAX SYSTEM WORKING SET SIZE

                               0000' 002A   123 	.WORD	SGN$C_SYSWSCNT		;

                                     002C   124 

                                     002C   125 	.ALIGN	LONG			; LONGWORDS ON LONGWORD BOUNDARY

                                     002C   126 SGN$GL_IRPCNT::				; COUNT OF I/O PACKETS TO ALLOCATE

                           0000000A  002C   127 	.LONG	10			; (S)WAG

                                     0030   128 SGN$GL_MAXWSCNT::			; MAXIMUM WORKING SET COUNT

                           00000100  0030   129 	.LONG	256			; 

SYSPARAM        - SYSTEM PARAMETERS                              22-AUG-1978 00:20:19   VAX-11 MACRO X0.3-11               Page   5

00              SYSGEN PARAMETERS                                                                                                (1)



                                     0034   130 SGN$GL_MAXWSREQ::			; MAXIMUM WORKING SET REQUEST

                           00000100  0034   131 	.LONG	256			;

                                     0038   132 

                                     0038   133 SGN$GL_NPAGEDYN::			; NON-PAGED POOL SIZE

                           00000000' 0038   134 	.LONG	SGN$C_NPAGEDYN		;

                                     003C   135 SGN$GL_PAGEDYN::			; PAGED DYNAMIC POOL

                           00000000' 003C   136 	.LONG	SGN$C_PAGEDYN		;

                                     0040   137 

SYSPARAM        - SYSTEM PARAMETERS                              22-AUG-1978 00:20:19   VAX-11 MACRO X0.3-11               Page   6

00              CONTROL PARAMETERS                                                                                               (1)



                                     0040   139 	.SBTTL	CONTROL PARAMETERS	

                                     0040   140 ;

                                     0040   141 ;	GENERAL SYSTEM CONTROL PARAMETERS

                                     0040   142 ;

                                     0040   143 SCH$GW_QUAN::				; PROCESS QUANTUM

                               FFE2  0040   144 	.WORD	-30			; 30 * 10MS TICKS

                                     0042   145 ;

                                     0042   146 ;	MODIFIED PAGE WRITER CONTROL PARAMETERS

                                     0042   147 ;

                                     0042   148 MPW$AW_INITVAL::

                               0008  0042   149 	.WORD	8			;MODIFIED PAGE LIST CLUSTER SIZE

                               0018  0044   150 	.WORD	24			;MODIFIED PAGE LIST HIGH THRESHOLD

                               000C  0046   151 	.WORD	12			;MODIFIED PAGE LIST LOW THRESHOLD

                                     0048   152 

                                     0048   153 	.ALIGN	LONG			;

                                     0048   154 ;

                                     0048   155 ;	PERMANENT DEFAULT SYSTEM FLAGS

                                     0048   156 ;

                                     0048   157 EXE$GL_DEFFLAGS::			;

                                     0048   158 	.LONG	<1@EXE$V_SYSPAGING>-	; ENABLE SYSTEM CODE PAGING

                                     0048   159 		!<1@EXE$V_POOLPGING>-	; ENABLE SYSTEM POOL PAGING

                                     0048   160 		!<1@EXE$V_SBIERR>-	; SBI ERROR DETECTION

                           00000001' 0048   161 		!<1@EXE$V_FATAL_BUG>	; FATAL BUG CHECKS

                                     004C   162 

SYSPARAM        - SYSTEM PARAMETERS                              22-AUG-1978 00:20:19   VAX-11 MACRO X0.3-11               Page   7

00              TERMINAL DRIVER SYSTEM PARAMETERS                                                                                (1)



                                     004C   164 	.SBTTL	TERMINAL DRIVER SYSTEM PARAMETERS

                                     004C   165 ;

                                     004C   166 ; DIALUP SUPPORT

                                     004C   167 ;

                                     004C   168 TTY$GL_DELTA::				; DELTA TIME FOR DIALUP TIMER

                           00989680  004C   169 	.LONG	100000*100		; 1 SEC

                                     0050   170 TTY$GB_DIALTYP::			; FLAGS FOR DIALUP TIMER SERACH

                                 00  0050   171 	.BYTE	0			; 0 IS NORMAL, 1 FOR UK

                                     0051   172 ;

                                     0051   173 ; NOTE ALIGNMENT!

                                     0051   174 ;

                                     0051   175 ; REMOTE TERMINAL CANONICAL CHARACTERISTICS

                                     0051   176 ; THESE CHARACTERISTICS ARE SET FOR TERMINALS WITH "TT$M_REMOTE" SET

                                     0051   177 ; WHEN THE TERMINAL LINE IS INITIALIZED.

                                     0051   178 ;

                                     0051   179 TTY$GB_DEFSPEED::			; DEFAULT SPEED FOR TERMINALS

                                 06' 0051   180 	.BYTE	TT$C_BAUD_300		; 300 BAUD

                                     0052   181 TTY$GW_DEFBUF::				; DEFAULT BUFFER SIZE

                               0084  0052   182 	.WORD	132			;

                                     0054   183 TTY$GL_DEFCHAR::			; DEFUALT CHARACTERISTICS

                           100022A0' 0054   184 	.LONG	<16@24>+TT$M_LOWER+TT$M_REMOTE+TT$M_TTSYNC+TT$M_WRAP

                                     0058   185 ;

                                     0058   186 ; END OF TERMINAL SYSTEM PARAMETERS

                                     0058   187 ;

                                     0058   188 ;

                                     0058   189 

                                     0058   190 ;

                                     0058   191 ;  RMS DEFAULT PARAMETERS

                                     0058   192 ;

                           00000059  0058   193 SYS$GB_DFMBC::		.BLKB	1	; DEFAULT MULTI-BLOCK COUNT

                           0000005A  0059   194 SYS$GB_DFMBFSDK::	.BLKB	1	; DEFAULT MULTI-BUFFER COUNT SEQ. DISK

                           0000005B  005A   195 SYS$GB_DFMBFSMT::	.BLKB	1	; DEFAULT MULTI-BUFFER COUNT MAGTAPE

                           0000005C  005B   196 SYS$GB_DFMBFSUR::	.BLKB	1	; DEFAULT MULTI-BUFFER COUNT UNIT REC.

                           0000005D  005C   197 SYS$GB_DFMBFREL::	.BLKB	1	; DEFAULT MULTI-BUFFER COUNT RELATIVE

                           0000005E  005D   198 SYS$GB_DFMBFIDX::	.BLKB	1	; DEFAULT MULTI-BUFFER COUNT INDEXED

                           0000005F  005E   199 SYS$GB_DFMBFHSH::	.BLKB	1	; DEFAULT MULTI-BUFFER COUNT HASHED

                                     005F   200 		.ALIGN	LONG

                                     0060   201 ;

                                     0060   202 ;  END OF RMS DEFAULT PARAMETERS

                                     0060   203 ;

                                     0060   204 

                           00000060  0060   205 EXE$C_SYSPARSZ==.-EXE$A_SYSPARAM	; SIZE OF SYSTEM PARAMETERS

                                     0060   206 

                                     0060   207 	.END

SYSPARAM        - SYSTEM PARAMETERS                              22-AUG-1978 00:20:19   VAX-11 MACRO X0.3-11               Page   8

SYMBOL TABLE                                                                                                                     (1)



BIT...         = 00000008            TT$C_BAUD_134  = 00000004            TT$_LA36       = 00000020            

EXE$A_SYSPARAM   00000000 RG    03   TT$C_BAUD_150  = 00000005            TT$_LAX        = 00000020            

EXE$C_SYSPARSZ = 00000060  G         TT$C_BAUD_1800 = 00000009            TT$_UNKNOWN    = 00000000            

EXE$GL_DEFFLAGS  00000048 RG    03   TT$C_BAUD_2000 = 0000000A            TT$_VT05       = 00000001            

EXE$GL_TODR      00000008 RG    03   TT$C_BAUD_2400 = 0000000B            TT$_VT52       = 00000040            

EXE$GQ_TODCBASE  00000000 RG    03   TT$C_BAUD_300  = 00000006            TT$_VT55       = 00000041            

EXE$V_FATAL_BUG  ********   X   03   TT$C_BAUD_3600 = 0000000C            TT$_VT5X       = 00000040            

EXE$V_POOLPGING  ********   X   03   TT$C_BAUD_4800 = 0000000D            TTY$GB_DEFSPEED  00000051 RG    03   

EXE$V_SBIERR     ********   X   03   TT$C_BAUD_50   = 00000001            TTY$GB_DIALTYP   00000050 RG    03   

EXE$V_SYSPAGING  ********   X   03   TT$C_BAUD_600  = 00000007            TTY$GL_DEFCHAR   00000054 RG    03   

GBL...         = 00000000            TT$C_BAUD_7200 = 0000000E            TTY$GL_DELTA     0000004C RG    03   

MPW$AW_INITVAL   00000042 RG    03   TT$C_BAUD_75   = 00000002            TTY$GW_DEFBUF    00000052 RG    03   

SCH$C_MAXPIX     ********   X   03   TT$C_BAUD_9600 = 0000000F            

SCH$GW_QUAN      00000040 RG    03   TT$M_CRFILL    = 00000400            

SGN$C_BALSETCNT  ********   X   03   TT$M_EIGHTBIT  = 00008000            

SGN$C_GBLSECCNT  ********   X   03   TT$M_ESCAPE    = 00000008            

SGN$C_MAXGPGCNT  ********   X   03   TT$M_HOLDSCREEN= 00004000            

SGN$C_MAXPSTCNT  ********   X   03   TT$M_HOSTSYNC  = 00000010            

SGN$C_MAXVPGCNT  ********   X   03   TT$M_LFFILL    = 00000800            

SGN$C_MINWSCNT   ********   X   03   TT$M_LOWER     = 00000080            

SGN$C_NPAGEDYN   ********   X   03   TT$M_MBXDSABL  = 00010000            

SGN$C_NPROCS     ********   X   03   TT$M_MECHTAB   = 00000100            

SGN$C_PAGEDYN    ********   X   03   TT$M_NOBRDCST  = 00020000            

SGN$C_SFTMAX     ********   X   03   TT$M_NOECHO    = 00000002            

SGN$C_SYSDWSCNT  ********   X   03   TT$M_NOTYPEAHD = 00000004            

SGN$C_SYSVECPGS  ********   X   03   TT$M_ODD       = 00000080            

SGN$C_SYSWSCNT   ********   X   03   TT$M_PAGE      = FE000000            

SGN$GL_IRPCNT    0000002C RG    03   TT$M_PARITY    = 00000040            

SGN$GL_MAXWSCNT  00000030 RG    03   TT$M_PASSALL   = 00000001            

SGN$GL_MAXWSREQ  00000034 RG    03   TT$M_REMOTE    = 00002000            

SGN$GL_NPAGEDYN  00000038 RG    03   TT$M_SCOPE     = 00001000            

SGN$GL_PAGEDYN   0000003C RG    03   TT$M_SCRIPT    = 00000040            

SGN$GW_BALSETCT  0000000C RG    03   TT$M_TTSYNC    = 00000020            

SGN$GW_DFPFC     0000000E RG    03   TT$M_WRAP      = 00000200            

SGN$GW_GBLSECNT  00000010 RG    03   TT$S_PAGE      = 00000008            

SGN$GW_MAXGPGCT  00000012 RG    03   TT$V_CRFILL    = 0000000A            

SGN$GW_MAXPIX    00000018 RG    03   TT$V_EIGHTBIT  = 0000000F            

SGN$GW_MAXPRCCT  00000014 RG    03   TT$V_ESCAPE    = 00000003            

SGN$GW_MAXPSTCT  00000016 RG    03   TT$V_HOLDSCREEN= 0000000E            

SGN$GW_MAXVPGCT  0000001A RG    03   TT$V_HOSTSYNC  = 00000004            

SGN$GW_MINWSCNT  0000001C RG    03   TT$V_LFFILL    = 0000000B            

SGN$GW_NPROCS    0000001E RG    03   TT$V_LOWER     = 00000007            

SGN$GW_PAGFILCT  00000020 RG    03   TT$V_MBXDSABL  = 00000010            

SGN$GW_PFLIBAS   00000022 RG    03   TT$V_MECHTAB   = 00000008            

SGN$GW_SFTMAX    00000024 RG    03   TT$V_NOBRDCST  = 00000011            

SGN$GW_SYSDWSCT  00000028 RG    03   TT$V_NOECHO    = 00000001            

SGN$GW_SYSVECPG  00000026 RG    03   TT$V_NOTYPEAHD = 00000002            

SGN$GW_SYSWSCNT  0000002A RG    03   TT$V_ODD       = 00000007            

SYS$GB_DFMBC     00000058 RG    03   TT$V_PAGE      = 00000019            

SYS$GB_DFMBFHSH  0000005E RG    03   TT$V_PARITY    = 00000006            

SYS$GB_DFMBFIDX  0000005D RG    03   TT$V_PASSALL   = 00000000            

SYS$GB_DFMBFREL  0000005C RG    03   TT$V_REMOTE    = 0000000D            

SYS$GB_DFMBFSDK  00000059 RG    03   TT$V_SCOPE     = 0000000C            

SYS$GB_DFMBFSMT  0000005A RG    03   TT$V_SCRIPT    = 00000006            

SYS$GB_DFMBFSUR  0000005B RG    03   TT$V_TTSYNC    = 00000005            

TT$C_BAUD_110  = 00000003            TT$V_WRAP      = 00000009            

TT$C_BAUD_1200 = 00000008            TT$_LA120      = 00000021            

SYSPARAM        - SYSTEM PARAMETERS                              22-AUG-1978 00:20:19   VAX-11 MACRO X0.3-11               Page   9

PROGRAM SECTION SYNOPSIS                                                                                                         (1)







PROGRAM SECTION SYNOPSIS



.  ABS  .        00000000      00     NOPIC   USR   CON   ABS   LCL NOSHR NOEXE NORD  NOWRT BYTE  

. BLANK .        00000000      01     NOPIC   USR   CON   REL   LCL NOSHR   EXE   RD    WRT BYTE  

$ABS$            00000000      02     NOPIC   USR   CON   ABS   LCL NOSHR   EXE   RD    WRT BYTE  

$$$017           00000060      03     NOPIC   USR   CON   REL   LCL NOSHR   EXE   RD    WRT PAGE  





THERE WERE NO ERRORS OR WARNINGS.

24124. BYTES LEFT IN FREE MEMORY POOL.

OBJ$:SYSPARAM,LIS$:SYSPARAM/-SP=LIB$:LIB/ML,SRC$:SYSPARAM

2 MLB DIR RDS - 136 GETS TO DEFINE 9 MACROS. 10 INTER. FILE WRITES. 

