# Motorola® PR860 Customer Programming Software

### Table of Contents

1. Introduction

2. What's new in this release

3. Requirements

4. Installation, removal

5. Important notes

6. Legal notice

### 1. Introduction

Welcome to the Motorola PR860 Customer Programming Software (CPS) for the PR860 radios.

### 2. What's new in this release

Version | Notes
R01.05 | Supports application feature registration for 20/25 kHz Channel Bandwidth capability by the common EID which is also shared with other CPS platforms.
R01.04 | Supports 12.5 kHz only. 20/25 kHz Channel Bandwidth capability is available via application features. Please contact Motorola customer service for details.
R01.03 | Support Firmware R05.13.04 and above.
R01.02 | Support non-standard DPL code. Fixed Voice Storage issue.
R01.01 | Support for the PR860 radios.
R01.00 | Support for basic and expert view.
| Drag and drop support between models.
| Support for renaming personalities, systems, and lists.
| Support for multiple selection configuration. For example, create several MDC systems and select them all in the treeview and set the Primary ID of all the MDC systems to the same value at once.
| Support for copying the receive frequency, with an optional user defined offset, to the transmit frequency.
| Supports per user settings for the preference settings and the dealer information fields printed on the customer handout report.

### 3. Requirements

Operating System | Required Patches
Microsoft® Windows® XP Microsoft® Windows® Vista Microsoft® Windows® 7 Microsoft® Windows® 8 |

Hardware Recommendations
· The application takes approximately 16 MB of free disk space on your PC. However, you may want more space to allow you to save archive files of your radios. Each archive file varies in size depending on the features of the radio that are enabled. A good rule of thumb is 75 KB per archive file.
· For processor speed and RAM, nothing is required beyond the recommendations given by Microsoft for the release of the operating system that you are using.
· The graphical user interface is best displayed using 1024*768 and 65536 color display or better (use small font).
· A CD-ROM drive.
· A serial port or USB to serial port adapter. The BAFO(R) BF-810 USB to serial port adapter has been tested successfully with the CPS application.

### 4. Installation, Removal

#### Installation

You need to have Administrator rights on the target PC in order to install the software if you are running Microsoft Windows XP, Microsoft Windows Vista, Microsoft Windows 7, or Microsoft Windows 8.

Proceed as follows:

- Insert the CD-ROM containing the installation into the CD-ROM drive.
- If the installation application doesn't start within 30 seconds, the auto-run feature for CD-ROMs for you operating system is likely disabled. Browse to your CD-ROM and run the autorun.exe program. For example, if the E:\ drive is the CD-ROM, run E:\autorun.exe.

#### Removal

From the Start button on the task bar of your operating system, select Settings > Control Panel. Select the Add/Remove Programs option within the control panel. Select the PR860 Customer Programming Software item in the "Currently installed programs" box and click the remove button.

### 5. Important Notes

The following behaviors are known problems with the latest release of the Motorola PR860 CPS.

- If the display setting's font size is set to "Custom setting" instead of "Small Fonts" or "Large Fonts" the Toolbar and Conventional Personalities folder may not display properly.
- The installation doesn't set the default path to save archive files and therefore the user will need to migrate to the directory of their choosing the first time they save a file.
- For Windows 8 OS support，need install .NET Framework 3.5 automatically on line as following picture showing:

  'Control Panel' -> 'Programs' -> 'Programs and Features' -> 'Turn Windows features on or off' -> enable the checkbox '.NET Framework 3.5 (includes .NET 2.0 and 3.0)' and its 2 sub checkboxes.

  This action can be implemented before or after CPS installing. Then Launch CPS, CPS can work normally.

### 6. Legal notice

Microsoft® and Windows® are registered trademarks of Microsoft Inc.
Motorola® is a registered trademark of Motorola Solutions, Inc.
BAFO® is a registered trademark of BAFO Technologies, Inc.
This product includes software developed by the Apache Software Foundation (http://www.apache.org/).