6 Pin Hirose Connector
----------------------

![pinout](pic/6_pin_hirose_female_receptacle_pinout.png)

View:

* Female receptacle viewed from mating face
* Male plug solder cups viewed from assembly face

Pinout map / wire color map:

* 1 - RED (N/C)
* 2 - GRN (DATA)
* 3 - YEL (SENSE)
* 4 - BLK (GND)
* 5 - WHT (N/C)
* 6 - BLU (N/C)

6 Pin Male Plug Hirose P/N: HR10A-7P-6P(73)

Hirose Cable Retention Crimp Tool P/N: HR10A-TC-02

AC100
-----

* 6 pin male plug Hirose to 6 pin male plug Hirose cable
* Wired straight through (pin 1 to pin 1, pin 2 to pin 2, etc)
* Pins 1, 5, and 6 are electrically connected in the cable assembly, however are not connected inside the KFDtool adapter

AC101
-----

* 6 pin male plug Hirose pigtail
* Pins 1, 5, and 6 are electrically connected in the cable assembly, however are not connected inside the KFDtool adapter
