================================================================
Professional Radio - Customer Programming Software R04.00.00
================================================================

Known CPS Issues:
----------------  

1) If your PC is running the first release of Microsoft Windows 95
   and Internet Explorer has not been installed, you may experience
   problems in installing and running the CPS due to certain
   components of the operating system being out of date.

   To eliminate this problem two Microsoft patches have been included
   on the CPS CD. If you experience any problems under Windows 95,
   please go to the CD and run:
     /Win95Patches/40comupd.exe
     /Win95Patches/dcom95.exe
   and then re-install the CPS. 
 
2) On some PCs, the CPS may abnormally terminate if Print Preview
   is attempted on the Print Custom screen. This problem only occurs
   when Print All is selected. This problem has been observed on 
   Compaq Windows 98 computers with the following programs running:
      * Easy Access Internet Program (cpqEasyAcc.exe)
      * Compaq Internet Watchdog Program (watchdog.exe)
   If this CPS function is to be used, it is recommended that these 
   programs be removed from the PC startup.  

3) When the tree view is printed some nodes may overlap on the
   printout and an extra blank page may be printed. This issue
   is more likely to occur on large codeplug configurations.   

4) The true value of "Max Ans. Mode Record Duration (sec)" in the
   radio will be approximately four seconds less than the value
   shown by the CPS.


Major CPS Enhancements:
-----------------------

1) Support for four line display models

2) Custom PL codes
Non-standard frequencies can be directly entered in 0.1Hz steps.

3) CPS access password protection
Prevent a radio or file from being read until the correct password
has been entered (LS Trunking, 4-line display and mobile models only).

4) LS Trunking Site file import/export

5) Support for 800MHz Portable radios

6) Radio firmware version display

7) Support for new Portable features
When using portable radios with firmware R03.00.00 or greater the
following features are now available:
 - Keypad Lock Password
 - Emergency Open Mic
 - MDC Message
 - MDC Status

8) Support for new Mobile features
When using mobile radios with firmware R03.00.00 or greater the
following features are now available:
 - Emergency Alarm/Call
 - Emergency cycles
 - Emergency Decode
 - Emergency Remote Monitor
 - Answer Machine mode
 - Remote Monitor
 

Programming Hints:
------------------

1) It should be noted that a new/added conventional personality 
   must be assigned to a zone/channel position. To add a zone to 
   a radio click the "+" in a Personality Assignment to Zone 
   Window. To add a conventional personality to the radio, click 
   the "+" on a Conventional Personality Window. To add an 
   additional conventional personality to a zone go to the 
   Personality Assignment to Zone:Channel window for the 
   desired zone.  Click the right mouse key within the channel 
   table to add a conventional personality entry. Please read 
   the CPS help for additional information. 

2) Speed Dial buttons should not be programmed to the P1, P2, and
   P3 buttons on radios, which overlay these buttons with the menu 
   navigation keys. The speed dial buttons will not operate 
   in this configuration because the buttons function as the menu
   navigation keys when phone mode is entered. 

3) When adding a new conventional personality, verify that the
   bandwidth selected on the Conventional Personality screen is 
   correct.  Incorrect selections will lead to poor radio 
   performance.   


