==================================================================================================

 SOFTWARE RELEASE NOTE

==================================================================================================

Product  : Unofficial Lab Firmware and Codeplugs for Lab FlashGrade Tool
Release  : R03.14.00
Date     : 02-September-2010
Language : English

==================================================================================================

 PURPOSE OF THE RELEASE

==================================================================================================
- Supported unofficial model number:
  
  Model Number   Tanapa Number   Version   Description
  -------------------------------------------------------------------------------- 
  H25KDN9AN8     PMUD14SPA       07.00     waris vhf GP1280 convert to special GP380
  H25RDN9AN8     PMUE14SPA       07.00     waris uhf GP1280 convert to special GP380



- New supported model number:
  
  Model Number   Tanapa Number   Version   Description
  -------------------------------------------------------------------------------- 
  H38SDH9AN6	 PMUE2791B	 07.00	   Min epp waterproof 450-527M pref fu
  H38SDF9AN5	 PMUE2781B	 07.00	   Min epp waterproof 450-527M pref li
  H38SDC9AN3	 PMUE2790B	 07.00	   Min epp waterproof 450-527M pop uhf
  H25BEC9AN3     PMUB1015B	 07.00     waris 29.7-42M pop LB1 band  
  H25CEC9AN3     PMUB1028B	 07.00	   waris 35-50M pop LB2 band
  H25BEH9AN6     PMUB1042B	 07.00	   waris 29.7-42M pref LB1 band  
  H25CEH9AN6     PMUB1043B	 07.00	   waris 35-50M pref LB2 band   



- Supported model number:

  Model Number   Tanapa Number   Version   Description
  --------------------------------------------------------------------------------
  H25KDC9AN0	 PMUD1492C	 07.00	   Laz plain-minus vhf band              
  H25SDC4AN3	 PMUE1484D	 07.00     Laz EPP POPULAR UHF2(INDIA 12.5KHz
  H25SDC9AN3	 PMUE1484D	 07.00	   Laz EPP POPULAR UHF2              
  H25SDH9AN6	 PMUE1485D	 07.00	   Laz EPP PREFERRED UHF2            
  H25SDH4AN6	 PMUE1485D	 07.00	   Laz EPP PREFERRED UHF2(INDIA 12.5K
  H38SDC9AN3	 PMUE1819D	 07.00	   Min EPP POPULAR UHF2               
  H38SDH9AN6	 PMUE1820D	 07.00	   Min EPP PREFERRED Full Keypad UHF2 
  H25BEC9AN3	 PMUB1015A	 07.00	   waris 29.7-42M pop LB1 band           
  H25BEH9AN6	 PMUB1042A	 07.00	   waris 29.7-42M pref LB1 band          
  H25CEC9AN3	 PMUB1028A	 07.00	   waris 35-50M pop LB2 band             
  H25CEH9AN6	 PMUB1043A	 07.00	   waris 35-50M pref LB2 band            
  H25EDC9AN3	 PMUD1546A	 07.00	   waris 300-350M pop 300 band           
  H25KCC4AN3	 PMUD1974A	 07.00	   Laz atex 136-174M pop vhf band        
  H25KCC4AN3	 PMUD1974B	 07.00	   Laz atex GP340(GP329) pop vhf band    
  H25KCC6AN3	 PMUD2050A	 07.00	   Laz atex 136-174M pop vhf band        
  H25KCC6AN3	 PMUD2050B	 07.00	   Laz atex GP340(GP329) pop vhf band    
  H25KCH4AN6	 PMUD1973A	 07.00	   Laz atex 136-174M pref vhf band       
  H25KCH4AN6	 PMUD1973B	 07.00	   Laz atex GP380(GP339) pref vhf band   
  H25KCH6AN6	 PMUD2049A	 07.00	   Laz atex 136-174M pref vhf band       
  H25KCH6AN6	 PMUD2049B	 07.00	   Laz atex GP380(GP339) pref vhf band   
  H25KDC4AN3	 PMUD1488C	 07.00	   Laz epp 136-174M pop vhf band         
  H25KDC9AN0	 PMUD1492A	 07.00	   waris plain-minus 136-174M vhf band   
  H25KDC9AN0	 PMUD1492B	 07.00	   Laz plain-minus 136-174M vhf band     
  H25KDC9AN2	 PMUD2318A	 07.00	   Laz epp GP330 4ch plain vhf band        
  H25KDC9AN3	 PMUD1488A	 07.00	   waris 136-174M pop vhf band           
  H25KDC9AN3	 PMUD1488B	 07.00	   Laz 136-174M pop vhf band             
  H25KDC9AN3	 PMUD1488C	 07.00	   Laz epp 136-174M pop vhf band         
  H25KDF9AN5	 PMUD1490A	 07.00	   waris 136-174M pref limited kp vhf ban
  H25KDF9AN5	 PMUD1490B	 07.00	   Laz 136-174M pref limited kp vhf band 
  H25KDF9AN5	 PMUD1490C	 07.00	   Laz epp 136-174M pref limited kp vhf b
  H25KDH4AN6	 PMUD1489C	 07.00	   Laz epp 136-174M pref vhf band        
  H25KDH9AN6	 PMUD1489A	 07.00	   waris 136-174M pref vhf band          
  H25KDH9AN6	 PMUD1489B	 07.00	   Laz 136-174M pref vhf band            
  H25KDH9AN6	 PMUD1489C	 07.00	   Laz epp 136-174M pref vhf band        
  H25RCC4AN3	 PMUE2218B	 07.00	   Laz atex 403-470M pop uhf band        
  H25RCC4AN3	 PMUE2218C	 07.00	   Laz epp atex 403-470M pop uhf band    
  H25RCC4AN3	 PMUE2218E	 07.00	   Laz atex GP340(GP329) pop uhf band   
  H25RCC6AN3	 PMUE2258B	 07.00	   Laz atex 403-470M pop uhf band        
  H25RCC6AN3	 PMUE2258C	 07.00	   Laz epp atex 403-470M pop uhf band    
  H25RCC6AN3	 PMUE2258E	 07.00	   Laz epp atex GP340(GP329) pop uhf band
  H25RCH4AN6	 PMUE2217B	 07.00	   Laz atex 403-470M pref uhf band       
  H25RCH4AN6	 PMUE2217C	 07.00	   Laz epp atex 403-470M pref uhf band   
  H25RCH4AN6	 PMUE2217E	 07.00	   Laz epp atex GP380(GP339) pref uhf ban
  H25RCH6AN6	 PMUE2257B	 07.00	   Laz atex 403-470M pref uhf band       
  H25RCH6AN6	 PMUE2257C	 07.00	   Laz epp atex 403-470M pref uhf band   
  H25RCH6AN6	 PMUE2257E	 07.00	   Laz epp atex GP380(GP339) pref uhf ban
  H25RDC4AN3	 PMUE1440C	 07.00	   Laz epp 403-470M pop uhf band         
  H25RDC4AN3	 PMUE1440D	 07.00	   Laz epp 403-470M pop uhf band         
  H25RDC9AN0	 PMUE1443A	 07.00	   waris plain-minus 403-470M uhf band   
  H25RDC9AN0	 PMUE1443B	 07.00	   Laz plain-minus 403-470M uhf band     
  H25RDC9AN0	 PMUE1443C	 07.00	   Laz plain-minus 403-470M uhf band     
  H25RDC9AN2	 PMUE2878A	 07.00	   Laz epp GP330 4ch plain uhf band        
  H25RDC9AN3	 PMUE1440A	 07.00	   waris 403-470M pop uhf band           
  H25RDC9AN3	 PMUE1440B	 07.00	   Laz 403-470M pop uhf band             
  H25RDC9AN3	 PMUE1440C	 07.00	   Laz epp 403-470M pop uhf band         
  H25RDC9AN3	 PMUE1440D	 07.00	   Laz epp 403-470M pop uhf band         
  H25RDF9AN5	 PMUE1444A	 07.00	   waris 403-470M pref limited kp uhf ban
  H25RDF9AN5	 PMUE1444B	 07.00	   Laz 403-470M pref limited kp uhf band 
  H25RDF9AN5	 PMUE1444C	 07.00	   Laz epp 403-470M pref limited kp uhf b
  H25RDF9AN5	 PMUE1444D	 07.00	   Laz epp 403-470M pref limited kp uhf b
  H25RDH4AN6	 PMUE1441C	 07.00	   Laz epp 403-470M pref uhf band        
  H25RDH4AN6	 PMUE1441D	 07.00	   Laz epp 403-470M pref uhf band        
  H25RDH9AN6	 PMUE1441A	 07.00	   waris 403-470M pref uhf band          
  H25RDH9AN6	 PMUE1441B	 07.00	   Laz 403-470M pref uhf band            
  H25RDH9AN6	 PMUE1441C	 07.00	   Laz epp 403-470M pref uhf band        
  H25RDH9AN6	 PMUE1441D	 07.00	   Laz epp 403-470M pref uhf band        
  H25SDC4AN3	 PMUE1484C	 07.00	   Laz epp 450-527M pop uhf2 band        
  H25SDC9AN3	 PMUE1484A	 07.00	   waris 450-527M pop uhf2 band          
  H25SDC9AN3	 PMUE1484B	 07.00	   Laz 450-527M pop uhf2 band            
  H25SDC9AN3	 PMUE1484C	 07.00	   Laz epp 450-527M pop uhf2 band        
  H25SDH4AN6	 PMUE1485C	 07.00	   Laz epp 450-527M pref uhf2 band       
  H25SDH9AN6	 PMUE1485A	 07.00	   waris 450-527M pref uhf2 band         
  H25SDH9AN6	 PMUE1485B	 07.00	   Laz 450-527M pref uhf2 band           
  H25SDH9AN6	 PMUE1485C	 07.00	   Laz epp 450-527M pref uhf2 band       
  H25TDC9AN3	 PMUE2950A	 07.00	   GP340 DE 450-470 MHZ 4W NK/P PW502C   
  H25TDC9AN3	 PMUE2950B	 07.00	   GP340 DE 450-470 MHZ 4W NK/P PW502C   
  H25TDF9AN5	 PMUE2956A	 07.00	   GP360 DE 450-470 MHZ 4W LK/P PW502F   
  H25TDF9AN5	 PMUE2956B	 07.00	   GP360 DE 450-470 MHZ 4W LK/P PW502F   
  H25TDH9AN6	 PMUE2951A	 07.00	   GP380 DE 450-470 MHZ 4W K/P PW502H    
  H25TDH9AN6	 PMUE2951B	 07.00	   GP380 DE 450-470 MHZ 4W K/P PW502H    
  H38KDC9AN3	 PMUD1742B	 07.00	   Min 136-174M pop vhf band          
  H38KDC9AN3	 PMUD1742C	 07.00	   Min epp 136-174M pop vhf band      
  H38KDC9AN3	 PMUD2242A	 07.00	   Min epp waterproof 136-174M pop vhf
  H38KDF9AN5	 PMUD2236A	 07.00	   Min epp waterproof 136-174M pref li
  H38KDH9AN6	 PMUD1743B	 07.00	   Min 136-174M pref full kp vhf band 
  H38KDH9AN6	 PMUD1743C	 07.00	   Min epp 136-174M pref full kp vhf b
  H38KDH9AN6	 PMUD2243A	 07.00	   Min epp waterproof 136-174M pref fu
  H38RDC9AN3	 PMUE1817B	 07.00	   Min 403-470M pop uhf band          
  H38RDC9AN3	 PMUE1817C	 07.00	   Min epp 403-470M pop uhf band      
  H38RDC9AN3	 PMUE1817D	 07.00	   Min epp 403-470M pop uhf band      
  H38RDC9AN3	 PMUE2788A	 07.00	   Min epp waterproof 403-470M pop uhf
  H38RDC9AN3	 PMUE2788B	 07.00	   Min epp waterproof 403-470M pop uhf
  H38RDF9AN5	 PMUE2779A	 07.00	   Min epp waterproof 403-470M pref li
  H38RDF9AN5	 PMUE2779B	 07.00	   Min epp waterproof 403-470M pref li
  H38RDH9AN6	 PMUE1818B	 07.00	   Min 403-470M pref full kp uhf band 
  H38RDH9AN6	 PMUE1818C	 07.00	   Min epp 403-470M pref full kp uhf b
  H38RDH9AN6	 PMUE1818D	 07.00	   Min epp 403-470M pref full kp uhf b
  H38RDH9AN6	 PMUE2789A	 07.00	   Min epp waterproof 403-470M pref fu
  H38RDH9AN6	 PMUE2789B	 07.00	   Min epp waterproof 403-470M pref fu
  H38SDC9AN3	 PMUE1819B	 07.00	   Min 450-527M pop uhf2 band         
  H38SDC9AN3	 PMUE1819C	 07.00	   Min epp 450-527M pop uhf2 band     
  H38SDC9AN3	 PMUE2790A	 07.00	   Min epp waterproof 450-527M pop uhf
  H38SDF9AN5	 PMUE2781A	 07.00	   Min epp waterproof 450-527M pref li
  H38SDH9AN6	 PMUE1820B	 07.00	   Min 450-527M pref full kp uhf2 band
  H38SDH9AN6	 PMUE1820C	 07.00	   Min epp 450-527M pref full kp uhf2 
  H38SDH9AN6	 PMUE2791A	 07.00	   Min epp waterproof 450-527M pref fu
  H38TDC9AN3	 PMUE2946A	 07.00	   GP344 DE 450-470 MHZ 4W NK/P PMW502C  
  H38TDC9AN3	 PMUE2957A	 07.00	   GP344R DE 450-470 MHZ 4W NKP PMR502C  
  H38TDF9AN5	 PMUE2958A	 07.00	   GP366R DE 450-470 MHZ 4W LKP PMR502F  
  H38TDH9AN6	 PMUE2947A	 07.00	   GP388 DE 450-470 MHZ 4W K/P PMW502H   
  H38TDH9AN6	 PMUE2959A	 07.00	   GP388R DE 450-470 MHZ 4W KP PMR502H   


=======================================================================================


REQUIRED EQUIPMENT


For the usage of this software the following radio accessories are required:

    - Flash adapter, P/N HLN9742A or B
    and (i)
    - Radio Interface Box, P/N RLN4008
      with battery or power supply
    - RIB to PC cable, P/N 3080369B72 (9pin) or 3080369B71 (25pin)
    - Programming/test cable, P/N RKN4074 (GP3xx, GP6xx, GP12xx)
    - Programming/test cable, P/N JMKN4123 (GP344, GP388, GP346)
    or (ii)
    -  RIBless programming cable, P/N RKN4075 (GP3xx, GP6xx, GP12xx)

    By using equipment (i) the Flash adapter has to be connected between the 
    Radio Interface Box and the Programming/test cable. Maximum baud rate for 
    this equipment is 19,200 Bd.

    By using equipment (ii) the Flash adapter has to be connected between the 
    PC and the RIBless programming cable.

    For Flash Adapter HLN9742A, "Flash mode on" means switch position "ON".

    For Flash Adapter HLN9742B, "Flash mode on" means switch position "A", 
    position "B" is not used for portable flashing.



=======================================================================================

RADIO SOFTWARE RELEASE NOTE

=======================================================================================
Release waris5t-R03.14.00

==================
Build Environment
==================

- The Lab firmware and codeplugs are converted on a Dell Optiplex 745 PC with HxD 1.7.6.6