===========================================================

 SOFTWARE RELEASE NOTE

===========================================================

Product  : Unofficial Lab Firmware and Codeplugs for Lab FlashGrade Tool
KIT No   : ENVN4019A
Release  : R01.00.20 Lab Phase 1
Date     : 09-Nov-2002
Language : English

===========================================================

 PURPOSE OF THE RELEASE
 
===========================================================
FIXES THE FOLLOWING ISSUES:
 
- This kit is for repairing dead radios,with a Phase 1 or 2 Codeplug inside!

HINTS:

- If a radio will not work, after you´ve forgotten to program the Phase 3 codeplug
  into the radio,before flashing the Phase 3 firmware,flash this firmware.
- After this load a Phase 3 codeplug and program the radio first before you flash 
  a Phase 3 Firmware.


===========================================================
For the usage of this software the following radio accessories are required:

    - Flash adapter, P/N HLN9742A or B
    and (i)
    - Radio Interface Box, P/N RLN4008
      with battery or power supply
    - RIB to PC cable, P/N 3080369B72 (9pin) or 3080369B71 (25pin)
    - Programming/test cable, P/N RKN4074 (GP3xx, GP6xx, GP12xx)
    - Programming/test cable, P/N MDJMKN4123 (GP344, GP388)
    or (ii)
    -  RIBless programming cable, P/N RKN4075 (GP3xx, GP6xx, GP12xx)

    By using equipment (i) the Flash adapter has to be connected between the 
    Radio Interface Box and the Programming/test cable. Maximum baud rate for 
    this equipment is 19,200 Bd.

    By using equipment (ii) the Flash adapter has to be connected between the 
    PC and the RIBless programming cable.

    For Flash Adapter HLN9742A, "Flash mode on" means switch position "ON".

    For Flash Adapter HLN9742B, "Flash mode on" means switch position "A", 
    position "B" is not used for portable flashing.


Associated Part Numbers :

Description

WARIS  Portable PLAIN-MINUS LAZARUS / POPULAR / PREFERRED Radios

SUPERTANAPAs Supported :-
Description                                  Sales Model NO      SUPERTANAPA
GP320            PLAIN-MINUS VHF       	      H25KDC9AN0          PMUD1492A      
GP320            PLAIN-MINUS UHF       	      H25RDC9AN0          PMUE1443A      
GP320		 LAZARUS PLAIN-MINUS VHF      H25KDC9AN0          PMUD1492B      
GP320		 LAZARUS PLAIN-MINUS UHF      H25RDC9AN0	  PMUE1443B      

GP340(GP329)     POPULAR LB1           	      H25BEC9AN3          PMUB1015A      
GP340(GP329)     POPULAR LB2           	      H25CEC9AN3          PMUB1028A      
GP340(GP329)     POPULAR VHF           	      H25KDC9AN3          PMUD1488A      
GP340(GP329)     LAZARUS POPULAR VHF   	      H25KDC9AN3          PMUD1488B      
GP340(GP329)     POPULAR 300           	      H25EDC9AN3          PMUD1546A         
GP340(GP329)     POPULAR UHF           	      H25RDC9AN3          PMUE1440A      
GP340(GP329)     LAZARUS POPULAR UHF   	      H25RDC9AN3          PMUE1440B      
GP340(GP329)     POPULAR UHF2          	      H25SDC9AN3          PMUE1484A      
GP340(GP329)     ATEX   POPULAR UHF    	      H25RCC9AN3          PMUE2218A      
GP340(GP329)     ATEX   POPULAR VHF           H25KCC9AN3          PMUD1974A      
GP340(GP329)     LAZARUS POPULAR UHF2  	      H25SDC9AN3          PMUE1484B      
GP340(GP329)     LAZARUS ATEX POPULAR VHF     H25KCC4AN3          PMUD1974B      
GP340(GP329)     LAZARUS ATEX POPULAR VHF     H25KCC6AN3          PMUD2050B      
GP340(GP329)     LAZARUS ATEX POPULAR UHF     H25RCC4AN3          PMUE2218B      
GP340(GP329)     LAZARUS ATEX POPULAR UHF     H25RCC6AN3          PMUE2258B      
GP346(GP329Plus) MINNOW POPULAR VHF           H38KDC9AN3          PMUD1742B      
GP346(GP329Plus) MINNOW POPULAR UHF    	      H38RDC9AN3          PMUE1817B      
GP346(GP329Plus) MINNOW POPULAR UHF2   	      H38SDC9AN3          PMUE1819B      

GP360            PREFERRED VHF         	      H25KDF9AN5          PMUD1490A      
GP360            LAZARUS PREFERRED VHF 	      H25KDF9AN5          PMUD1490B      
GP360            PREFERRED  UHF               H25RDF9AN5          PMUE1444A      
GP360            LAZARUS    PREFERRED UHF     H25RDF9AN5          PMUE1444B      


GP380(GP339)     PREFERRED LB1         	      H25BEH9AN6          PMUB1042A      
GP380(GP339)     PREFERRED LB2         	      H25CEH9AN6          PMUB1043A      
GP380(GP339)     PREFERRED VHF                H25KDH9AN6          PMUD1489A      
GP380(GP339)     LAZARUS PREFERRED VHF        H25KDH9AN6          PMUD1489B      
GP380(GP339)     PREFERRED UHF         	      H25RDH9AN6          PMUE1441A      
GP380(GP339)     LAZARUS PREFERRED UHF 	      H25RDH9AN6          PMUE1441B      
GP380(GP339)     PREFERRED UHF2               H25SDH9AN6          PMUE1485A      
GP380(GP339)     ATEX PREFERRED UHF    	      H25RCH9AN6          PMUE2217A      
GP380(GP339)     ATEX PREFERRED VHF    	      H25KCH9AN6          PMUD1973A      
GP380(GP339)     LAZARUS PREFERRED UHF2       H25SDH9AN6          PMUE1485B      
GP380(GP339)     LAZARUS ATEX PREFFERED VHF   H25KCH4AN6          PMUD1973B      
GP380(GP339)     LAZARUS ATEX PREFFERED VHF   H25KCH6AN6	  PMUD2049B      
GP380(GP339)     LAZARUS ATEX PREFFERED UHF   H25RCH4AN6	  PMUE2217B      
GP380(GP339)     LAZARUS ATEX PREFFERED UHF   H25RCH6AN6	  PMUE2257B      


GP386(GP339Plus) MINNOW PREFERRED VHF  	      H38KDH9AN6          PMUD1743B      
GP386(GP339Plus) MINNOW PREFERRED UHF  	      H38RDH9AN6          PMUE1818B      
GP386(GP339Plus) MINNOW PREFERRED UHF2 	      H38SDH9AN6          PMUE1820B      


==================
Build Environment
==================

- The Lab firmware and codeplugs are converted on a Siemens Scenic 860 series PC 
  with Hexworkshop 3.11
