==============================================================
            MTR2000 RSS Version R03.02.05
==============================================================
This RSS version works with the MTR2000 Station Software 
Version R01.00.000, R02.00.000, R02.02.001, R02.02.002, 
R02.03.002, R03.01.001, R03.01.003, R03.01.004, R03.01.006,
R03.01.007, R03.02.003, R03.02.005, R03.02.006, R03.02.007 

Run the program setup.exe on disk 1 under windows to install the
RSS files to your harddisk.

==============================================================
RSS updates: RSS R03.02.05 Enhancements over release R03.02.03
==============================================================
- Enhancement to default Main Standby wildcard file functionality.
  The affected files are main.wcd and standby.wcd
- RSS functionality has been validated under Windows 98
  (the Windows 95 restrictions given below apply under Windows 98)
- Miscellaneous revisions to the helpfiles.
==============================================================
Known RSS limitations:
==============================================================
Known differences running the MTR2000 RSS under Windows 95 
- All non editable fields appear in light grey
- Windows 95 links are not handled from the File Load/Save dialog
- Long filenames are not supported by the RSS
- Some lists enable a scrollbar, because a different font is used
Help differences under Windows 95
- Shown Pictures in help reflect Windows 3.1 appearance e.g. 
  title bar, icons in desktop, ...
- Context help for X button missing (new close button in title bar
  for Windows 95)


==============================================================
The following options are available in the RSS but are
not supported by the Station Software:
==============================================================
- 2nd Receiver connected         (Station Configuration)
- Audio Source                   (Channel Information->Audio)
- Remote Control Type-DC;-Binary (Wireline)
- External PTT Mapping entries 
  ('Aux. Audio & Receiver' and 'Call Sign') (Channel Information PTT)

end
---