Filename: REDFISH_X10_314.bin  version: 3.14  Date: 08-27-2015

Support Motherboard: X10DRU-I+, X10DRT-P, X10DRG-H, X10DRW-I, X10DRI-T4+, X10DDW-I,
					 X10DRFR, X10DRI-T, X10DRFF, X10DRT-HIBF, X10DRFR-T, X10DRD,
					 X10DRD-L, X10SRH
1.  Category: fix                                                                 
    Description:                                                                  
       Remove debug message against Systems/1   
    Affected functions:                                                         
    Validation :                                                                  
        1.verify Systems/1 with LSI enabled.

2.  Category: enhancement                                                                 
    Description:                                                                  
       Present all EthernetInterface members against Systems/1/EthernetInterfaces
    Affected functions:                                                         
    Validation :                                                                  
        1.verify Systems/1/EthernetInterfaces and its child path.

3.  Category: fix                                                                 
    Description:                                                                  
        [65010] Redfish API doens't push event to webserver       
    Affected functions:                                                         
    Validation :                                                                  
        1.Do factory default
        2.Create an event sbuscription with destination point to the webserver
        3.Remove platform FAN to generate an event.
        4.Check with your webserver's reaction.
        
========================================================================================	
Filename: REDFISH_X10_313.bin  version: 3.13  Date: 08-26-2015

Support Motherboard: X10DRU-I+, X10DRT-P, X10DRG-H, X10DRW-I, X10DRI-T4+, X10DDW-I,
					 X10DRFR, X10DRI-T, X10DRFF, X10DRT-HIBF, X10DRFR-T, X10DRD,
					 X10DRD-L, X10SRH

1.  Category: fix                                                                 
    Description:                                                                  
       [64881] [Redfish FW 3.12] Fail To Use Active Directory To Log In Redfish↵          
        API.                                                                     
    Affected functions:                                                         
    Validation :                                                                  
        1.use AD account to login redfish service.					 
					 
2. 	Category: New                                                                 
    Description:                                                                  
        X10SRH support redfish service.                                                                
    Affected functions:                                                         
    Validation :                                                                  

3.  Category: Fix
    Description:
       [64832] Missing MB_10G Temp in IPMI Web GUI with REDFISH 3.12.

    Infected motherboard: X10DRU-i+, X10DRU-X(LL)
    Affected functions:
    Validation :
        1. After updating FW, power cycle the SUT.
        2. Check the MB_10G Temp1 and Temp2 value.    
    
4.  Category: fix                                                                 
    Description: 
        [64840][IPMi_3.12]API Status report error      
	Affected functions:                                                         
    Validation :
        1. when pws fail, check status https://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Power
        2. also check overall status https://xxx.xxx.xxx.xxx/redfish/v1/Systems/1   
        
5.  Category: fix                                                                 
    Description: 
        [64873][v3.12] will not allow save/mount virtual media drive       
	Affected functions:                                                         
    Validation :
		1. Allow "\" character in path, \XXX\YYY.iso could be save and mount.
      
========================================================================================					 
1.	Category: fix
    Description:
		[64571] Inconsistent Fan Fail Behavior between IPMI and Redfish 
		
	Affected functions:
    Validation :
        1.Disconnecting a system fan while system is online triggers Fan Failure Alert in IPMI.
		2.https://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Thermal
		3.to see status and health of Fan sensor.

2.	Category: fix
    Description:
		Voltage sensor is absent but redfish show status OK. 
		
	Affected functions:
    Validation :
        1.https://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Power
		3.Check voltage sensor status.

3.	Category: fix
    Description:
		Session Audit and AC Power On event log can't show message in log service. 
		
	Affected functions:
    Validation :
	    1.Generate Session Audit and AC Power On event.
		2.https://xxx.xxx.xxx.xxx/redfish/v1/Managers/1/LogServices/Log1/Entries/
		3.Check event entries to see the message.

4. 	Category: fix
    Description:
		[64644][IPMI_3.11] HTTPS always pops out the first time after flash
		
	Affected functions:
    Validation :
	    1.check if SSL redirection is enable on ipmi web.       


========================================================================================
Filename: REDFISH_X10_311.bin  version: 3.11  Date: 08-14-2015

Support Motherboard: X10DRU-I+, X10DRT-P, X10DRG-H, X10DRW-I, X10DRI-T4+, X10DDW-I,
					 X10DRFR, X10DRI-T, X10DRFF, X10DRT-HIBF, X10DRFR-T, X10DRD,
					 X10DRD-L
	
1.  Category: fix
    Description:
		[64504] Redfish IPMI FW 3.10: Redfish responses "200 OK" if we PATCH Accounts Password with empty string  
		
	Affected functions:
    Validation :
        1. https://xxx.xxx.xxx.xxx/redfish/v1/AccountService/Accounts/3/
        2. [patch] {"UserName":"opera123", "Password":"","RoleId":"Admin"}
		3. Password length should be great than 8.
		
2.  Category: fix
    Description:
		[64324] Redfish 1.03: Event subscription doesnot display correct error message after creating max number of subscription 
		
	Infected motherboard:   
    Affected functions:
    Validation :
        Step1: try to create 16 subscriptions. status code should be 403.

3.  Category: fix
    Description:
		[64439] Redfish IPMI FW 3.10: After upgrading fw with factory default restored, previous event subscriptions remains present. 
		
	Infected motherboard:   
    Affected functions:
    Validation :
        1. do factory default
		2. check https://xxx.xxx.xxx.xxx/redfish/v1/EventService/Subscriptions/
		
4.  Category: fix
    Description:
		[64441]  Redfish IPMI FW 3.10: Redfish responses "200 OK" if we POST ComputerSystem reset operation without parsing payload.  
		
	Infected motherboard:   
    Affected functions:
    Validation :
        1.[POST] https://xxx.xxx.xxx.xxx/redfish/v1/Systems/1/Actions/ComputerSystem.Reset without payload data.
		2.will return status cod 400 and error message.

5.  Category: fix
    Description:
		[64505] Redfish 1.03: HTTP response 200 on PATCH Accounts RoleId with unknow type 
		
	Affected functions:
    Validation :
        1. https://xxx.xxx.xxx.xxx/redfish/v1/AccountService/Accounts/3/
        2. [patch] {"UserName":"opera123","RoleId":"123"}
		3. will return error code and error message.

6.  Category: fix
    Description:
		[64506] Redfish 1.03: Account Collections miss Account after PATCH Account RoldId with unknow type 
		
	Affected functions:
    Validation :
        1. https://xxx.xxx.xxx.xxx/redfish/v1/AccountService/Accounts/3/
        2. [patch] {"UserName":"opera123","RoleId":"123"}
		3. will return error code and error message.

7.	Category: fix
    Description:
		[64465] [Redfish] Sensor readings missing in IPMI3.10 
	Motherboard: MBD-X10DRU-I+-P	
	Affected functions:
    Validation :
        1. https://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Power

8.	Category: fix
    Description:
		[64535] Redfish Managers/1/SerialInterface/1 InterfaceEnabled not available   
	
	Affected functions:
    Validation :
        1. https://xxx.xxx.xxx.xxx/redfish/v1/Managers/1/SerialInterface/1
        
9.	Category: fix
    Description:
		[64556] Redfish /redfish/v1/Systems/1/Processors/2 and /redfish/v1/Systems/1/Processors/1 were swapped  
	
	Affected functions:
    Validation :
        1. https://xxx.xxx.xxx.xxx/redfish/v1/Systems/1/Processors

10.	Category: fix
    Description:
		SerialNumber and PartNumber of /redfish/v1/Systems/1 are from FRU0  
	
	Affected functions:
    Validation :
        1. https://xxx.xxx.xxx.xxx/redfish/v1/Systems/1
========================================================================================

Filename: REDFISH_X10_310.bin  version: 3.10  Date: 08-07-2015

1. Category: fix
    Description:
	fix the mismtach for odata.type	field
    Motherboard: X10 motherboards
    Affected functions:
    Validation : 
	1. please use PostMan to verify.

2.  Category: fix
    Description:
	fix the wrong for odata.context url	
    Motherboard: X10 motherboards
    Affected functions:
    Validation : 
	1. please use PostMan to verify.

3.  Category: fix
    Description:
		[62000] PWS serial number does not match when run
		http://172.31.41.45/redfish/v1/Chassis/1/Power this command 

    Affected functions:
    Validation :
        1. http://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Power
        2. Check PowerSupplies -> SerialNumber
     

4.  Category: fix
    Description:
		[62003] Some sensor readings are showing wrong when run
		http://172.31.41.45/redfish/v1/Chassis/1/Thermal command 
		
	Infected motherboard: X10DRI  
    Affected functions:
    Validation :
        1. http://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Thermal
        2. Check "PCH Temp" -> "Status" -> "Health"

5.  Category: fix
    Description:
		[62005] Fans sernsor reading show wrong readings when Fans are not 
		plugged in with command http://172.31.41.45/redfish/v1/Chassis/1/Thermal 
		
	Infected motherboard: X10DRI  
    Affected functions:
    Validation :
        1. http://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Thermal
        2. Check "FAN" -> "Status" -> "Health"
		
6.  Category: fix
    Description:
		[62714] Log service entries have no detail & time stamp do not match with IPMI SEL 
		when run "http://172.16.140.218/redfish/v1/Managers/1/LogServices/Log1/Entries/2" command  
		
	Infected motherboard:   
    Affected functions:
    Validation :
        1. check how many event log in BMC.
        2. Check event entries"http://xxx.xxx.xxx.xxx/redfish/v1/Managers/1/LogServices/Log1/Entries/

7.  Category: fix
    Description:
		[63641] Incorrect data type found on Redfish, using firmware version 1.0.2    
		
	Infected motherboard:   
    Affected functions:
    Validation :
        1. http://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Thermal to check "SensorNumber"  data type: Integer

8.  Category: fix
    Description:
		[63946]  redfish/v1/Chassis/1/Thermal: DIMM MIN/MAX Voltage values are not defined properly
		
	Infected motherboard:   
    Affected functions:
    Validation :
        1. http://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Thermal to check DIMM MIN/MAX values
		
8.  Category: fix
    Description:
		[64167] Redfish_FW 1.03: Event Subscription does not accept "ResourceRemoved" added inside “Event Type”  
		
	Infected motherboard:   
    Affected functions:
    Validation :
        Step1: Posting subscription->got 201 created 
			[Post]http://IP/redfish/v1/EventService/Subscriptions/
			{"Destination":"http://www.dnsname.com/Destination1","Context":"user1_test","EventTypes":["Alert","StatusChange", "ResourceRemoved"],"Protocol":"Redfish"}
		Step2: Validating Subscription:http://IP/redfish/v1/EventService/Subscriptions/

9.  Category: fix
    Description:
		[64324] Redfish 1.03: Event subscription doesnot display correct error message after creating max number of subscription 
		
	Infected motherboard:   
    Affected functions:
    Validation :
        Step1: try to create 16 subscriptions 


		
        
		
========================================================================================
Filename: REDFISH_X10_103.bin  version: 1.03  Date: 07-27-2015

1. Category: New implementation
    Description:
		enable Https by default.
		Note:please do the reset-to-default
	Motherboard: X10 motherboards
    Affected functions:
    Validation : 
		1. please use PostMan to verify.

2.  Category: New implementation
    Description:
		Support NvME and LSI under Systems/1/SimpleStorage/
		Note:  LSI is restricted to LSI 3108 series
	Motherboard: X10 motherboards
    Affected functions:
    Validation : 
		1. MUST have NvME SSD or LSI storage card populated in the system.
		2. please use PostMan to verify.
3. 	Category: Fix
    Description:
		fix the odata.context_url in some resources 
	Motherboard: X10 motherboards
    Affected functions:
    Validation : please use PostMan to verify.
	
4. 	Category: New implementation
    Description:
		Support Fan Mode under /redfish/v1/Chassis/1 
	Motherboard: X10 motherboards
    Affected functions:
    Validation : please use PostMan to verify.
	
5.  Category: New implementation
    Description:
		Support EventService and send out alert through redfish.
	Motherboard: X10 motherboards
    Affected functions:
    Validation : please use PostMan to verify.
		
	


========================================================================================
Filename: REDFISH_X10_102.bin  version: 1.02  Date: 06-018-2015


1.  Category: New implementation
    Description:
	Support to create, update and delete resource which is listed as below through redfish.
	It is supposed to be consistent with IPMI web.


/redfish/v1/Systems/1
update: Boot BootSourceOverrideEnabled BootSourceOverrideTarget IndicatorLED

/redfish/v1/Managers/1
update : DateTime (Note: value is changed when ntp is disabled)
	 DateTimeLocalOffset (Note: value is changed when ntp is enabled)

/redfish/v1/Managers/1/NetworkProtocol/
update :
HTTP
Enabled
Port
HTTPS
Enabled
Port
IPMI
Enabled
Port
KVMIP
Enabled
Port
SNMP
Enabled
Port
SSH
Enabled
Port
VirtualMedia (Note: When KVMIP is disabled, VirtualMedia will get disabled together)
Enabled
Port

/Managers/1/SerialInterfaces/1/
update : BitRate, FlowControl
/Managers/1/EthernetInterfaces/1/
update : AutoNeg, FullDuplex, SpeedMbps, HostName, VLAN{ VLANEnable, VLANId}, IPv4Addresses{ AddressOrigin, Address, SubnetMask, Gateway}, NameServers

/AccountService/Account
UserName Password and RoleId are required to create users.
/AccountService/Account/[num] 
delete users and update user.
/SesssionService/
update :SessionTimeout
	
Chassis/1/
update: AssetTag

========================================================================================
Filename: REDFISH_X10_101.bin  version: 1.01  Date: 06-01-2015
	
    1. 
	Category: New implementation
    Description:
		Support the below new RedFish APIs and redfish authentication following "Redfish Scalable Platforms Management API Specification"
		Be noted that please do reset-to-default and take new settings into effect.

    Motherboard: X10 motherboards
    Affected functions:
    Validation : please use PostMan to verify.
	

/redfish/v1/Managers/1/LogServices/
/redfish/v1/Managers/1/LogServices/Log1/
/redfish/v1/Managers/1/LogServices/Log1/Entries
/redfish/v1/Managers/1/LogServices/Log1/Entries/[num]
/redfish/v1/SessionService/
/redfish/v1/SessionService/Sessions/
/redfish/v1/SessionService/Sessions/[num]
/redfish/v1/Systems
/redfish/v1/Systems/1
/redfish/v1/Systems/1/Processors/[num]
/redfish/v1/Systems/1/EthernetInterfaces/[num]  (MUST install TAS)
/redfish/v1/Managers/1/LogServices/Log1/Actions/LogService.Reset
/redfish/v1/Managers/1/Actions/Manager.Reset
/redfish/v1/Systems/1/Actions/ComputerSystem.Reset  
	2. 
	Category: Fix
    Description:
		fix the issues under the below urls.
		/redfish/v1/Chassis/1
		/redfish/v1/Chassis/1/Power/Voltages/1
		/redfish/v1/Managers/1/
		/redfish/v1/Managers/1/SerialInterfaces
		/redfish/v1/Managers/1/EthernetInterfaces

    Motherboard: X10 motherboards
    Affected functions:
    Validation : 
	3. 
	Category: Fix
    Description:
		fix the typo on IPMI web.
		
    Motherboard: X10 motherboards
    Affected functions:
    Validation : 

========================================================================================
Filename: REDFISH_X10_100.bin  version: 1.00  Date: 04-29-2015
1. 

	Category: New implementation
	Description:
		Support the below RedFish APIs. 
		Be noted that please do reset-to-default and take new settings into effect.

    Motherboard: X10 motherboards
    Affected functions:
    Validation :
		Please install JsonViewer and PostMan plugins in the browser, chrome or Firefox.
		
/redfish/v1/
/redfish/v1/$metadata
/redfish/v1/Chassis
/redfish/v1/Chassis/1
/redfish/v1/Chassis/1/Thermal
/redfish/v1/Chassis/1/Power
/redfish/v1/Managers
/redfish/v1/Managers/1
/redfish/v1/Managers/1/NetworkProtocol
/redfish/v1/Managers/1/EthernetInterfaces
/redfish/v1/Managers/1/EthernetInterfaces/1
/redfish/v1/Managers/1/SerialInterfaces
redfish/v1/Managers/1/SerialInterfaces/1
/redfish/v1/AccountService
/redfish/v1/AccountService/Accounts/
/redfish/v1/AccountService/Accounts/[num]
/redfish/v1/AccountService/Roles
/redfish/v1/AccountService/Roles/Admin
/redfish/v1/AccountService/Roles/Operator
/redfish/v1/AccountService/Roles/ReadOnlyUser






