Grandstream Networks - Date: 10/20/2004
Budgetone 100 Series SIP Phones - Ring Tone Generation Tool


Grandstream made available 2 tools used for converting music files (mp3, .wav, etc) 
to a Grandstream music ring tone format for our IP phones.  The ZIP files contains one file for Solaris and one for Linux.

Usage: sox input output.ring
 
The extension of output file has to be ".ring"

For example for ring one:
sox sound.wav ring1.ring

Then rename the file “ring1.ring” to “ring1.bin” and the file is ready for download.

Place the file in the TFTP server folder containing the firmware. The Budgetone phones will
load the ring tones in the next reboot.


Note:

The Budgetone phones support up to three ring tones.

The tool converts music files into PCMU (G.711A) format of up to 64KB each.


