# Enum - HostNumericSensorType(vim.host.NumericSensorInfo.SensorType)

Since
  VI API 2.5

## Enum Description

Sensor Types for specific hardware component are either based on class of sensor or what the sensor monitors to allow for grouping

Enum Constants

Name | Description
--- | ---
battery | Since
bios | Since
cable | Since
fan |
memory | Since
other |
power |
processor | Since
storage | Since
systemBoard | Since
temperature |
voltage |
watchdog | Since

Show WSDL type definition
<simpleType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="HostNumericSensorType"> <restriction base="xsd:string"> <enumeration value="fan"/> <enumeration value="power"/> <enumeration value="temperature"/> <enumeration value="voltage"/> <enumeration value="other"/> <enumeration value="processor"/> <enumeration value="memory"/> <enumeration value="storage"/> <enumeration value="systemBoard"/> <enumeration value="battery"/> <enumeration value="bios"/> <enumeration value="cable"/> <enumeration value="watchdog"/> </restriction> </simpleType>