# Enum - HostNvmeTransportParametersNvmeAddressFamily(vim.host.NvmeTransportParameters.NvmeAddressFamily)

Since
  vSphere API 7.0

## Enum Description

This enum specifies the supported address families for NVME over Fabrics.

For details, see:

- "NVM Express over Fabrics 1.0", Section 5.3, Figure 34, "Discovery Log Page Entry"

Enum Constants

Name | Description
--- | ---
fc | Fibre Channel address family.
infiniBand | InfiniBand address family.
ipv4 | IPv4 address, format specified in IETF RFC 791.
ipv6 | IPv6 address, format specified in IETF RFC 2373.
loopback | Intra-host transport.
unknown | Unrecognized address family.

Show WSDL type definition
<simpleType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:vsan="urn:vsan" name="HostNvmeTransportParametersNvmeAddressFamily"> <restriction base="xsd:string"> <enumeration value="ipv4"/> <enumeration value="ipv6"/> <enumeration value="infiniBand"/> <enumeration value="fc"/> <enumeration value="loopback"/> <enumeration value="unknown"/> </restriction> </simpleType>