# Enum - VirtualEthernetCardLegacyNetworkDeviceName(vim.vm.device.VirtualEthernetCardOption.LegacyNetworkBackingOption.LegacyNetworkDeviceName)

Since
  2.0

## Enum Description

Possible device names for legacy network backing option are listed below. Note: This is not an exhaustive list. It is possible to specify a specific device as well. For example, on ESX hosts, the device name could be specified as "vmnic[0-9]" or vmnet_[0-9]. For VMware Server Windows hosts, the device name could be specified as "vmnet[0-9]" and for VMware Server Linux hosts, the device name could be specified as "/dev/vmnet[0-9]" depending on what devices are available on that particular host.

Enum Constants

Name | Description
--- | ---
bridged |
hostonly |
nat |

Show WSDL type definition
<simpleType xmlns="http://www.w3.org/2001/XMLSchema" xmlns:pbm="urn:pbm" name="VirtualEthernetCardLegacyNetworkDeviceName"> <restriction base="xsd:string"> <enumeration value="bridged"/> <enumeration value="nat"/> <enumeration value="hostonly"/> </restriction> </simpleType>